<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-43.4" y1="16.5" x2="-43.4" y2="-16.5" width="0.01" layer="20"/>
<wire x1="-43.4" y1="-16.5" x2="-3.2" y2="-16.5" width="0.01" layer="20"/>
<wire x1="-0.66" y1="-10.16" x2="-1.85" y2="-11.35" width="0.01" layer="20" curve="-90"/>
<wire x1="-1.85" y1="-11.35" x2="-1.93" y2="-11.35" width="0.01" layer="20"/>
<wire x1="-0.66" y1="-16.8" x2="-0.66" y2="-15.32" width="0.01" layer="20"/>
<wire x1="-0.66" y1="-15.32" x2="-1.93" y2="-14.05" width="0.01" layer="20" curve="90"/>
<wire x1="-0.66" y1="16.8" x2="-0.66" y2="15.32" width="0.01" layer="20"/>
<wire x1="-0.66" y1="15.32" x2="-1.93" y2="14.05" width="0.01" layer="20" curve="-90"/>
<wire x1="-1.93" y1="14.05" x2="-3.2" y2="15.32" width="0.01" layer="20" curve="-90"/>
<wire x1="-3.2" y1="15.32" x2="-3.2" y2="16.5" width="0.01" layer="20"/>
<wire x1="-0.66" y1="5.08" x2="-0.66" y2="2.62" width="0.01" layer="20"/>
<wire x1="-0.66" y1="2.62" x2="-1.93" y2="1.35" width="0.01" layer="20" curve="-90"/>
<wire x1="-1.93" y1="1.35" x2="-3.2" y2="2.62" width="0.01" layer="20" curve="-90"/>
<wire x1="-1.93" y1="11.35" x2="-0.66" y2="10.08" width="0.01" layer="20" curve="-90"/>
<wire x1="-0.66" y1="10.08" x2="-0.66" y2="7.62" width="0.01" layer="20"/>
<wire x1="-1.93" y1="11.35" x2="-3.2" y2="10.08" width="0.01" layer="20" curve="90"/>
<wire x1="-3.2" y1="10.08" x2="-3.2" y2="2.62" width="0.01" layer="20"/>
<wire x1="-1.93" y1="-1.35" x2="-0.66" y2="-2.62" width="0.01" layer="20" curve="-90"/>
<wire x1="-0.66" y1="-2.62" x2="-0.66" y2="-7.62" width="0.01" layer="20"/>
<wire x1="-1.93" y1="-1.35" x2="-3.2" y2="-2.62" width="0.01" layer="20" curve="90"/>
<wire x1="-1.93" y1="-11.35" x2="-3.2" y2="-10.08" width="0.01" layer="20" curve="-90"/>
<wire x1="-3.2" y1="-10.08" x2="-3.2" y2="-2.62" width="0.01" layer="20"/>
<wire x1="-1.93" y1="-14.05" x2="-3.2" y2="-15.32" width="0.01" layer="20" curve="90"/>
<wire x1="-3.2" y1="-15.32" x2="-3.2" y2="-16.5" width="0.01" layer="20"/>
<wire x1="-3.2" y1="16.5" x2="-43.4" y2="16.5" width="0.01" layer="20"/>
<wire x1="-0.66" y1="5.08" x2="14.58" y2="5.08" width="0.01" layer="20"/>
<wire x1="15.85" y1="-1.35" x2="17.12" y2="-2.62" width="0.01" layer="20" curve="-90"/>
<wire x1="17.12" y1="-2.62" x2="17.12" y2="-8.89" width="0.01" layer="20"/>
<wire x1="15.85" y1="-1.35" x2="14.58" y2="-2.62" width="0.01" layer="20" curve="90"/>
<wire x1="14.58" y1="-2.62" x2="14.58" y2="-7.62" width="0.01" layer="20"/>
<wire x1="17.12" y1="6.35" x2="17.12" y2="2.62" width="0.01" layer="20"/>
<wire x1="17.12" y1="2.62" x2="15.85" y2="1.35" width="0.01" layer="20" curve="-90"/>
<wire x1="15.85" y1="1.35" x2="14.58" y2="2.62" width="0.01" layer="20" curve="-90"/>
<wire x1="14.58" y1="2.62" x2="14.58" y2="5.08" width="0.01" layer="20"/>
<wire x1="14.58" y1="-7.62" x2="-0.66" y2="-7.62" width="0.01" layer="20"/>
<wire x1="-0.66" y1="7.62" x2="15.85" y2="7.62" width="0.01" layer="20"/>
<wire x1="15.85" y1="7.62" x2="17.12" y2="6.35" width="0.01" layer="20" curve="-90"/>
<wire x1="17.12" y1="-8.89" x2="15.85" y2="-10.16" width="0.01" layer="20" curve="-90"/>
<wire x1="15.85" y1="-10.16" x2="-0.66" y2="-10.16" width="0.01" layer="20"/>
<wire x1="-0.66" y1="16.8" x2="22.33" y2="16.8" width="0.01" layer="20"/>
<wire x1="28.35" y1="15.53" x2="23.6" y2="15.53" width="0.01" layer="20"/>
<wire x1="23.6" y1="15.53" x2="22.33" y2="16.8" width="0.01" layer="20" curve="-90"/>
<wire x1="28.35" y1="15.53" x2="28.35" y2="-15.53" width="0.01" layer="20"/>
<hole x="-1.93" y="12.7" drill="0.6"/>
<hole x="-1.93" y="0" drill="0.6"/>
<hole x="-1.93" y="-12.7" drill="0.5"/>
<text>+</text>
<text>-</text>
<text>TX+</text>
<text>TX-</text>
<text>D+(A)/RX+</text>
<text>D-(B)/RX-</text>
<text>485
D+/A</text>
<text>422
RX+</text>
<text>485
D-/B</text>
<text>422
RX-</text>
<text>422
TX+</text>
<text>422
TX-</text>
<text>+V</text>
<text>GND</text>
<text>CMD</text>
<text>422 485</text>
<text>Power</text>
<text>Connected</text>
<text>Power</text>
<text>Connected</text>
<text>Reset</text>
<text>WIZnet
WIZ108SR
Adapterboard</text>
<text>v1.5
by R.E. 2016.03.05</text>
<text>LDO/DC-DC-3.3V out</text>
<text>TOP</text>
<text>BOT</text>
<text>BOT</text>
<wire x1="22.33" y1="-16.8" x2="-0.66" y2="-16.8" width="0.01" layer="20"/>
<text>VSS</text>
<text>VSS</text>
<text>2</text>
<text>4</text>
<text>1</text>
<text>3</text>
<text>2</text>
<text>4</text>
<text>1</text>
<text>3</text>
<text>422</text>
<text>485</text>
<text>422-485</text>
<text>422-485</text>
<text>CMD</text>
<text>CMD-RUN</text>
<text>-RUN</text>
<wire x1="22.33" y1="-16.8" x2="23.6" y2="-15.53" width="0.01" layer="20" curve="-90"/>
<wire x1="23.6" y1="-15.53" x2="28.35" y2="-15.53" width="0.01" layer="20"/>
<text>CMD</text>
<text>RUN</text>
<text>Connected</text>
<text>Power</text>
<text>Reset</text>
<text>Connected</text>
<text>Power</text>
<text>Reset</text>
<text>422-485</text>
<text>RUN</text>
<text>CMD-RUN</text>
<text>CMD</text>
<text>422-485</text>
<text>TOP</text>
<text>WIZnet
WIZ108SR
Adapterboard
(Display)</text>
<hole x="-1.93" y="13.6" drill="0.6"/>
<hole x="-1.93" y="11.8" drill="0.6"/>
<hole x="-1.93" y="-11.8" drill="0.5"/>
<hole x="-1.93" y="-13.6" drill="0.5"/>
<hole x="-1.93" y="0.9" drill="0.6"/>
<hole x="-1.93" y="-0.9" drill="0.6"/>
<hole x="15.85" y="0" drill="0.6"/>
<hole x="15.85" y="0.9" drill="0.6"/>
<hole x="15.85" y="-0.9" drill="0.6"/>
<text>CUT OUT</text>
<text>CUT OUT</text>
<text>CUT OUT</text>
<text>CUT OUT</text>
<hole x="-17" y="0" drill="0.6"/>
<hole x="-17" y="-10" drill="0.6"/>
<hole x="27.85" y="3" drill="0.6"/>
<hole x="27.85" y="-3" drill="0.6"/>
<hole x="27.85" y="-10.2" drill="0.6"/>
<hole x="27.85" y="10" drill="0.6"/>
<text>RUN</text>
<text>RESET</text>
<text>LDO: Brücke </text>
</plain>
<libraries>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="!Ralf1">
<packages>
<package name="MJTP1236B">
<description>&lt;b&gt;Kurzhubtaster - Tactile Switch&lt;br&gt;
6x6mm, Höhe 8.35 mm / 8.4 mm&lt;/b&gt;&lt;br&gt;
MJTP1236B&lt;br&gt;
PHAP3305B&lt;br&gt;
Reichelt Taster 3305B&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-master-EU">
<description>&lt;b&gt;R/C MASTER! - v1.19 (10/25/2011)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD and through hole resistors and capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
As a general guideline, SMD resistors are typically rated as follows:&lt;p&gt;
0402 = 1/16 watt&lt;br&gt;
0603 = 1/10 watt&lt;br&gt;
0805 = 1/8  watt&lt;br&gt;
1206 = 1/4  watt&lt;br&gt;
2010 = 1/2  watt&lt;br&gt;
2512 = 1    watt&lt;br&gt;&lt;p&gt;
&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007-2008, Bob Starr&lt;br&gt; 
&lt;a href="http://www.bobstarr.net"&gt;http://www.bobstarr.net&lt;/a&gt;
&lt;/author&gt;</description>
<packages>
<package name="C7343-TE-D">
<description>&lt;b&gt;SMD TANTALUM&lt;/b&gt; - Panasonic Size D&lt;p&gt; 
EIA Code 7343, Size D, 7.3 mm x 4.3 mm, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="led1">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="!Ralf_TRY_Library">
<packages>
<package name="SMD1.6X3.8">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;&lt;br&gt;
1,6 x 3,8 mm&lt;br&gt;
(für Pin Header 3-3,8mm)</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="tracopower_tsr-1">
<packages>
<package name="TSR-1_TO220V">
<description>&lt;b&gt;Traco TSR-1&lt;/b&gt;&lt;p&gt;
inkl. TO220V Package für alternative Bestückung
&lt;p&gt;
DC/DC-Konverter&lt;br&gt;
TSR-1 Serie, 1 A&lt;p&gt;
&lt;p&gt;&lt;i&gt;www.tracopower.com&lt;/i&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-sprincon-ria_ast">
<packages>
<package name="AST025_06">
</package>
</packages>
</library>
<library name="jumper_RE">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP3WV">
</package>
<package name="JUMPER_VERTICAL">
</package>
<package name="JP2_NO_NUM">
</package>
</packages>
</library>
<library name="rc-master-smd-EU">
<description>&lt;b&gt;R/C MASTER-SMD! - v1.14 (03/30/2013)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD ONLY resistors and capacitors by various manufacturers. The pad sizes, spacing and silkscreen widths have been tweaked for use in dense fine pitch layouts where space, alignment and precision are critical. In general these components are designed for routing in grid increments of 5 mils&lt;/p&gt;
&lt;p&gt;* Silkscreen line elements are a minimum of 8 mils in width. All components have text sizes of 0.032"  or 0.04".&lt;/p&gt;
&lt;p&gt;* A silkscreen text values use a ratio of 18 in all cases.&lt;/p&gt;
&lt;p&gt;* ALL PADS AND PART OUTLINES ARE SNAPPED TO A 5 MIL GRID!&lt;/p&gt;
&lt;p&gt;* See ULP script &lt;b&gt;migrate-rc-master.ulp&lt;/b&gt; to auto-migrate parts from &lt;b&gt;rcl.lbr&lt;/b&gt;&lt;/h4&gt;.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All components are prefixed using the following conventions:&lt;/h4&gt;&lt;/p&gt;&lt;br&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
As a general guideline, SMD resistors are typically rated as follows:&lt;p&gt;
0402 = 1/16 watt&lt;br&gt;
0603 = 1/10 watt&lt;br&gt;
0805 = 1/8  watt&lt;br&gt;
1206 = 1/4  watt&lt;br&gt;
2010 = 1/2  watt&lt;br&gt;
2512 = 1    watt&lt;br&gt;&lt;p&gt;
&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007-2008, Bob Starr&lt;br&gt; 
&lt;a href="http://www.bobstarr.net"&gt;http://www.bobstarr.net&lt;/a&gt;
&lt;/author&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; - 0805</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAP&lt;/b&gt; - 0805</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="traco_tmr">
<description>&lt;b&gt;Traco Power TMR series: 2-3W DC-DC converters in compact SIP-8 package&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="TRACO_SIP-8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="pinhead" package="2X06" value="MPE 087-2-012">
<attribute name="VALUE"/>
</element>
<element name="J5" library="jumper_RE" package="JP2_NO_NUM" value="MPE 087-1-003">
<attribute name="VALUE"/>
</element>
<element name="R1" library="rc-master-smd-EU" package="R0805" value="820R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led1" package="CHIP-LED0805" value="rt">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rc-master-smd-EU" package="R0805" value="820R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led1" package="CHIP-LED0805" value="gn">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rc-master-smd-EU" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="jumper_RE" package="JP2_NO_NUM" value="MPE 087-1-003">
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="6x6mm TASTER 9302">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="LED3MM" value="3mm rt LowCurrent">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="LED3MM" value="3mm ge LowCurrent">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="!Ralf1" package="MJTP1236B" value="Taster3305">
<attribute name="VALUE"/>
</element>
<element name="R3" library="rc-master-smd-EU" package="R0805" value="820R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rc-master-smd-EU" package="R0805" value="820R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV5" library="pinhead" package="2X06" value="2.54_PINHD_female 8.5mm">
<attribute name="VALUE"/>
</element>
<element name="SV6" library="pinhead" package="2X06" value="2.54mm_PINHD_female 7mm">
<attribute name="VALUE"/>
</element>
<element name="PAD2-1" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-GND">
<attribute name="VALUE"/>
</element>
<element name="PAD2-3" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-NRESET">
<attribute name="VALUE"/>
</element>
<element name="PAD2-2" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-GND">
<attribute name="VALUE"/>
</element>
<element name="PAD1-1" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-HW_TRIG">
<attribute name="VALUE"/>
</element>
<element name="J2" library="pinhead" package="2X02" value="MPE 094-2-004">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="LED3MM" value="3mm 2mA rt LowCurrent ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="LED3MM" value="3mm 2mA gn LowCurrent">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2-4" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-3V3">
<attribute name="VALUE"/>
</element>
<element name="PAD1-2" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-486_SEL">
<attribute name="VALUE"/>
</element>
<element name="PAD1-3" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-GND">
<attribute name="VALUE"/>
</element>
<element name="PAD1-4" library="!Ralf_TRY_Library" package="SMD1.6X3.8" value="SMDPAD-GND">
<attribute name="VALUE"/>
</element>
<element name="J3" library="pinhead" package="2X02" value="MPE 094-2-004">
<attribute name="VALUE"/>
</element>
<element name="SV4" library="con-sprincon-ria_ast" package="AST025_06" value="AST025_06">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="jumper_RE" package="JP3WV" value="Stiftleiste 3x2 (3-reihig)">
<attribute name="NAME"/>
</element>
<element name="U$4" library="jumper_RE" package="JUMPER_VERTICAL" value=""/>
<element name="U$1" library="jumper_RE" package="JUMPER_VERTICAL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="1,6/0,9" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad" package="1,6/0,9" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="1,6/0,9" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="1,6/0,9" value="">
<attribute name="VALUE"/>
</element>
<element name="DC1" library="traco_tmr" package="TRACO_SIP-8" value="TMR"/>
<element name="C2" library="rc-master-smd-EU" package="C0805" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rc-master-smd-EU" package="C0805" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rc-master-EU" package="C7343-TE-D" value="47u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IC1B1" library="tracopower_tsr-1" package="TSR-1_TO220V" value="TS 2940 CZ33">
<attribute name="VALUE"/>
</element>
<element name="C1" library="rc-master-EU" package="C7343-TE-D" value="47u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="rc-master-smd-EU" package="C0805" value="330pF/2kV"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="11"/>
<contactref element="J1" pad="12"/>
<contactref element="C6" pad="2"/>
<contactref element="J4" pad="3"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="3"/>
<contactref element="J5" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="-"/>
<contactref element="DC1" pad="7"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1B1" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED4" pad="K"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1B1" pad="1"/>
<contactref element="DC1" pad="2"/>
<contactref element="SV4" pad="6"/>
</signal>
<signal name="+3V3">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="J3" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="+"/>
<contactref element="IC1B1" pad="3"/>
<contactref element="DC1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="HW_TRIG">
<contactref element="J1" pad="8"/>
<contactref element="J5" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED3" pad="K"/>
</signal>
<signal name="NRESET">
<contactref element="J1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="485_SEL">
<contactref element="J1" pad="10"/>
<contactref element="J4" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="485+_RXD+">
<contactref element="J1" pad="3"/>
<contactref element="SV4" pad="1"/>
</signal>
<signal name="485-_RXD-">
<contactref element="J1" pad="5"/>
<contactref element="SV4" pad="2"/>
</signal>
<signal name="TXD+">
<contactref element="J1" pad="7"/>
<contactref element="SV4" pad="3"/>
</signal>
<signal name="TXD-">
<contactref element="J1" pad="9"/>
<contactref element="SV4" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="LED5" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="1"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="+3V3_2">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="PAD2-4" pad="1"/>
</signal>
<signal name="NRESET_">
<contactref element="S2" pad="1"/>
<contactref element="PAD2-3" pad="1"/>
</signal>
<signal name="3V3_3">
<contactref element="SV6" pad="1"/>
<contactref element="SV5" pad="1"/>
<contactref element="SV6" pad="2"/>
<contactref element="SV5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="SV6" pad="3"/>
<contactref element="SV5" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="SV6" pad="5"/>
<contactref element="SV5" pad="5"/>
</signal>
<signal name="N$18">
<contactref element="SV5" pad="7"/>
<contactref element="SV6" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="SV6" pad="9"/>
<contactref element="SV5" pad="9"/>
</signal>
<signal name="GND3">
<contactref element="SV5" pad="11"/>
<contactref element="SV6" pad="11"/>
<contactref element="SV5" pad="12"/>
<contactref element="SV6" pad="12"/>
</signal>
<signal name="N$22">
<contactref element="SV5" pad="4"/>
<contactref element="SV6" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="SV6" pad="6"/>
<contactref element="SV5" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="SV5" pad="8"/>
<contactref element="SV6" pad="8"/>
</signal>
<signal name="N$25">
<contactref element="SV6" pad="10"/>
<contactref element="SV5" pad="10"/>
</signal>
<signal name="GND2">
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="PAD2-1" pad="1"/>
<contactref element="PAD2-2" pad="1"/>
<contactref element="PAD1-4" pad="1"/>
<contactref element="PAD1-3" pad="1"/>
<contactref element="LED5" pad="K"/>
<contactref element="J6" pad="1"/>
<contactref element="J6" pad="4"/>
<contactref element="PAD3" pad="1"/>
<contactref element="PAD5" pad="1"/>
</signal>
<signal name="HW_TRIG_2">
<contactref element="LED6" pad="K"/>
<contactref element="PAD1-1" pad="1"/>
<contactref element="J6" pad="5"/>
<contactref element="PAD4" pad="1"/>
</signal>
<signal name="486_SEL_2">
<contactref element="PAD1-2" pad="1"/>
<contactref element="J6" pad="2"/>
<contactref element="PAD6" pad="1"/>
</signal>
<signal name="GND_B">
<contactref element="DC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="C3" pad="1"/>
<contactref element="SV4" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
