<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="-23.8" y1="68.9" x2="22.15" y2="68.9" width="0" layer="20"/>
<wire x1="22.15" y1="68.9" x2="22.15" y2="12.75" width="0" layer="20"/>
<text>PCIe x4 Carrier</text>
<text>Copyright (C) 2017 H. Poetzl</text>
<text>3V3</text>
<text>1V8</text>
<text>VIN</text>
<text>TDO</text>
<text>TDI</text>
<text>TMS</text>
<text>TCK</text>
<text>GND</text>
<text>VDD</text>
<text>BOOTMODE</text>
<text>VCCIO15</text>
<text>V0.5
R1.0</text>
<wire x1="-23.8" y1="68.9" x2="-23.8" y2="4.5" width="0" layer="20"/>
</plain>
<libraries>
<library name="PCIe">
<packages>
<package name="PCIE-64-SLOT">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_10X200_NOTEXT">
</package>
</packages>
</library>
<library name="LSHM-150-XX.X-XX-DV-A-S">
<packages>
<package name="LSHM-150-XX.X-XX-DV-A-S">
<description>0.5MM TERMINAL/SOCKET COMBO.
MANUFACTURER: SAMTEC.</description>
</package>
</packages>
</library>
<library name="ft260">
<packages>
<package name="QFN50P500X500X80-29N">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP10R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="usb">
<packages>
<package name="MICRO-AB-H-SMT">
</package>
</packages>
</library>
<library name="generic-rcl">
<packages>
<package name="0201-B">
</package>
<package name="0402-C">
</package>
</packages>
</library>
<library name="pinhead-2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de, Modified by Cougar@CasaDelGato.Com&lt;/author&gt;</description>
<packages>
<package name="1X06-S">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="1X03-S">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="1X02-S">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X15">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="esd">
<packages>
<package name="R-PDSO-N5">
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
<variantdef name="Beta"/>
</variantdefs>
<elements>
<element name="CON1" library="PCIe" package="PCIE-64-SLOT" value="PCIE-64SLOT"/>
<element name="LOGO1" library="ohw-logo" package="OSHW_10X200_NOTEXT" value="OSHW_LOGO_10MILX0200-NT"/>
<element name="JM2" library="LSHM-150-XX.X-XX-DV-A-S" package="LSHM-150-XX.X-XX-DV-A-S" value="LSHM-150-XX.X-XX-DV-A-S">
<attribute name="NAME"/>
</element>
<element name="JM1" library="LSHM-150-XX.X-XX-DV-A-S" package="LSHM-150-XX.X-XX-DV-A-S" value="LSHM-150-XX.X-XX-DV-A-S">
<attribute name="NAME"/>
</element>
<element name="U1" library="ft260" package="QFN50P500X500X80-29N" value="FT260">
<attribute name="NAME"/>
</element>
<element name="JP2" library="pinhead-2" package="1X06-S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead-2" package="1X02-S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="generic-rcl" package="0201-B" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="generic-rcl" package="0201-B" value="33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="generic-rcl" package="0402-C" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="generic-rcl" package="0402-C" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="generic-rcl" package="0402-C" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="generic-rcl" package="0402-C" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="esd" package="R-PDSO-N5" value="TPD3E001DRL">
<attribute name="NAME"/>
</element>
<element name="R2" library="generic-rcl" package="0201-B" value="5k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="generic-rcl" package="0201-B" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FS" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead-2" package="1X02-S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="led" package="CHIPLED_0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="D2" library="led" package="CHIPLED_0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="D3" library="led" package="CHIPLED_0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="D4" library="led" package="CHIPLED_0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="R6" library="generic-rcl" package="0402-C" value="10k">
<attribute name="NAME"/>
</element>
<element name="R7" library="generic-rcl" package="0402-C" value="10k">
<attribute name="NAME"/>
</element>
<element name="R8" library="generic-rcl" package="0402-C" value="10k">
<attribute name="NAME"/>
</element>
<element name="R9" library="generic-rcl" package="0402-C" value="10k">
<attribute name="NAME"/>
</element>
<element name="X1" library="usb" package="MICRO-AB-H-SMT" value="5_USB_3S">
<attribute name="NAME"/>
</element>
<element name="C6" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="led" package="CHIPLED_0603" value="LED">
<attribute name="NAME"/>
</element>
<element name="R5" library="generic-rcl" package="0402-C" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead-2" package="2X15" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead-2" package="1X03-S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3V3AUX" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="12V" library="testpad" package="TP10R" value="TPTP10R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="R12" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="generic-rcl" package="0402-C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="HSI0_P">
<contactref element="CON1" pad="A16"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="HSI0_N">
<contactref element="CON1" pad="A17"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="HSI1_P">
<contactref element="CON1" pad="A21"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="HSI1_N">
<contactref element="CON1" pad="A22"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="PRSNT_X1">
<contactref element="CON1" pad="B17"/>
</signal>
<signal name="PRSNT_X4">
<contactref element="CON1" pad="B31"/>
</signal>
<signal name="PRSNT#1">
<contactref element="CON1" pad="A1"/>
</signal>
<signal name="PWRGD">
<contactref element="CON1" pad="A11"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="!WAKE">
<contactref element="CON1" pad="B11"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="GND">
<contactref element="CON1" pad="A4"/>
<contactref element="CON1" pad="A28"/>
<contactref element="CON1" pad="A27"/>
<contactref element="CON1" pad="A24"/>
<contactref element="CON1" pad="A15"/>
<contactref element="CON1" pad="A12"/>
<contactref element="CON1" pad="A23"/>
<contactref element="CON1" pad="A20"/>
<contactref element="CON1" pad="A31"/>
<contactref element="CON1" pad="A18"/>
<contactref element="CON1" pad="B18"/>
<contactref element="CON1" pad="B21"/>
<contactref element="CON1" pad="B7"/>
<contactref element="CON1" pad="B32"/>
<contactref element="CON1" pad="B13"/>
<contactref element="CON1" pad="B4"/>
<contactref element="CON1" pad="B29"/>
<contactref element="CON1" pad="B16"/>
<contactref element="CON1" pad="B25"/>
<contactref element="CON1" pad="B26"/>
<contactref element="CON1" pad="B22"/>
<contactref element="JM1" pad="6"/>
<contactref element="JM1" pad="5"/>
<contactref element="JM1" pad="11"/>
<contactref element="JM1" pad="17"/>
<contactref element="JM1" pad="23"/>
<contactref element="JM1" pad="29"/>
<contactref element="JM1" pad="47"/>
<contactref element="JM1" pad="F1"/>
<contactref element="JM1" pad="F2"/>
<contactref element="JM1" pad="12"/>
<contactref element="JM1" pad="18"/>
<contactref element="JM1" pad="24"/>
<contactref element="JM1" pad="30"/>
<contactref element="JM1" pad="48"/>
<contactref element="JM1" pad="66"/>
<contactref element="JM1" pad="84"/>
<contactref element="JM1" pad="98"/>
<contactref element="JM1" pad="100"/>
<contactref element="JM2" pad="36"/>
<contactref element="JM2" pad="17"/>
<contactref element="JM2" pad="F1"/>
<contactref element="JM2" pad="F2"/>
<contactref element="JM2" pad="83"/>
<contactref element="JM2" pad="35"/>
<contactref element="JM2" pad="72"/>
<contactref element="JM2" pad="90"/>
<contactref element="U1" pad="29"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="JP2" pad="5"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="19"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="Z1"/>
<contactref element="X1" pad="Z4"/>
<contactref element="X1" pad="Z3"/>
<contactref element="X1" pad="Z2"/>
<contactref element="X1" pad="Z6"/>
<contactref element="X1" pad="Z5"/>
<contactref element="D5" pad="C"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="12"/>
<contactref element="JP1" pad="22"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="11"/>
<contactref element="JP1" pad="21"/>
</signal>
<signal name="+3V3">
<contactref element="CON1" pad="A10"/>
<contactref element="CON1" pad="A9"/>
<contactref element="CON1" pad="B8"/>
</signal>
<signal name="+12V">
<contactref element="CON1" pad="A3"/>
<contactref element="CON1" pad="B2"/>
<contactref element="CON1" pad="B1"/>
<contactref element="CON1" pad="A2"/>
<contactref element="12V" pad="TP"/>
</signal>
<signal name="3V3AUX">
<contactref element="CON1" pad="B10"/>
<contactref element="3V3AUX" pad="TP"/>
</signal>
<signal name="HSI2_N">
<contactref element="CON1" pad="A26"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="HSI2_P">
<contactref element="CON1" pad="A25"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="HSI3_N">
<contactref element="CON1" pad="A30"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="HSI3_P">
<contactref element="CON1" pad="A29"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="MGT_RX3_P">
<contactref element="JM1" pad="1"/>
<contactref element="CON1" pad="B28"/>
</signal>
<signal name="MGT_RX3_N">
<contactref element="JM1" pad="3"/>
<contactref element="CON1" pad="B27"/>
</signal>
<signal name="MGT_RX2_P">
<contactref element="JM1" pad="7"/>
<contactref element="CON1" pad="B24"/>
</signal>
<signal name="MGT_RX2_N">
<contactref element="JM1" pad="9"/>
<contactref element="CON1" pad="B23"/>
</signal>
<signal name="MGT_RX1_P">
<contactref element="JM1" pad="13"/>
<contactref element="CON1" pad="B20"/>
</signal>
<signal name="MGT_RX1_N">
<contactref element="JM1" pad="15"/>
<contactref element="CON1" pad="B19"/>
</signal>
<signal name="MGT_RX0_P">
<contactref element="JM1" pad="19"/>
<contactref element="CON1" pad="B15"/>
</signal>
<signal name="MGT_RX0_N">
<contactref element="JM1" pad="21"/>
<contactref element="CON1" pad="B14"/>
</signal>
<signal name="ADC_P">
<contactref element="JM1" pad="25"/>
</signal>
<signal name="ADC_N">
<contactref element="JM1" pad="27"/>
</signal>
<signal name="MGT_CLK0_P">
<contactref element="JM1" pad="2"/>
<contactref element="CON1" pad="A13"/>
</signal>
<signal name="MGT_CLK0_N">
<contactref element="JM1" pad="4"/>
<contactref element="CON1" pad="A14"/>
</signal>
<signal name="MGT_TX3_P">
<contactref element="JM1" pad="8"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="MGT_TX3_N">
<contactref element="JM1" pad="10"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="MGT_TX2_P">
<contactref element="JM1" pad="14"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="MGT_TX2_N">
<contactref element="JM1" pad="16"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="MGT_TX1_P">
<contactref element="JM1" pad="20"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="MGT_TX1_N">
<contactref element="JM1" pad="22"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="MGT_TX0_P">
<contactref element="JM1" pad="26"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="MGT_TX0_N">
<contactref element="JM1" pad="28"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="B34_L2_P">
<contactref element="JM1" pad="31"/>
</signal>
<signal name="B34_L2_N">
<contactref element="JM1" pad="33"/>
</signal>
<signal name="B34_L1_P">
<contactref element="JM1" pad="35"/>
</signal>
<signal name="B34_L1_N">
<contactref element="JM1" pad="37"/>
</signal>
<signal name="B34_L4_P">
<contactref element="JM1" pad="39"/>
</signal>
<signal name="B34_L4_N">
<contactref element="JM1" pad="41"/>
</signal>
<signal name="B34_L5_P">
<contactref element="JM1" pad="43"/>
</signal>
<signal name="B34_L5_N">
<contactref element="JM1" pad="45"/>
</signal>
<signal name="B34_L10_P">
<contactref element="JM1" pad="49"/>
</signal>
<signal name="B34_L10_N">
<contactref element="JM1" pad="51"/>
</signal>
<signal name="B34_L11_N">
<contactref element="JM1" pad="53"/>
</signal>
<signal name="B34_L11_P">
<contactref element="JM1" pad="55"/>
</signal>
<signal name="B34_L12_N">
<contactref element="JM1" pad="57"/>
</signal>
<signal name="B34_L12_P">
<contactref element="JM1" pad="59"/>
</signal>
<signal name="VCCIO34">
<contactref element="JM1" pad="61"/>
</signal>
<signal name="B34_L17_N">
<contactref element="JM1" pad="63"/>
</signal>
<signal name="B34_L17_P">
<contactref element="JM1" pad="65"/>
</signal>
<signal name="B34_L21_P">
<contactref element="JM1" pad="67"/>
</signal>
<signal name="B34_L21_N">
<contactref element="JM1" pad="69"/>
</signal>
<signal name="B34_L19_N">
<contactref element="JM1" pad="71"/>
</signal>
<signal name="B34_L19_P">
<contactref element="JM1" pad="73"/>
</signal>
<signal name="B34_L22_N">
<contactref element="JM1" pad="75"/>
</signal>
<signal name="B34_L22_P">
<contactref element="JM1" pad="77"/>
</signal>
<signal name="B34_L23_N">
<contactref element="JM1" pad="79"/>
</signal>
<signal name="B34_L23_P">
<contactref element="JM1" pad="81"/>
</signal>
<signal name="3V3">
<contactref element="JM1" pad="83"/>
<contactref element="D1" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="R5" pad="2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="B14_L24_N">
<contactref element="JM1" pad="85"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="B14_L24_P">
<contactref element="JM1" pad="87"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="B14_L23_N">
<contactref element="JM1" pad="89"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="B14_L23_P">
<contactref element="JM1" pad="91"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="B14_L21_P">
<contactref element="JM1" pad="93"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="B14_L21_N">
<contactref element="JM1" pad="95"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="VIN">
<contactref element="JM1" pad="97"/>
<contactref element="JM1" pad="99"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="B34_L6_P">
<contactref element="JM1" pad="32"/>
</signal>
<signal name="B34_L6_N">
<contactref element="JM1" pad="34"/>
</signal>
<signal name="B34_L7_P">
<contactref element="JM1" pad="36"/>
</signal>
<signal name="B34_L7_N">
<contactref element="JM1" pad="38"/>
</signal>
<signal name="B34_L3_P">
<contactref element="JM1" pad="40"/>
</signal>
<signal name="B34_L3_N">
<contactref element="JM1" pad="42"/>
</signal>
<signal name="B34_L9_P">
<contactref element="JM1" pad="44"/>
</signal>
<signal name="B34_L9_N">
<contactref element="JM1" pad="46"/>
</signal>
<signal name="B34_L8_P">
<contactref element="JM1" pad="50"/>
</signal>
<signal name="B34_L8_N">
<contactref element="JM1" pad="52"/>
</signal>
<signal name="B34_L13_P">
<contactref element="JM1" pad="54"/>
</signal>
<signal name="B34_L13_N">
<contactref element="JM1" pad="56"/>
</signal>
<signal name="B34_L14_P">
<contactref element="JM1" pad="58"/>
</signal>
<signal name="B34_L14_N">
<contactref element="JM1" pad="60"/>
</signal>
<signal name="B34_L15_N">
<contactref element="JM1" pad="62"/>
</signal>
<signal name="B34_L15_P">
<contactref element="JM1" pad="64"/>
</signal>
<signal name="B34_L16_N">
<contactref element="JM1" pad="68"/>
</signal>
<signal name="B34_L16_P">
<contactref element="JM1" pad="70"/>
</signal>
<signal name="B34_L18_P">
<contactref element="JM1" pad="72"/>
</signal>
<signal name="B34_L18_N">
<contactref element="JM1" pad="74"/>
</signal>
<signal name="B34_L20_N">
<contactref element="JM1" pad="76"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="B34_L20_P">
<contactref element="JM1" pad="78"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="B34_L24_N">
<contactref element="JM1" pad="80"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="B34_L24_P">
<contactref element="JM1" pad="82"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="TDI">
<contactref element="JM1" pad="86"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="TDO">
<contactref element="JM1" pad="88"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="TCK">
<contactref element="JM1" pad="90"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="TMS">
<contactref element="JM1" pad="92"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="PROG_B">
<contactref element="JM1" pad="94"/>
</signal>
<signal name="DONE">
<contactref element="JM1" pad="96"/>
<contactref element="D5" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="B15_L7_N">
<contactref element="JM2" pad="1"/>
<contactref element="JP1" pad="30"/>
</signal>
<signal name="B15_L7_P">
<contactref element="JM2" pad="3"/>
<contactref element="JP1" pad="29"/>
</signal>
<signal name="B15_L8_P">
<contactref element="JM2" pad="5"/>
<contactref element="JP1" pad="28"/>
</signal>
<signal name="B15_L8_N">
<contactref element="JM2" pad="7"/>
<contactref element="JP1" pad="27"/>
</signal>
<signal name="B15_L10_P">
<contactref element="JM2" pad="9"/>
<contactref element="JP1" pad="26"/>
</signal>
<signal name="B15_L10_N">
<contactref element="JM2" pad="11"/>
<contactref element="JP1" pad="25"/>
</signal>
<signal name="B15_L9_P">
<contactref element="JM2" pad="13"/>
<contactref element="JP1" pad="24"/>
</signal>
<signal name="B15_L9_N">
<contactref element="JM2" pad="15"/>
<contactref element="JP1" pad="23"/>
</signal>
<signal name="B15_L15_N">
<contactref element="JM2" pad="19"/>
</signal>
<signal name="B15_L15_P">
<contactref element="JM2" pad="21"/>
</signal>
<signal name="B15_L16_N">
<contactref element="JM2" pad="23"/>
</signal>
<signal name="B15_L16_P">
<contactref element="JM2" pad="25"/>
</signal>
<signal name="B15_L18_N">
<contactref element="JM2" pad="27"/>
</signal>
<signal name="B15_L18_P">
<contactref element="JM2" pad="29"/>
</signal>
<signal name="B15_L17_N">
<contactref element="JM2" pad="31"/>
</signal>
<signal name="B15_L17_P">
<contactref element="JM2" pad="33"/>
</signal>
<signal name="B15_L24_N">
<contactref element="JM2" pad="37"/>
</signal>
<signal name="B15_L24_P">
<contactref element="JM2" pad="39"/>
</signal>
<signal name="B15_L19_N">
<contactref element="JM2" pad="41"/>
</signal>
<signal name="B15_L19_P">
<contactref element="JM2" pad="43"/>
</signal>
<signal name="B15_L21_N">
<contactref element="JM2" pad="45"/>
</signal>
<signal name="B15_L21_P">
<contactref element="JM2" pad="47"/>
</signal>
<signal name="B15_L23_P">
<contactref element="JM2" pad="49"/>
</signal>
<signal name="B15_L23_N">
<contactref element="JM2" pad="51"/>
</signal>
<signal name="VCCIO0">
<contactref element="JM2" pad="53"/>
<contactref element="JP2" pad="6"/>
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="B14_L4_P">
<contactref element="JM2" pad="55"/>
<contactref element="JP1" pad="20"/>
</signal>
<signal name="B14_L4_N">
<contactref element="JM2" pad="57"/>
<contactref element="JP1" pad="19"/>
</signal>
<signal name="B14_L7_N">
<contactref element="JM2" pad="59"/>
<contactref element="JP1" pad="18"/>
</signal>
<signal name="B14_L7_P">
<contactref element="JM2" pad="61"/>
<contactref element="JP1" pad="17"/>
</signal>
<signal name="B14_L15_P">
<contactref element="JM2" pad="63"/>
<contactref element="JP1" pad="16"/>
</signal>
<signal name="B14_L15_N">
<contactref element="JM2" pad="65"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="SPI-CLK">
<contactref element="JM2" pad="67"/>
</signal>
<signal name="SPI-CS">
<contactref element="JM2" pad="69"/>
</signal>
<signal name="SPI-DQ1">
<contactref element="JM2" pad="71"/>
</signal>
<signal name="SPI-DQ2">
<contactref element="JM2" pad="73"/>
</signal>
<signal name="B14_L10_P">
<contactref element="JM2" pad="75"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="B14_L10_N">
<contactref element="JM2" pad="77"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="B14_L16_P">
<contactref element="JM2" pad="79"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="B14_L16_N">
<contactref element="JM2" pad="81"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="B14_L18_N">
<contactref element="JM2" pad="85"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="B14_L18_P">
<contactref element="JM2" pad="87"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="B14_L17_N">
<contactref element="JM2" pad="89"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="B14_L17_P">
<contactref element="JM2" pad="91"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="B14_L20_P">
<contactref element="JM2" pad="93"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="B14_L20_N">
<contactref element="JM2" pad="95"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="B14_L25">
<contactref element="JM2" pad="97"/>
</signal>
<signal name="B14_L0">
<contactref element="JM2" pad="99"/>
</signal>
<signal name="BOOTMODE">
<contactref element="JM2" pad="100"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="B14_L22_P">
<contactref element="JM2" pad="98"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="B14_L22_N">
<contactref element="JM2" pad="96"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="B14_L19_N">
<contactref element="JM2" pad="94"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="B14_L19_P">
<contactref element="JM2" pad="92"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="B14_L13_P">
<contactref element="JM2" pad="88"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="B14_L13_N">
<contactref element="JM2" pad="86"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="B14_L12_N">
<contactref element="JM2" pad="84"/>
</signal>
<signal name="B14_L12_P">
<contactref element="JM2" pad="82"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="B14_L14_P">
<contactref element="JM2" pad="80"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="B14_L14_N">
<contactref element="JM2" pad="78"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="B14_L11_P">
<contactref element="JM2" pad="76"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="B14_L11_N">
<contactref element="JM2" pad="74"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="SPI-DQ3">
<contactref element="JM2" pad="70"/>
</signal>
<signal name="SPI-DQ0">
<contactref element="JM2" pad="68"/>
</signal>
<signal name="B14_L9_N">
<contactref element="JM2" pad="66"/>
</signal>
<signal name="B14_L9_P">
<contactref element="JM2" pad="64"/>
</signal>
<signal name="B14_L8_N">
<contactref element="JM2" pad="62"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="B14_L8_P">
<contactref element="JM2" pad="60"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="B14_L5_N">
<contactref element="JM2" pad="58"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="B14_L5_P">
<contactref element="JM2" pad="56"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="VCCIO15">
<contactref element="JM2" pad="54"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="B15_L20_P">
<contactref element="JM2" pad="52"/>
</signal>
<signal name="B15_L20_N">
<contactref element="JM2" pad="50"/>
</signal>
<signal name="B15_L22_P">
<contactref element="JM2" pad="48"/>
</signal>
<signal name="B15_L22_N">
<contactref element="JM2" pad="46"/>
</signal>
<signal name="B15_L14_P">
<contactref element="JM2" pad="44"/>
</signal>
<signal name="B15_L14_N">
<contactref element="JM2" pad="42"/>
</signal>
<signal name="B15_L13_P">
<contactref element="JM2" pad="40"/>
</signal>
<signal name="B15_L13_N">
<contactref element="JM2" pad="38"/>
</signal>
<signal name="B15_L12_N">
<contactref element="JM2" pad="34"/>
</signal>
<signal name="B15_L12_P">
<contactref element="JM2" pad="32"/>
</signal>
<signal name="B15_L11_N">
<contactref element="JM2" pad="30"/>
</signal>
<signal name="B15_L11_P">
<contactref element="JM2" pad="28"/>
</signal>
<signal name="B15_L6_N">
<contactref element="JM2" pad="26"/>
</signal>
<signal name="B15_L6_P">
<contactref element="JM2" pad="24"/>
</signal>
<signal name="B15_L2_P">
<contactref element="JM2" pad="22"/>
</signal>
<signal name="B15_L2_N">
<contactref element="JM2" pad="20"/>
</signal>
<signal name="1V8">
<contactref element="JM2" pad="18"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="B15_L1_P">
<contactref element="JM2" pad="16"/>
</signal>
<signal name="B15_L1_N">
<contactref element="JM2" pad="14"/>
</signal>
<signal name="B15_L4_P">
<contactref element="JM2" pad="12"/>
</signal>
<signal name="B15_L4_N">
<contactref element="JM2" pad="10"/>
</signal>
<signal name="B15_L5_N">
<contactref element="JM2" pad="8"/>
</signal>
<signal name="B15_L5_P">
<contactref element="JM2" pad="6"/>
</signal>
<signal name="B15_L3_N">
<contactref element="JM2" pad="4"/>
</signal>
<signal name="B15_L3_P">
<contactref element="JM2" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="U2" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="23"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="D_P">
<contactref element="U1" pad="21"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="D_N">
<contactref element="U1" pad="20"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="DD_N">
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="DD_P">
<contactref element="R3" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$47">
<contactref element="U2" pad="4"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="26"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="25"/>
<contactref element="FS" pad="TP"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="C"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="C"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D4" pad="C"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="SMCLK">
<contactref element="CON1" pad="B5"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="SMDAT">
<contactref element="CON1" pad="B6"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
</signals>
</board>
</drawing>
</eagle>
