<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="109.855" y1="25.4" x2="109.855" y2="16.79575" width="0.254" layer="20"/>
<wire x1="109.855" y1="16.79575" x2="98.7425" y2="16.79575" width="0.254" layer="20"/>
<wire x1="98.7425" y1="16.79575" x2="98.7425" y2="25.4" width="0.254" layer="20"/>
<wire x1="96.8375" y1="16.79575" x2="45.085" y2="16.79575" width="0.254" layer="20"/>
<wire x1="45.085" y1="16.79575" x2="45.085" y2="25.4" width="0.254" layer="20"/>
<wire x1="45.085" y1="25.4" x2="36.83" y2="25.4" width="0.254" layer="20"/>
<wire x1="36.83" y1="25.4" x2="36.83" y2="80.01" width="0.254" layer="20"/>
<wire x1="109.855" y1="25.4" x2="118.745" y2="25.4" width="0.254" layer="20"/>
<wire x1="118.745" y1="25.4" x2="118.745" y2="80.01" width="0.254" layer="20"/>
<wire x1="118.745" y1="80.01" x2="36.83" y2="80.01" width="0.254" layer="20"/>
<wire x1="96.8375" y1="16.79575" x2="96.8375" y2="25.4" width="0.254" layer="20"/>
<wire x1="96.8375" y1="25.4" x2="98.7425" y2="25.4" width="0.254" layer="20"/>
<text>128</text>
<text> 64</text>
<text> 32</text>
<text> 16</text>
<text>  8</text>
<text>  4</text>
<text>  2</text>
<text>  1</text>
<text>TourVision V4
HuCard adapter v1.0</text>
<text>https://blog.system11.org</text>
<text>GAME ID
(binary)

DOWN = 0
  UP = 1</text>
</plain>
<libraries>
<library name="tourvision">
<packages>
<package name="TV-EDGE">
</package>
<package name="HUCARD">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EPG-08">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="tourvision" package="TV-EDGE" value=""/>
<element name="E$2" library="special" package="EPG-08" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="tourvision" package="HUCARD" value=""/>
</elements>
<signals>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="S$3">
</signal>
<signal name="S$4">
</signal>
<signal name="S$5">
</signal>
<signal name="S$6">
</signal>
<signal name="S$7">
</signal>
<signal name="S$8">
</signal>
<signal name="S$9">
</signal>
<signal name="S$10">
</signal>
<signal name="S$11">
</signal>
<signal name="S$12">
</signal>
<signal name="S$13">
</signal>
<signal name="S$14">
</signal>
<signal name="S$15">
</signal>
<signal name="S$16">
</signal>
<signal name="S$17">
</signal>
<signal name="S$18">
</signal>
<signal name="S$19">
</signal>
<signal name="S$20">
<contactref element="E$2" pad="8"/>
</signal>
<signal name="S$21">
<contactref element="E$2" pad="7"/>
</signal>
<signal name="S$22">
<contactref element="E$2" pad="6"/>
</signal>
<signal name="S$23">
<contactref element="E$2" pad="5"/>
</signal>
<signal name="S$24">
<contactref element="E$2" pad="4"/>
</signal>
<signal name="S$25">
<contactref element="E$2" pad="3"/>
</signal>
<signal name="S$26">
<contactref element="E$2" pad="2"/>
</signal>
<signal name="S$27">
<contactref element="E$2" pad="1"/>
</signal>
<signal name="S$28">
</signal>
<signal name="S$29">
</signal>
<signal name="S$30">
</signal>
<signal name="S$31">
</signal>
<signal name="S$32">
</signal>
<signal name="S$33">
</signal>
<signal name="S$34">
</signal>
<signal name="S$35">
</signal>
<signal name="S$36">
</signal>
<signal name="S$37">
</signal>
<signal name="S$38">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$41">
</signal>
<signal name="S$42">
</signal>
<signal name="S$43">
</signal>
<signal name="S$44">
</signal>
<signal name="S$45">
</signal>
<signal name="S$46">
<contactref element="E$3" pad="CD"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
