(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 16)
    (zones 0)
    (modules 2)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
  )
  (module misc_footprints:CGB_VOL_SLIDER_v2 (layer F.Cu) (tedit 5DE47A5A)
    (at 160.782 93.25)
    (fp_text reference J2 (at 0 15.25) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 -29.25) (layer F.Fab))
    (pad 1 smd rect (at 4 -9.25 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 2 -9.25 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 5 smd rect (at -4 -9.25 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -2 -9.25 90) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -9.25 90) (size 2 1) (layers F.Cu F.Paste F.Mask))
  )
  (module misc_footprints:AGS_VOL_SLIDER (layer F.Cu) (tedit 5DD0D7FF)
    (at 160.782 90.868)
    (fp_text reference J1 (at 0 5.25) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 -5.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 6.5 1) (size 1.75 1) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole rect (at 6.5 -1) (size 1.75 1) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole rect (at -6.5 1) (size 1.75 1) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole rect (at -6.5 -1) (size 1.75 1) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole rect (at 4.5 -3.25 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 5 thru_hole rect (at -4.5 -3.25 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
  )
  (gr_line (start 156 83.3) (end 156 83) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156 83.7) (end 156 84.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156 85) (end 156 84.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.337 86.614) (end 156 85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.5 85) (end 165.227 86.614) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.5 83) (end 165.5 85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156 83) (end 165.5 83) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.337 88.646) (end 156.337 86.614) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.305 89.154) (end 156.337 88.646) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.305 92.583) (end 154.305 89.154) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.259 92.583) (end 154.305 92.583) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.259 89.027) (end 167.259 92.583) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.227 88.646) (end 167.259 89.027) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.227 86.614) (end 165.227 88.646) (layer Edge.Cuts) (width 0.05))
  (gr_text makho (at 159.258 91.5035) (layer F.Cu))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154 83) (xy 167.5 83) (xy 167.5 92.5) (xy 154 92.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154 83) (xy 167.5 83) (xy 167.5 92.5) (xy 154 92.5)
      )
    )
  )
)
