(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 57)
    (no_connects 0)
    (area 114.224999 48.377 190.575001 121.469)
    (thickness 1.6)
    (drawings 39)
    (tracks 270)
    (zones 0)
    (modules 27)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.4)
    (uvia_drill 0.2)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/Users/Eduardo Hernandez/Documents/PCBs/Modulo_I2C/gerber/"))
  )
  (net 0 "")
  (net 1 MOTOR-)
  (net 2 +24VCD)
  (net 3 SDA)
  (net 4 GND)
  (net 5 +5V)
  (net 6 SCL)
  (net 7 GND_DRIVER)
  (net 8 "Net-(Q1-Pad1)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(R2-Pad2)")
  (net 11 "Net-(R3-Pad2)")
  (net 12 "Net-(R6-Pad1)")
  (net 13 "Net-(R6-Pad2)")
  (net 14 OUT4)
  (net 15 OUT2)
  (net 16 OUT3)
  (net 17 IN4)
  (net 18 IN3)
  (net 19 IN2)
  (net 20 IN1)
  (net_class Default "Este es el tipo de red por defecto."
    (clearance 0.3)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
    (add_net +5V)
    (add_net GND)
    (add_net IN1)
    (add_net IN2)
    (add_net IN3)
    (add_net IN4)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net OUT2)
    (add_net OUT3)
    (add_net OUT4)
    (add_net SCL)
    (add_net SDA)
  )
  (net_class MOTOR ""
    (clearance 0.3)
    (trace_width 2)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
    (add_net +24VCD)
    (add_net GND_DRIVER)
    (add_net MOTOR-)
  )
  (module w_conn_kk100:kk100_22-23-2061 (layer F.Cu) (tedit 0)
    (at 161.15 61.5762)
    (descr "6 pin vert. connector, Molex KK100 series")
    (fp_text reference P1 (at 0 -4.318) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 4.56946) (layer F.SilkS))
    (pad 4 thru_hole oval (at 1.27 -0.0762) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 SDA))
    (pad 3 thru_hole oval (at -1.27 -0.0762) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 6 thru_hole oval (at 6.35 -0.0762) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 5 thru_hole oval (at 3.81 -0.0762) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 SCL))
    (pad 1 thru_hole rect (at -6.35 -0.0762) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND_DRIVER))
    (pad 2 thru_hole oval (at -3.81 -0.0762) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +24VCD))
    (model walter/conn_kk100/22-23-2061.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "../../../../../../Users/Eduardo Hernandez/Downloads/Librerias KiCad/walter/conn_kk100/22-23-2061.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_kk100:kk100_22-23-2061 (layer F.Cu) (tedit 0)
    (at 147.5 108.5 180)
    (descr "6 pin vert. connector, Molex KK100 series")
    (fp_text reference P2 (at 0 -4.318 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 4.56946 180) (layer F.SilkS))
    (pad 4 thru_hole oval (at 1.27 -0.0762 180) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 SDA))
    (pad 3 thru_hole oval (at -1.27 -0.0762 180) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 6 thru_hole oval (at 6.35 -0.0762 180) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 5 thru_hole oval (at 3.81 -0.0762 180) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 SCL))
    (pad 1 thru_hole rect (at -6.35 -0.0762 180) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND_DRIVER))
    (pad 2 thru_hole oval (at -3.81 -0.0762 180) (size 1.524 2.1971) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +24VCD))
    (model walter/conn_kk100/22-23-2061.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "../../../../../../Users/Eduardo Hernandez/Downloads/Librerias KiCad/walter/conn_kk100/22-23-2061.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 57CED974)
    (at 162.04 91.5 270)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 4 -3.96 270) (layer F.SilkS))
    (fp_text value PC817 (at 3.5 0.54 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R6-Pad1)"))
    (pad 3 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(Q1-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +24VCD))
    (model Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED99A)
    (at 166.376 85.238 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R11 (at -2.624 -0.262 180) (layer F.SilkS))
    (fp_text value 1K (at 5.08 0.238 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 IN4))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED997)
    (at 166.376 81.7376 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at -2.624 -0.2624 180) (layer F.SilkS))
    (fp_text value 1K (at 5.08 0.2376 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 IN3))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED994)
    (at 166.376 78.2376 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at -2.624 -0.2624 180) (layer F.SilkS))
    (fp_text value 1K (at 4.876 0.2376 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 IN2))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED990)
    (at 166.5 74.5 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at -2.5 0 180) (layer F.SilkS))
    (fp_text value 1K (at 5.08 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 IN1))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED98C)
    (at 166.5 71 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at -2.5 0 180) (layer F.SilkS))
    (fp_text value 10K (at 5 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 GND_DRIVER))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED9A0)
    (at 134.147 84.7305 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 12.2305 -0.647 90) (layer F.SilkS))
    (fp_text value 470 (at 5.2305 -0.147 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(R6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(R6-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED9A4)
    (at 137.647 84.7305 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 12.2305 0.353 90) (layer F.SilkS))
    (fp_text value 10K (at 5.2305 -0.147 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 SCL))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED9A8)
    (at 141.147 84.7305 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 12.2305 0.353 90) (layer F.SilkS))
    (fp_text value 10K (at 5.2305 -0.147 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 SDA))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED9AC)
    (at 144.647 84.7305 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 12.2305 0.353 90) (layer F.SilkS))
    (fp_text value 1K (at 5.08 -0.147 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED9AF)
    (at 148.147 84.7305 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 12.2305 0.353 90) (layer F.SilkS))
    (fp_text value 1K (at 5.2305 0.353 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(R2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57CED9B9)
    (at 151.647 84.7305 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 12.2305 0.353 90) (layer F.SilkS))
    (fp_text value 1K (at 5.08 -0.147 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Horizontal (layer F.Cu) (tedit 57CED968)
    (at 124.96 84.5)
    (descr "TO-220, Neutral, Horizontal,")
    (tags "TO-220, Neutral, Horizontal,")
    (fp_text reference Q1 (at 0 -22.3012) (layer F.SilkS))
    (fp_text value IRF540N (at -0.29972 -8) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 MOTOR-))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(Q1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND_DRIVER))
    (pad "" np_thru_hole circle (at 0 -16.764 90) (size 3.79984 3.79984) (drill 3.79984) (layers *.Cu *.Mask F.SilkS))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-8pol (layer F.Cu) (tedit 57CED987)
    (at 176 96 90)
    (descr "8-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P5 (at 6.5 -6.5 90) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 17 -3.5 90) (layer F.SilkS))
    (pad 8 thru_hole circle (at 35 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 7 thru_hole circle (at 30 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 17 IN4))
    (pad 6 thru_hole circle (at 25 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 5 thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 18 IN3))
    (pad 4 thru_hole circle (at 15 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 3 thru_hole circle (at 10 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 19 IN2))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 IN1))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-8pol.wrl
      (at (xyz 0.68897 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 57CED982)
    (at 124.5 107)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P4 (at 2.5 -6.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.5 -3.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 +24VCD))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 MOTOR-))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-3pol (layer F.Cu) (tedit 57CED97D)
    (at 168 107)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P3 (at 5 -6) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5 -4) (layer F.SilkS))
    (pad 3 thru_hole circle (at 10 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 OUT4))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 OUT2))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 OUT3))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-3pol.wrl
      (at (xyz 0.1968 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:hole (layer F.Cu) (tedit 576C52E9)
    (at 117.5 117.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:hole (layer F.Cu) (tedit 576C52E9)
    (at 187.5 117.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:hole (layer F.Cu) (tedit 576C52E9)
    (at 187.5 52.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:hole (layer F.Cu) (tedit 576C52E9)
    (at 117.5 52.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value "" (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module w_switch:dip_1-300 (layer F.Cu) (tedit 0)
    (at 148.25 63.56 180)
    (descr "Dip switch, DIL2 x 0,3\"")
    (tags DIP)
    (fp_text reference SW1 (at 0 -6.35 180) (layer F.SilkS))
    (fp_text value SW_DIP_1 (at 0 6.604 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 3.81 180) (size 1.4986 2.1971) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 0 -3.81 180) (size 1.4986 2.1971) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model "../../../../../../Users/Eduardo Hernandez/Downloads/Librerias KiCad/walter/switch/dip_1-300.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:dip_1-300 (layer F.Cu) (tedit 0)
    (at 145.75 63.56 180)
    (descr "Dip switch, DIL2 x 0,3\"")
    (tags DIP)
    (fp_text reference SW2 (at 0 -6.35 180) (layer F.SilkS))
    (fp_text value SW_DIP_1 (at 0 6.604 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 3.81 180) (size 1.4986 2.1971) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R2-Pad2)"))
    (pad 2 thru_hole oval (at 0 -3.81 180) (size 1.4986 2.1971) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model "../../../../../../Users/Eduardo Hernandez/Downloads/Librerias KiCad/walter/switch/dip_1-300.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:dip_1-300 (layer F.Cu) (tedit 0)
    (at 143.25 63.56 180)
    (descr "Dip switch, DIL2 x 0,3\"")
    (tags DIP)
    (fp_text reference SW3 (at 0 -6.35 180) (layer F.SilkS))
    (fp_text value SW_DIP_1 (at 0 6.604 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 3.81 180) (size 1.4986 2.1971) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R3-Pad2)"))
    (pad 2 thru_hole oval (at 0 -3.81 180) (size 1.4986 2.1971) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model "../../../../../../Users/Eduardo Hernandez/Downloads/Librerias KiCad/walter/switch/dip_1-300.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_diodes:diode_do15 (layer F.Cu) (tedit 57CDE6EA)
    (at 135.5 65 90)
    (descr "Diode, DO-15 package")
    (fp_text reference D1 (at 2.5 -3 90) (layer F.SilkS))
    (fp_text value 1N4001 (at -1 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -6 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 +24VCD))
    (pad 2 thru_hole circle (at 6 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 MOTOR-))
    (model walter/pth_diodes/diode_do15.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "../../../../../../Users/Eduardo Hernandez/Downloads/Librerias KiCad/walter/pth_diodes/diode_do15.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pth_circuits:dil_16-300 (layer F.Cu) (tedit 0)
    (at 141.15 93.69)
    (descr "IC, DIL16 x 0,3\"")
    (tags DIL)
    (fp_text reference U1 (at 0 -6.35) (layer F.SilkS))
    (fp_text value PCF8574 (at 0 6.604) (layer F.SilkS))
    (pad 1 thru_hole oval (at -8.89 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at -6.35 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R2-Pad2)"))
    (pad 3 thru_hole oval (at -3.81 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R3-Pad2)"))
    (pad 4 thru_hole oval (at -1.27 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R6-Pad2)"))
    (pad 5 thru_hole oval (at 1.27 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 OUT2))
    (pad 6 thru_hole oval (at 3.81 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 OUT3))
    (pad 7 thru_hole oval (at 6.35 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 OUT4))
    (pad 8 thru_hole oval (at 8.89 3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 9 thru_hole oval (at 8.89 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 IN1))
    (pad 10 thru_hole oval (at 6.35 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 IN2))
    (pad 11 thru_hole oval (at 3.81 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 IN3))
    (pad 12 thru_hole oval (at 1.27 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 IN4))
    (pad 13 thru_hole oval (at -1.27 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at -3.81 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 SCL))
    (pad 15 thru_hole oval (at -6.35 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 SDA))
    (pad 16 thru_hole oval (at -8.89 -3.81) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (model walter/pth_circuits/dil_16-300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "../../../../../../Users/Eduardo Hernandez/Downloads/Librerias KiCad/walter/pth_circuits/dil_16-300.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 114.3 120.65) (end 114.3 49.53) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 120.65) (end 114.3 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 49.53) (end 190.5 120.65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 49.53) (end 190.5 49.53) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "VENDING CONTROL I2C_V1.0" (at 116.75 101 90) (layer F.Cu))
  (gr_text "HECHO EN MEXICO" (at 183.75 52.5) (layer B.Cu))
  (gr_text "SisConElectric\nVENDING CONTROL I2C_V1.1\n" (at 183.5 116.5) (layer B.Cu))
  (gr_text SENSORS (at 186.5 79 90) (layer F.SilkS))
  (gr_text OUTPUT (at 147 116.5) (layer F.SilkS))
  (gr_text INPUT (at 162.5 54) (layer F.SilkS))
  (gr_text ADDRESS (at 146 55.5) (layer F.SilkS))
  (gr_text A0 (at 150 57.5) (layer F.SilkS))
  (gr_text A1 (at 146 57.5) (layer F.SilkS))
  (gr_text A2 (at 142 57.5) (layer F.SilkS))
  (gr_text +5VCD (at 167.5 56 90) (layer F.SilkS))
  (gr_text SCL (at 165 57 90) (layer F.SilkS))
  (gr_text SDA (at 162.5 57 90) (layer F.SilkS))
  (gr_text GND (at 160 57 90) (layer F.SilkS))
  (gr_text +24VCD (at 157.5 56 90) (layer F.SilkS))
  (gr_text "GND\nDRIVER" (at 154.5 56 90) (layer F.SilkS))
  (gr_text IN1 (at 183 96) (layer F.SilkS))
  (gr_text -5VCD (at 183 91) (layer F.SilkS))
  (gr_text IN2 (at 183 86) (layer F.SilkS))
  (gr_text +5VCD (at 183 81) (layer F.SilkS))
  (gr_text IN3 (at 183 76) (layer F.SilkS))
  (gr_text +5VCD (at 183 71) (layer F.SilkS))
  (gr_text IN4 (at 183 66) (layer F.SilkS))
  (gr_text +5VCD (at 183 61) (layer F.SilkS))
  (gr_text OUT4 (at 178.5 114 270) (layer F.SilkS))
  (gr_text OUT3 (at 173.5 114 270) (layer F.SilkS))
  (gr_text OUT2 (at 169 114 270) (layer F.SilkS))
  (gr_text "GND\nDRIVER" (at 154.5 114 270) (layer F.SilkS))
  (gr_text +24VCD (at 151.5 114.5 270) (layer F.SilkS))
  (gr_text GND (at 149 113.5 270) (layer F.SilkS))
  (gr_text SDA (at 146.5 113.5 270) (layer F.SilkS))
  (gr_text SCL (at 144 113.5 270) (layer F.SilkS))
  (gr_text +5VCD (at 141.5 114 270) (layer F.SilkS))
  (gr_text MOTOR- (at 129.5 114.5 270) (layer F.SilkS))
  (gr_text MOTOR+ (at 124.5 114.5 270) (layer F.SilkS))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 50) (xy 190 50) (xy 190 120) (xy 115 120)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 50) (xy 190 50) (xy 190 120) (xy 115 120)
      )
    )
  )
)
