(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu17.04.1)
  (general
    (links 29)
    (no_connects 0)
    (area 134.544999 86.284999 162.635001 123.265001)
    (thickness 1.6)
    (drawings 32)
    (tracks 94)
    (zones 0)
    (modules 8)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFF5E21)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad10)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J2-Pad4)")
  (net 10 "Net-(J1-Pad5)")
  (net 11 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad1)")
  )
  (module kflopbreakout:rj45-shield2 (layer F.Cu) (tedit 59F2D071)
    (at 148.59 92.71 180)
    (descr "RJ45, shielded")
    (fp_text reference "Wurth 615008140621" (at 0 -7.62 180) (layer F.SilkS))
    (fp_text value RJ45->HEDL-Encoder (at 0 -9.525 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 1.52146 -2.48412 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 3.55092 -2.48412 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.53746 -4.26466 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 0.508 -4.26466 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -0.508 -2.48412 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -1.52146 -4.26466 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -2.53746 -2.48412 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -3.55092 -4.26466 180) (size 1.19888 1.19888) (drill 0.8001) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 10 thru_hole circle (at -8.12038 -3.37312 180) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad10)"))
    (pad 9 thru_hole circle (at 8.12038 -3.37312 180) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad10)"))
    (pad "" np_thru_hole circle (at -6.33984 0.05588 180) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu))
    (pad "" np_thru_hole circle (at 6.33984 0.05588 180) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu))
    (model walter/conn_pc/rj45-shield.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 59F2CC3F)
    (at 160.02 105.0141 270)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J2 (at 0 -6.35 270) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19 270) (layer F.Fab))
    (fp_text user %R (at 0 11.43 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 59F2CC44)
    (at 160.02 111.76 270)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J3 (at 0 -6.35 270) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19 270) (layer F.Fab))
    (fp_text user %R (at 0 11.43 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 59F2CC55)
    (at 153.67 118.11 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J4 (at -2.54 22.86 270) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 1.27 12.49 270) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59F2D14B)
    (at 137.16 88.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference M3 (at -1.27 2.54) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59F2D153)
    (at 160.02 88.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference M3 (at 1.27 2.54) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59F2D15D)
    (at 137.16 120.65)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference M3 (at -1.27 -2.54) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59F2CF52)
    (at 160.02 120.65)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference M3 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text Z (at 137.16 109.22) (layer B.SilkS))
  (gr_text ~Z (at 139.7 109.22) (layer B.SilkS))
  (gr_text B (at 142.24 109.22) (layer B.SilkS))
  (gr_text ~B (at 144.78 109.22) (layer B.SilkS))
  (gr_text A (at 147.32 109.22) (layer B.SilkS))
  (gr_text ~A (at 149.86 109.22) (layer B.SilkS))
  (gr_text G (at 154.94 109.22) (layer B.SilkS))
  (gr_text 5 (at 157.48 109.22) (layer B.SilkS))
  (gr_text Z (at 137.16 109.22) (layer F.Paste))
  (gr_text ~Z (at 139.7 109.22) (layer F.Paste))
  (gr_text B (at 142.24 109.22) (layer F.Paste))
  (gr_text ~B (at 144.78 109.22) (layer F.Paste))
  (gr_text A (at 147.32 109.22) (layer F.Paste))
  (gr_text ~A (at 149.86 109.22) (layer F.Paste))
  (gr_text G (at 154.94 109.22) (layer F.Paste))
  (gr_text 5 (at 157.48 109.22) (layer F.Paste))
  (gr_text 5 (at 157.48 109.22) (layer F.SilkS))
  (gr_text Z (at 137.16 109.22) (layer F.SilkS))
  (gr_text ~Z (at 139.7 109.22) (layer F.SilkS))
  (gr_text G (at 154.94 109.22) (layer F.SilkS))
  (gr_text B (at 142.24 109.22) (layer F.SilkS))
  (gr_text ~B (at 144.78 109.22) (layer F.SilkS))
  (gr_text A (at 147.32 109.22) (layer F.SilkS))
  (gr_text ~A (at 149.86 109.22) (layer F.SilkS))
  (gr_line (start 134.62 123.19) (end 134.62 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 123.19) (end 134.62 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 86.36) (end 162.56 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 86.36) (end 162.56 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 105.41) (end 134.62 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
)
