(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 54)
    (no_connects 2)
    (area 72.949999 69.774999 99.770001 121.360001)
    (thickness 1.6)
    (drawings 44)
    (tracks 104)
    (zones 0)
    (modules 19)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.8)
    (zone_45_only yes)
    (trace_min 0.25)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (user_via 3.5 3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.55 1.3)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(P1-Pad4)")
  (net 4 "Net-(P1-Pad5)")
  (net 5 "Net-(P1-Pad6)")
  (net 6 "Net-(P1-Pad7)")
  (net 7 "Net-(P1-Pad8)")
  (net 8 "Net-(P2-Pad1)")
  (net 9 "Net-(P2-Pad2)")
  (net 10 "Net-(P2-Pad3)")
  (net 11 "Net-(P2-Pad4)")
  (net 12 "Net-(P2-Pad6)")
  (net 13 "Net-(P2-Pad7)")
  (net 14 "Net-(P2-Pad5)")
  (net 15 VCC)
  (net 16 "Net-(P5-Pad1)")
  (net 17 "Net-(P1-Pad10)")
  (net 18 "Net-(P1-Pad9)")
  (net 19 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P5-Pad1)")
    (add_net VCC)
  )
  (net_class Thick ""
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
  )
  (module CPB:ESP-12Emin (layer F.Cu) (tedit 58D700A7)
    (at 79.375 73.025)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 0.381 -1.651) (layer F.SilkS))
    (fp_text value ESP-12E (at 8.255 5.08) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad10)"))
    (pad 2 thru_hole oval (at 0 2) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P1-Pad9)"))
    (pad 3 thru_hole oval (at 0 4) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad8)"))
    (pad 4 thru_hole oval (at 0 6) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad7)"))
    (pad 5 thru_hole oval (at 0 8) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad6)"))
    (pad 6 thru_hole oval (at 0 10) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad5)"))
    (pad 7 thru_hole oval (at 0 12) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad4)"))
    (pad 8 thru_hole oval (at 0 14) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 9 thru_hole oval (at 14 14) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 14 12) (size 2.5 1.1) (drill 0.65 (offset 0.6 0)) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P2-Pad7)"))
    (pad 11 thru_hole oval (at 14 10) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad6)"))
    (pad 12 thru_hole oval (at 14 8) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P2-Pad5)"))
    (pad 13 thru_hole oval (at 14 6) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad4)"))
    (pad 14 thru_hole oval (at 14 4) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P2-Pad3)"))
    (pad 15 thru_hole oval (at 14 2) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P2-Pad2)"))
    (pad 16 thru_hole oval (at 14 0) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad1)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 58CEE760)
    (at 94.615 108.585 90)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P5 (at 2.667 -1.524 90) (layer F.SilkS))
    (fp_text value PWR (at 2.54 1.905 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 58CEE378)
    (at 74.93 94.615 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 24.13 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad10)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 58CF1492)
    (at 75.946 102.235 270)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 0.127 1.651 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.27 -1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 58CF117F)
    (at 84.455 99.06 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.397 0.762 90) (layer F.SilkS))
    (fp_text value 100n (at 1.397 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58CF1426)
    (at 78.105 98.425 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.064 0 90) (layer F.SilkS))
    (fp_text value 10k (at 3.937 0.508 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(P1-Pad8)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58CF1429)
    (at 81.28 98.425 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 3.937 0 90) (layer F.SilkS))
    (fp_text value 10k (at 3.937 0.635 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(P1-Pad10)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58CF1438)
    (at 93.98 90.805 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 10k (at 3.683 -0.635 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(P2-Pad7)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58CF142E)
    (at 83.947 90.932)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0.635) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 "Net-(P2-Pad5)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 58CF1497)
    (at 75.946 110.744 90)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 10uF (at 1.27 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 VCC))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CPB:SW_SPST_PTS645 (layer F.Cu) (tedit 58D70115)
    (at 78.105 116.205 180)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (fp_text reference SW1 (at -0.127 -0.127 180) (layer F.SilkS))
    (fp_text value RST (at -0.127 -1.524 180) (layer F.Fab))
    (pad 2 thru_hole rect (at -3.81 2.54 180) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad10)"))
    (pad 1 thru_hole rect (at -3.81 -2.54 180) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 3.81 -2.54 180) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 3.81 2.54 180) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad10)"))
  )
  (module CPB:SW_SPST_PTS645 (layer F.Cu) (tedit 58D70136)
    (at 88.265 116.205)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (fp_text reference SW2 (at 0 0.127) (layer F.SilkS))
    (fp_text value PRG (at 0.127 1.778) (layer F.Fab))
    (pad 2 thru_hole rect (at -3.81 2.54) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -3.81 -2.54) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P2-Pad5)"))
    (pad 1 thru_hole rect (at 3.81 -2.54) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P2-Pad5)"))
    (pad 2 thru_hole rect (at 3.81 2.54) (size 1.55 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module CPB:DPDT6_DIP_SW (layer F.Cu) (tedit 58CF0F6B)
    (at 96.52 116.078 90)
    (fp_text reference SW3 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value SPST (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 -1.27 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 VCC))
    (pad 2 thru_hole circle (at 0 -1.27 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P5-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 -1.27 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P5-Pad1)"))
    (pad 4 thru_hole circle (at 2.54 1.27 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -2.54 1.27 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  )
  (module CPB:AMS1117_HT73 (layer F.Cu) (tedit 58D6A651)
    (at 82.55 105.918)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 2.159 -0.635) (layer F.SilkS))
    (fp_text value AP1117E33 (at 0 0.762 180) (layer F.Fab))
    (pad 4 thru_hole rect (at 0 -3.302) (size 3.6576 2.032) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 thru_hole rect (at 2.286 3.302) (size 1.016 2.032) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 VCC))
    (pad 1 thru_hole rect (at -2.286 3.302) (size 1.016 2.032) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 58CEE37D)
    (at 97.79 71.755)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 58CEE6D7)
    (at 87.757 107.823 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value Socket_Strip_Straight_1x02 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 58CF118C)
    (at 88.9 99.314 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.524 -1.778 90) (layer F.SilkS))
    (fp_text value Led_Small (at 1.3 -2.9 90) (layer F.Fab) hide)
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 58D6A72F)
    (at 91.567 93.853 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference RLED (at 3.683 0 180) (layer F.SilkS))
    (fp_text value 100R (at 3.429 -0.508 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +3V3))
  )
  (module Connect:1pin (layer F.Cu) (tedit 58D700AE)
    (at 85.852 85.344)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text 3V3 (at 82.677 100.838) (layer F.SilkS))
  (gr_text VCC (at 84.836 111.125) (layer F.SilkS))
  (gr_text GND (at 80.264 111.125) (layer F.SilkS))
  (gr_text VCC (at 87.757 110.871 90) (layer F.SilkS))
  (gr_text GND (at 87.884 102.362 90) (layer F.SilkS))
  (gr_text "ESP-12\ndevboard\nbeauregardcp\n@gmail" (at 87.884 78.105 90) (layer B.SilkS))
  (gr_text "ESP-12\ndevboard\nbeauregardcp\n@gmail" (at 88.138 77.978 90) (layer F.SilkS))
  (gr_text "GND\n" (at 97.79 97.409) (layer F.SilkS))
  (gr_text 15 (at 95.885 87.122 90) (layer F.SilkS))
  (gr_text 2 (at 95.885 84.455 90) (layer F.SilkS))
  (gr_text 0 (at 95.885 82.042 90) (layer F.SilkS))
  (gr_text 4 (at 95.885 79.883 90) (layer F.SilkS))
  (gr_text 5 (at 96.012 76.962 90) (layer F.SilkS))
  (gr_text RX (at 95.885 74.422 90) (layer F.SilkS))
  (gr_text TX (at 96.012 71.628 90) (layer F.SilkS))
  (gr_text 3V3 (at 74.93 97.409) (layer F.SilkS))
  (gr_text 13 (at 76.835 86.995 90) (layer F.SilkS))
  (gr_text 12 (at 76.835 84.582 90) (layer F.SilkS))
  (gr_text 14 (at 76.835 81.788 90) (layer F.SilkS))
  (gr_text 16 (at 76.835 79.248 90) (layer F.SilkS))
  (gr_text CH (at 76.835 76.708 90) (layer F.SilkS))
  (gr_text RS (at 76.835 71.755 90) (layer F.SilkS))
  (gr_text AD (at 76.835 74.295 90) (layer F.SilkS))
  (gr_text GND (at 98.298 103.886 270) (layer B.SilkS))
  (gr_text VCC (at 98.298 108.966 270) (layer B.SilkS))
  (gr_text VCC (at 98.298 108.966 90) (layer F.SilkS))
  (gr_text GND (at 98.298 103.124 90) (layer F.SilkS))
  (gr_text ON (at 96.52 120.65) (layer F.SilkS))
  (gr_text PROG (at 88.646 120.396) (layer F.SilkS))
  (gr_text RESET (at 78.232 120.396) (layer F.SilkS))
  (gr_line (start 73.025 121.285) (end 73.025 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.695 121.285) (end 73.025 121.285) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.695 69.85) (end 99.695 121.285) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.025 69.85) (end 99.695 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.105 64.135) (xy 78.105 70.485) (xy 94.615 70.485) (xy 94.615 64.135)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.8) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 73.025 69.85) (xy 99.695 69.85) (xy 99.695 121.285) (xy 73.025 121.285)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.708 96.52) (xy 73.152 96.52) (xy 73.152 88.392) (xy 76.708 88.392) (xy 76.708 96.52)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.885 96.52) (xy 95.885 96.393) (xy 95.886984 96.393) (xy 95.885 96.52)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.012 88.392) (xy 99.695 88.392) (xy 99.695 96.393) (xy 95.886984 96.393) (xy 96.012 88.392)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.107 117.221) (xy 99.06 117.221) (xy 99.06 120.015) (xy 94.107 120.015)
      )
    )
  )
)
