(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 14)
    (no_connects 0)
    (area 148.514999 100.254999 158.825001 118.185001)
    (thickness 1.6)
    (drawings 10)
    (tracks 75)
    (zones 0)
    (modules 3)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J2-Pad1)")
  (net 9 "Net-(J2-Pad2)")
  (net 10 "Net-(J2-Pad3)")
  (net 11 "Net-(J2-Pad4)")
  (net 12 "Net-(J2-Pad5)")
  (net 13 "Net-(J2-Pad6)")
  (net 14 "Net-(J2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer B.Cu) (tedit 595B3313)
    (at 149.86 101.6 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X07 (at 0 -17.57 180) (layer B.Fab))
    (fp_text user %R (at 0 2.33 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer B.Cu) (tedit 595B3315)
    (at 157.48 101.6 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X07 (at 0 -17.57 180) (layer B.Fab))
    (fp_text user %R (at 0 2.33 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TSSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 595C342E)
    (at 153.67 109.265 90)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP]")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -3.55 90) (layer F.SilkS) hide)
    (fp_text value TSSOP (at 4.49 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.8 -1.95 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.8 -1.3 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -2.8 -0.65 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -2.8 0 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -2.8 0.65 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -2.8 1.3 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -2.8 1.95 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 2.8 1.95 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad7)"))
    (pad 9 smd rect (at 2.8 1.3 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad6)"))
    (pad 10 smd rect (at 2.8 0.65 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad5)"))
    (pad 11 smd rect (at 2.8 0 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad4)"))
    (pad 12 smd rect (at 2.8 -0.65 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 13 smd rect (at 2.8 -1.3 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 14 smd rect (at 2.8 -1.95 90) (size 1.6 0.35) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "github.com/\nrpwoodbu/\ntssop_14_breakout" (at 153.67 117.856 270) (layer B.SilkS))
  (gr_text 8 (at 156.21 116.84) (layer F.SilkS))
  (gr_text 7 (at 151.13 116.84) (layer F.SilkS))
  (gr_text 14 (at 156.21 101.6) (layer F.SilkS))
  (gr_text 1 (at 151.13 101.6) (layer F.SilkS))
  (gr_text "rpwoodbu\njbebel\nv1" (at 153.67 100.584 270) (layer B.SilkS))
  (gr_line (start 148.59 118.11) (end 148.59 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 118.11) (end 148.59 118.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 100.33) (end 158.75 118.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 100.33) (end 158.75 100.33) (layer Edge.Cuts) (width 0.15))
)
