<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="1.651" y1="0" x2="37.846" y2="0" width="0.2032" layer="20"/>
<wire x1="37.846" y1="0" x2="39.37" y2="1.524" width="0.2032" layer="20"/>
<wire x1="39.37" y1="1.524" x2="40.894" y2="0" width="0.2032" layer="20"/>
<wire x1="40.894" y1="0" x2="55.88" y2="0" width="0.2032" layer="20"/>
<wire x1="55.88" y1="0" x2="57.15" y2="1.27" width="0.2032" layer="20"/>
<wire x1="57.15" y1="1.27" x2="57.15" y2="3.81" width="0.2032" layer="20"/>
<wire x1="57.15" y1="3.81" x2="59.69" y2="6.35" width="0.2032" layer="20"/>
<wire x1="59.69" y1="6.35" x2="59.69" y2="21.59" width="0.2032" layer="20"/>
<wire x1="59.69" y1="21.59" x2="57.15" y2="24.13" width="0.2032" layer="20"/>
<wire x1="57.15" y1="24.13" x2="57.15" y2="26.67" width="0.2032" layer="20"/>
<wire x1="57.15" y1="26.67" x2="59.69" y2="29.21" width="0.2032" layer="20"/>
<wire x1="59.69" y1="29.21" x2="59.69" y2="41.91" width="0.2032" layer="20"/>
<wire x1="59.69" y1="41.91" x2="57.15" y2="44.45" width="0.2032" layer="20"/>
<wire x1="57.15" y1="44.45" x2="57.15" y2="52.07" width="0.2032" layer="20"/>
<wire x1="57.15" y1="52.07" x2="55.88" y2="53.34" width="0.2032" layer="20"/>
<wire x1="55.88" y1="53.34" x2="36.449" y2="53.34" width="0.2032" layer="20"/>
<wire x1="36.449" y1="53.34" x2="34.925" y2="51.816" width="0.2032" layer="20"/>
<wire x1="34.925" y1="51.816" x2="33.401" y2="53.34" width="0.2032" layer="20"/>
<wire x1="33.401" y1="53.34" x2="13.335" y2="53.34" width="0.2032" layer="20"/>
<wire x1="13.335" y1="53.34" x2="12.065" y2="52.07" width="0.2032" layer="20"/>
<wire x1="12.065" y1="52.07" x2="9.525" y2="52.07" width="0.2032" layer="20"/>
<wire x1="9.525" y1="52.07" x2="8.255" y2="53.34" width="0.2032" layer="20"/>
<wire x1="8.255" y1="53.34" x2="5.08" y2="53.34" width="0.2032" layer="20"/>
<wire x1="3.81" y1="51.943" x2="3.81" y2="49.53" width="0.2032" layer="20"/>
<wire x1="3.81" y1="49.53" x2="2.54" y2="48.26" width="0.2032" layer="20"/>
<wire x1="2.54" y1="48.26" x2="2.54" y2="21.971" width="0.2032" layer="20"/>
<wire x1="2.54" y1="21.971" x2="-0.254" y2="19.177" width="0.2032" layer="20"/>
<wire x1="-0.254" y1="19.177" x2="-0.254" y2="2.286" width="0.2032" layer="20"/>
<wire x1="3.81" y1="51.943" x2="5.08" y2="53.34" width="0.2032" layer="20"/>
<wire x1="-0.254" y1="2.286" x2="1.651" y2="0" width="0.2032" layer="20"/>
<text>D6</text>
<text>D9</text>
<text>D10</text>
<text>D11</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>kaleidoscope</text>
<text>leds</text>
<text>leds</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>batteries-&gt;</text>
<text>butterfly
power</text>
<text>board
power</text>
<text>butterfly
power</text>
<text>always on -&gt;</text>
<text>kaleidoscope</text>
<text>butterfly army</text>
<text>PROGRAMMED WITH INTEL CURIE</text>
<text>PROGRAMMED WITH INTEL CURIE</text>
<text>butterfly army</text>
<text>butterfly army</text>
<text>-</text>
<text>-</text>
<text>v1.12</text>
<text>so powerful</text>
<text>a5</text>
<text>a4</text>
<text>button</text>
<text>button</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="DUEMILANOVE_SHIELD">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="pololu">
<packages>
<package name="1_8V_500MA_REG">
</package>
<package name="5V_STEPUP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-THM">
<description>4UCon #01528
http://www.4uconnector.com/online/object/4udrawing/01528.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="JST-3-PTH">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun" package="DUEMILANOVE_SHIELD" value="Arduino"/>
<element name="Q1" library="SparkFun" package="TO220V" value="IRF"/>
<element name="Q2" library="SparkFun" package="TO220V" value="IRF"/>
<element name="Q3" library="SparkFun" package="TO220V" value="IRF"/>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="AXIAL-0.3" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="AXIAL-0.3" value="10K">
<attribute name="VALUE"/>
</element>
<element name="Q4" library="SparkFun" package="TO220V" value="IRF"/>
<element name="R4" library="SparkFun" package="AXIAL-0.3" value="10K">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value=""/>
<element name="JP9" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value=""/>
<element name="JP10" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value=""/>
<element name="JP11" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value=""/>
<element name="U$1" library="pololu" package="1_8V_500MA_REG" value="1_8V_500MA_REG">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="pololu" package="1_8V_500MA_REG" value="1_8V_500MA_REG">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="pololu" package="1_8V_500MA_REG" value="1_8V_500MA_REG">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="pololu" package="1_8V_500MA_REG" value="1_8V_500MA_REG">
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="JP3" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.3EZ" value=""/>
<element name="U$5" library="pololu" package="5V_STEPUP" value="5V_STEPUP">
<attribute name="VALUE"/>
</element>
<element name="CN2" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="CN3" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="R6" library="SparkFun" package="AXIAL-0.3" value="10K"/>
<element name="CN4" library="adafruit" package="JST-PH-2-THM" value=""/>
<element name="R7" library="SparkFun" package="AXIAL-0.3" value="10K"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.3EZ" value=""/>
<element name="JP5" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="JST-3-PTH" value=""/>
<element name="JP4" library="SparkFun-Passives" package="SJ_2S" value="">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="AXIAL-0.3" value=" 0.1Ω"/>
<element name="R10" library="SparkFun" package="AXIAL-0.3" value=" 0.1Ω"/>
<element name="R11" library="SparkFun" package="AXIAL-0.3" value=" 0.1Ω"/>
<element name="R12" library="SparkFun" package="AXIAL-0.3" value=" 0.1Ω"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q1" pad="3"/>
<contactref element="R4" pad="P$1"/>
<contactref element="Q4" pad="3"/>
<contactref element="U1" pad="GND@2"/>
<contactref element="U1" pad="GND@1"/>
<contactref element="U1" pad="GND@0"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$2" pad="GND"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$4" pad="GND"/>
<contactref element="CN1" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="U$5" pad="GND"/>
<contactref element="CN2" pad="2"/>
<contactref element="CN3" pad="2"/>
<contactref element="CN4" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="D11-1.8V">
<contactref element="Q1" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="D10-1.8V">
<contactref element="Q2" pad="2"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="D9-1.8V">
<contactref element="Q3" pad="2"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="D11">
<contactref element="U1" pad="D11"/>
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="D10"/>
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="D9"/>
<contactref element="Q3" pad="1"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="D6"/>
<contactref element="Q4" pad="1"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="D5"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="D3"/>
</signal>
<signal name="D6-1.8V">
<contactref element="Q4" pad="2"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="A3_LAT">
<contactref element="U1" pad="A3"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="A4"/>
<contactref element="CN4" pad="1"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="A5"/>
<contactref element="CN2" pad="1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="RES"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="3.3V"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="AREF"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="RX"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="TX"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="D2"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="D4"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="D7"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="D8"/>
</signal>
<signal name="D12">
<contactref element="U1" pad="D12"/>
</signal>
<signal name="D13">
<contactref element="U1" pad="D13"/>
</signal>
<signal name="1.8V">
<contactref element="JP6" pad="2"/>
<contactref element="JP9" pad="2"/>
<contactref element="JP10" pad="2"/>
<contactref element="JP11" pad="2"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R10" pad="P$1"/>
<contactref element="R11" pad="P$1"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="U$5" pad="IN"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="5VDC">
<contactref element="U1" pad="5V"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$5" pad="OUT"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="LED_BAT">
<contactref element="CN1" pad="1"/>
<contactref element="CN3" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="A0_DAT">
<contactref element="U1" pad="A0"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="A1_CLK">
<contactref element="U1" pad="A1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="A2_OE">
<contactref element="U1" pad="A2"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="B_PWR">
<contactref element="U$1" pad="IN"/>
<contactref element="U$2" pad="IN"/>
<contactref element="U$4" pad="IN"/>
<contactref element="U$3" pad="IN"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="P$1"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="P$1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$1">
<contactref element="U$1" pad="OUT"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="OUT"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="OUT"/>
<contactref element="R11" pad="P$2"/>
</signal>
<signal name="N$7">
<contactref element="U$4" pad="OUT"/>
<contactref element="R12" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
