<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="7.62" width="0" layer="20"/>
<wire x1="25.4" y1="7.62" x2="0" y2="7.62" width="0" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="0" width="0" layer="20"/>
<text>(c) 2015 DLB</text>
</plain>
<libraries>
<library name="0-Lantzer">
<packages>
<package name="TP1">
</package>
</packages>
</library>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="RELAY:SPDT-OMRON(G8N-1)">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+" library="0-Lantzer" package="TP1" value="TESTPOINT">
<attribute name="NAME"/>
</element>
<element name="-" library="0-Lantzer" package="TP1" value="TESTPOINT">
<attribute name="NAME"/>
</element>
<element name="C" library="0-Lantzer" package="TP1" value="TESTPOINT">
<attribute name="NAME"/>
</element>
<element name="NC" library="0-Lantzer" package="TP1" value="TESTPOINT">
<attribute name="NAME"/>
</element>
<element name="NO" library="0-Lantzer" package="TP1" value="TESTPOINT">
<attribute name="NAME"/>
</element>
<element name="RELAY" library="QuantumOptics" package="RELAY:SPDT-OMRON(G8N-1)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="+" pad="1"/>
<contactref element="RELAY" pad="P$5"/>
</signal>
<signal name="N$2">
<contactref element="RELAY" pad="P$2"/>
<contactref element="-" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="RELAY" pad="P$1"/>
<contactref element="C" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="RELAY" pad="P$3"/>
<contactref element="NC" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="RELAY" pad="P$4"/>
<contactref element="NO" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
