(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 7)
    (no_connects 0)
    (area 134.601193 91.134385 167.96202 138.227614)
    (thickness 1.6)
    (drawings 23)
    (tracks 39)
    (zones 0)
    (modules 7)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.762)
    (via_drill 0.508)
    (via_min_size 0.762)
    (via_min_drill 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad0)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad17A)")
  (net 10 "Net-(J1-Pad3V1)")
  (net 11 "Net-(J1-PadG2)")
  (net 12 "Net-(J1-PadPGM)")
  (net 13 "Net-(J1-PadDAC)")
  (net 14 "Net-(J1-Pad16)")
  (net 15 "Net-(J1-Pad17)")
  (net 16 "Net-(J1-PadG3)")
  (net 17 "Net-(J1-Pad22)")
  (net 18 "Net-(J1-PadVIN)")
  (net 19 "Net-(J1-Pad21)")
  (net 20 "Net-(J1-Pad20)")
  (net 21 "Net-(J1-Pad23)")
  (net 22 "Net-(J1-Pad14)")
  (net 23 "Net-(J1-Pad15)")
  (net 24 /CS)
  (net 25 /RST)
  (net 26 /GND)
  (net 27 /VIN)
  (net 28 "Net-(J1-Pad4)")
  (net 29 /Data)
  (net 30 /CLK)
  (net 31 /DC)
  (net 32 "Net-(J1-Pad18)")
  (net 33 "Net-(J1-Pad19)")
  (net 34 "Net-(J2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DC)
    (add_net /Data)
    (add_net /GND)
    (add_net /RST)
    (add_net /VIN)
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad17A)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadG2)")
    (add_net "Net-(J1-PadG3)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad3)")
  )
  (module Wickerlib:TEENSY-LC (layer F.Cu) (tedit 5773C019)
    (at 148.5011 105.0036)
    (fp_text reference J1 (at 2.8829 20.2184) (layer F.SilkS) hide)
    (fp_text value TEENSY-LC (at -2.54 20.32 180) (layer F.Fab))
    (fp_text user "TEENSY LC" (at -3.5941 10.5664) (layer F.SilkS) hide)
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Data))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CLK))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DC))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /CS))
    (pad 17A thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad17A)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad3V1)"))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-PadG2)"))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RST))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad16)"))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad17)"))
    (pad G3 thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-PadG3)"))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad15)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5773C005)
    (at 162.687 101.854)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value OLED_128x64 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /CS))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RST))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DC))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CLK))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Data))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 5773BBD6)
    (at 146.05 103.505 90)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912 90) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 90) (layer B.Fab))
  )
  (module Wickerlib:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5773C0FA)
    (at 163.83 95.504 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module teensy-big-oled:osh-park-logo-300dpi-normal-copper (layer F.Cu) (tedit 0)
    (at 145.923 99.695)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module teensy-big-oled:osh-park-logo-300dpi-normal-silk (layer F.Cu) (tedit 0)
    (at 146.177 118.999)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module teensy-big-oled:osh-park-logo-300dpi-normal-silk (layer F.Cu) (tedit 0)
    (at 161.925 127.381)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "drew@oshpark.com\n" (at 146.685 92.964 180) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 136.144 110.998 270) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 145.542 130.175) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 157.226 110.236 270) (layer F.SilkS))
  (gr_text "DREW FUSTINI" (at 159.512 109.982 270) (layer F.SilkS))
  (gr_text "DREW FUSTINI" (at 149.987 104.521 270) (layer B.Cu))
  (gr_text "DREW FUSTINI" (at 149.987 104.521 270) (layer B.Mask))
  (gr_line (start 136.525 91.567) (end 137.16 91.567) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 134.747 93.98) (end 134.747 95.504) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 136.906 93.726) (end 134.747 94.107) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 162.56 91.567) (end 164.465 91.567) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 167.259 95.377) (end 167.259 94.488) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 164.211 94.615) (end 164.338 91.567) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 134.747 128.397) (end 134.747 129.54) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 136.906 132.715) (end 138.176 132.715) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 167.259 128.651) (end 167.259 129.54) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 163.576 129.032) (end 167.259 129.413) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 137.541 129.921) (end 137.033 132.715) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 167.259 94.742) (end 167.259 128.524) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 134.747 128.397) (end 134.747 127.381) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 134.747 95.25) (end 134.747 128.397) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.414 132.715) (end 164.084 132.715) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.033 91.567) (end 164.084 91.567) (angle 90) (layer Edge.Cuts) (width 0.2))
  (zone (net 26) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.763 92.583) (xy 137.16 92.075) (xy 163.957 92.202) (xy 166.37 94.107) (xy 166.37 129.794)
        (xy 163.576 131.953) (xy 137.033 131.953) (xy 135.255 130.175) (xy 135.255 93.599)
      )
    )
  )
  (zone (net 27) (net_name /VIN) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.017 92.202) (xy 163.83 92.329) (xy 166.624 94.488) (xy 166.116 129.54) (xy 162.814 131.699)
        (xy 137.287 131.699) (xy 135.636 130.048) (xy 135.509 94.107)
      )
    )
    (polygon
      (pts        (xy 141.605 96.012) (xy 150.241 96.012) (xy 151.257 96.012) (xy 151.13 113.03) (xy 141.605 113.03)
      )
    )
  )
)
