<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="-1.778" y1="144.9578" x2="-1.778" y2="144.958321875" width="0" layer="20" curve="-0.023544"/>
<wire x1="79.10295" y1="138.57505" x2="84.60005" y2="133.07795" width="0" layer="20"/>
<wire x1="84.60005" y1="133.07795" x2="86.396103125" y2="132.334" width="0" layer="20" curve="45.00007"/>
<wire x1="86.396103125" y1="132.334" x2="89.371896875" y2="132.334" width="0" layer="20"/>
<wire x1="89.371896875" y1="132.334" x2="91.16795" y2="131.59005" width="0" layer="20" curve="-45.00005"/>
<wire x1="91.16795" y1="131.59005" x2="92.72805" y2="130.02995" width="0" layer="20"/>
<wire x1="92.72805" y1="130.02995" x2="93.472" y2="128.233896875" width="0" layer="20" curve="-45.00007"/>
<wire x1="93.472" y1="128.233896875" x2="93.472" y2="69.124103125" width="0" layer="20"/>
<wire x1="93.472" y1="69.124103125" x2="92.72805" y2="67.32805" width="0" layer="20" curve="-45.00005"/>
<wire x1="92.72805" y1="67.32805" x2="91.16795" y2="65.76795" width="0" layer="20"/>
<wire x1="91.16795" y1="65.76795" x2="89.371896875" y2="65.024" width="0" layer="20" curve="-45.00007"/>
<wire x1="89.371896875" y1="65.024" x2="86.396103125" y2="65.024" width="0" layer="20"/>
<wire x1="86.396103125" y1="65.024" x2="84.60005" y2="64.28005" width="0" layer="20" curve="45.00005"/>
<wire x1="84.60005" y1="64.28005" x2="84.590890625" y2="64.270890625" width="0" layer="20"/>
<wire x1="84.590890625" y1="64.270890625" x2="84.573196875" y2="64.253021875" width="0" layer="20" curve="0.567249"/>
<wire x1="84.573196875" y1="64.253021875" x2="78.95825625" y2="58.52578125" width="0" layer="20"/>
<wire x1="78.95825625" y1="58.52578125" x2="78.232" y2="56.7476" width="0" layer="20" curve="44.432751"/>
<wire x1="78.232" y1="56.7476" x2="78.232" y2="53.757103125" width="0" layer="20"/>
<wire x1="78.232" y1="53.757103125" x2="77.48805" y2="51.96105" width="0" layer="20" curve="-45.00005"/>
<wire x1="77.48805" y1="51.96105" x2="76.18195" y2="50.65495" width="0" layer="20"/>
<wire x1="76.18195" y1="50.65495" x2="74.385896875" y2="49.911" width="0" layer="20" curve="-45.00007"/>
<wire x1="74.385896875" y1="49.911" x2="15.276103125" y2="49.911" width="0" layer="20"/>
<wire x1="15.276103125" y1="49.911" x2="13.48005" y2="50.65495" width="0" layer="20" curve="-45.00005"/>
<wire x1="13.48005" y1="50.65495" x2="12.17395" y2="51.96105" width="0" layer="20"/>
<wire x1="12.17395" y1="51.96105" x2="11.43" y2="53.757103125" width="0" layer="20" curve="-45.00007"/>
<wire x1="11.43" y1="53.757103125" x2="11.43" y2="56.74630625" width="0" layer="20"/>
<wire x1="11.43" y1="56.74630625" x2="10.667046875" y2="58.5611625" width="0" layer="20" curve="45.603089"/>
<wire x1="10.667046875" y1="58.5611625" x2="4.677571875" y2="64.42585625" width="0" layer="20"/>
<wire x1="4.677571875" y1="64.42585625" x2="2.900525" y2="65.151" width="0" layer="20" curve="44.396911"/>
<wire x1="2.900525" y1="65.151" x2="0.036103125" y2="65.151" width="0" layer="20"/>
<wire x1="0.036103125" y1="65.151" x2="-1.75995" y2="65.89495" width="0" layer="20" curve="-45.00005"/>
<wire x1="-1.75995" y1="65.89495" x2="-3.32005" y2="67.45505" width="0" layer="20"/>
<wire x1="-3.32005" y1="67.45505" x2="-4.064" y2="69.251103125" width="0" layer="20" curve="-45.00007"/>
<wire x1="-4.064" y1="69.251103125" x2="-4.064" y2="128.741896875" width="0" layer="20"/>
<wire x1="-4.064" y1="128.741896875" x2="-3.32005" y2="130.53795" width="0" layer="20" curve="-45.00005"/>
<wire x1="-3.32005" y1="130.53795" x2="-2.26795" y2="131.59005" width="0" layer="20"/>
<wire x1="-2.26795" y1="131.59005" x2="-0.471896875" y2="132.334" width="0" layer="20" curve="-45.00007"/>
<wire x1="-0.471896875" y1="132.334" x2="2.656903125" y2="132.334" width="0" layer="20"/>
<wire x1="2.656903125" y1="132.334" x2="4.421175" y2="133.046721875" width="0" layer="20" curve="43.994968"/>
<wire x1="4.421175" y1="133.046721875" x2="10.27326875" y2="138.69701875" width="0" layer="20"/>
<wire x1="10.27326875" y1="138.69701875" x2="11.049" y2="140.5243" width="0" layer="20" curve="46.005153"/>
<wire x1="11.049" y1="140.5243" x2="11.049" y2="143.473896875" width="0" layer="20"/>
<wire x1="11.049" y1="143.473896875" x2="11.79295" y2="145.26995" width="0" layer="20" curve="-45.00005"/>
<wire x1="11.79295" y1="145.26995" x2="13.22605" y2="146.70305" width="0" layer="20"/>
<wire x1="13.22605" y1="146.70305" x2="15.022103125" y2="147.447" width="0" layer="20" curve="-45.00007"/>
<wire x1="15.022103125" y1="147.447" x2="74.258896875" y2="147.447" width="0" layer="20"/>
<wire x1="74.258896875" y1="147.447" x2="76.05495" y2="146.70305" width="0" layer="20" curve="-45.00005"/>
<wire x1="76.05495" y1="146.70305" x2="77.61505" y2="145.14295" width="0" layer="20"/>
<wire x1="77.61505" y1="145.14295" x2="78.359" y2="143.346896875" width="0" layer="20" curve="-45.00007"/>
<wire x1="78.359" y1="143.346896875" x2="78.359" y2="140.371103125" width="0" layer="20"/>
<wire x1="78.359" y1="140.371103125" x2="79.10295" y2="138.57505" width="0" layer="20" curve="45.00005"/>
<text>ACCEL_SCK</text>
<text>ACCEL_MOSI</text>
<text>ACCEL_MISO</text>
<text>ACCEL_CS</text>
<text>ACCEL_INT1</text>
<text>ACCEL_INT2</text>
<text>GND</text>
<text>RESET</text>
<text>GND</text>
<text>GPS_HS_SS</text>
<text>GPS_HS_CLK</text>
<text>GPS_HS_SIGN</text>
<text>GND</text>
<text>SDCS</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>DTO</text>
<text>DTI</text>
<text>FCS</text>
<text>FWP</text>
<text>HOLD</text>
<text>POWER</text>
<text>ON</text>
<text>OFF</text>
<text>PGOOD</text>
<text>STAT1</text>
<text>STAT2</text>
<text>CTX</text>
<text>CRX</text>
<text>GND</text>
<text>BUTTON EXTERNAL</text>
<text>BUTTON PCB</text>
<text>USER_LED0</text>
<text>BOOT JMP</text>
<text>GND</text>
<text>IN</text>
<text>IU SOIC</text>
<text>TC GPS R003</text>
<text>P442 Dig Sys</text>
</plain>
<libraries>
<library name="stmf3">
<packages>
<package name="TQFP100">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ADXL362">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MC-306">
<description>&lt;b&gt;MC-306 CRYSTAL UNIT&lt;/b&gt;&lt;p&gt;
Source: MC-306_405_406_E07X.PDF</description>
</package>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
<package name="BATTCON_12MM">
</package>
<package name="LIPO-1100">
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="DRC-10">
<description>&lt;h3&gt;10-pin QFN/SON package&lt;/h3&gt;
Package Type: SON&lt;br&gt;
Package Drawing: DRC&lt;Br&gt;
Pitch: 0.5mm&lt;br&gt;
Overall Dimensions: 3.15x3.15mm&lt;br&gt;
Pins: 10 (+1 exposed heatsink pin)&lt;br&gt;
&lt;br&gt;Related ICs:&lt;ul&gt;&lt;li&gt; TI's BQ2402x - http://focus.ti.com/lit/ds/symlink/bq24023.pdf&lt;br&gt;
&lt;/ul&gt;

Last modified: 8/16/10&lt;br&gt;
&lt;B&gt;Unproven!!!&lt;/B&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="MICRO-SD-SOCKET-PP">
</package>
</packages>
</library>
<library name="con-cortex">
<description>This library is for the ARM Cortex connectors as defined here:
http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf

For any information, please contact Shannon at strutz.shannon@gmail.com</description>
<packages>
<package name="2X10_0.05&quot;_SMD_NS">
<description>2x10, 0.05" pitch, surface-mount, unshrouded header from FCI, part number 20021121-00020C4LF</description>
</package>
<package name="2X10_0.1&quot;_TH_SH">
</package>
<package name="2X5_0.05&quot;_TH_NS">
<description>2x5 0.05" pitch, through-hole, unshrouded header from FCI, product number 20021111-00010T4LF
http://www.digikey.com/product-detail/en/20021111-00010T4LF/609-3712-ND/2209072</description>
</package>
</packages>
</library>
<library name="Kemet_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 28/03/2012 12:54:09</description>
<packages>
<package name="CAPC2013X110N">
</package>
<package name="CAPC2013X88N">
</package>
</packages>
</library>
<library name="ina">
<packages>
<package name="MSOP-8">
</package>
</packages>
</library>
<library name="Vishay_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 16:36:08</description>
<packages>
<package name="RESC1608X60N">
</package>
<package name="RESC1005X40N">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="trans">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gps">
<packages>
<package name="NAVSPARK_ARDUINO">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-THM">
<description>4UCon #01528
http://www.4uconnector.com/online/object/4udrawing/01528.pdf</description>
</package>
</packages>
</library>
<library name="memory">
<packages>
<package name="WSON-8">
</package>
</packages>
</library>
<library name="bluetooth">
<packages>
<package name="WS_CORE51822">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="usb">
<packages>
<package name="MINI-B-VERTICAL-WURTH">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.0 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-Sensors" package="ADXL362" value="ADXL362">
<attribute name="PROD_ID" value="IC-11297"/>
</element>
<element name="Q1" library="crystal" package="MC-306" value="MC-306">
<attribute name="OC_NEWARK" value="31M5576"/>
<attribute name="OC_FARNELL" value="1278040"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC-306 60.0KHZ  100PPM ,12.5PF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="6.8pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="6.8pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="SOT23-5" value="LDO-TPS78233">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT4" library="SparkFun-Electromechanical" package="BATTCON_12MM" value="3V">
<attribute name="PROD_ID" value="BATT-08044"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-Connectors" package="MICRO-SD-SOCKET-PP" value="USD-SOCKETNEW">
<attribute name="PROD_ID" value="CONN-07820"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0805" value="100pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="con-cortex" package="2X10_0.05&quot;_SMD_NS" value="2X10_0.05&quot;_CORTEX_DEBUG_WITH_ETMSMD_UNSHROUDED"/>
<element name="C9" library="Kemet_By_element14_Batch_1" package="CAPC2013X110N" value="1uF">
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C105K4RACTU"/>
<attribute name="OC_NEWARK" value="77C5351"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="9227792"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Kemet_By_element14_Batch_1" package="CAPC2013X110N" value="1uF">
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C105K4RACTU"/>
<attribute name="OC_NEWARK" value="77C5351"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="9227792"/>
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="stmf3" package="TQFP100" value="STM32F303VCT6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="ina" package="MSOP-8" value="INA225">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="Vishay_By_element14_Batch_1" package="RESC1608X60N" value="10 Ohms">
<attribute name="OC_FARNELL" value="1553930"/>
<attribute name="OC_NEWARK" value="71M1229"/>
<attribute name="TOLERANCE" value="± 0.1 %"/>
<attribute name="MPN" value="TNPW060310R0BEEN"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="WATTAGE" value="0.1 W"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="300">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="300">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Passives" package="0805" value="100pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Passives" package="0805" value="100pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP13" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="SOT23" value="BC847">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$10" library="gps" package="NAVSPARK_ARDUINO" value="NAVSPARK_ARDUINO">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="crystal" package="CSM-7X-DU" value="ECS-80-20-5PVX">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Passives" package="0603-CAP" value="20pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Passives" package="0603-CAP" value="20pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="SparkFun-PowerIC" package="DRC-10" value="BQ24022">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="SparkFun-Passives" package="0603-RES" value="1.13k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="SparkFun-Passives" package="0603-RES" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="SparkFun-Passives" package="0603-RES" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="SparkFun-Passives" package="0603-RES" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="SparkFun-Passives" package="0603-RES" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="Kemet_By_element14_Batch_1" package="CAPC2013X110N" value="1uF">
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="C0805C105K4RACTU"/>
<attribute name="OC_FARNELL" value="9227792"/>
<attribute name="OC_NEWARK" value="77C5351"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="Kemet_By_element14_Batch_1" package="CAPC2013X110N" value="1uF">
<attribute name="VOLTAGERATING" value="16V"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="MPN" value="C0805C105K4RACTU"/>
<attribute name="OC_FARNELL" value="9227792"/>
<attribute name="OC_NEWARK" value="77C5351"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="SparkFun-Passives" package="0603-RES" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP17" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="memory" package="WSON-8" value="GD5F1GQ4UCY1G">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$12" library="con-cortex" package="2X10_0.1&quot;_TH_SH" value="TRADITIONALJTAG/SWDTH_SHROUDED">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R41" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="OC_NEWARK" value="-"/>
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="OC_NEWARK" value="-"/>
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="OC_NEWARK" value="-"/>
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="Vishay_By_element14_Batch_1" package="RESC1005X40N" value="100K Ohms">
<attribute name="OC_NEWARK" value="-"/>
<attribute name="MPN" value="CRCW0402100KFKED"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="WATTAGE" value="0.063W"/>
<attribute name="OC_FARNELL" value="1469671"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP14" library="pinhead" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="bluetooth" package="WS_CORE51822" value="WS_CORE51822">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="SparkFun-LED" package="LED-0603" value="BLUE">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Passives" package="0603-RES" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$15" library="con-cortex" package="2X5_0.05&quot;_TH_NS" value="2X5_0.05&quot;_CORTEX_DEBUGTH_NOKEY_UNSHROUDED"/>
<element name="U$16" library="SparkFun-Electromechanical" package="LIPO-1100" value="LIPO-OUTLINE1100"/>
<element name="TP2" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="usb" package="MINI-B-VERTICAL-WURTH" value="USB-MINI-B-VERTICAL-WURTH"/>
<element name="D8" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S4" library="SparkFun-Electromechanical" package="AYZ0202" value="DPDT">
<attribute name="PROD_ID" value="SWCH-08179"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Passives" package="0603-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="SparkFun-DiscreteSemi" package="SOD-323" value="250mA/100V">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN2" library="adafruit" package="JST-PH-2-THM" value="">
<attribute name="NAME"/>
</element>
<element name="H1" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="H2" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="H3" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="H4" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="H5" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="H6" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="H7" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="H8" library="holes" package="3,0-PAD" value="MOUNT-PAD-ROUND3.0"/>
<element name="U$13" library="trans" package="SOT23" value="IRLML9301TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$17" library="trans" package="SOT23" value="IRLML9301TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$18" library="trans" package="SOT23" value="IRLML9301TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$19" library="trans" package="SOT23" value="IRLML9301TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="trans" package="SOT23" value="IRLML9301TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="Kemet_By_element14_Batch_1" package="CAPC2013X88N" value="10nF">
<attribute name="OC_NEWARK" value="01J3314"/>
<attribute name="MPN" value="C0805C103K5RACTU"/>
<attribute name="SUPPLIER" value="Kemet"/>
<attribute name="TOLERANCE" value="±10%"/>
<attribute name="OC_FARNELL" value="1414662"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="JP3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U$3" pad="100"/>
<contactref element="U$3" pad="75"/>
<contactref element="U$3" pad="28"/>
<contactref element="U$3" pad="50"/>
<contactref element="U$3" pad="22"/>
<contactref element="U$3" pad="21"/>
<contactref element="U$2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="U$12" pad="2"/>
<contactref element="U$12" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="R43" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="U$1" pad="P$8"/>
<contactref element="R8" pad="2"/>
<contactref element="U$13" pad="2"/>
<contactref element="U$17" pad="2"/>
<contactref element="U$18" pad="2"/>
<contactref element="U$19" pad="2"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RCC_OSC32_IN">
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="U$3" pad="8"/>
</signal>
<signal name="VPOWER">
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="U2" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="S4" pad="1"/>
</signal>
<signal name="NRST">
<contactref element="S3" pad="3"/>
<contactref element="C8" pad="1"/>
<contactref element="U$2" pad="10"/>
<contactref element="U$3" pad="14"/>
<contactref element="U$12" pad="15"/>
</signal>
<signal name="BUTTON_PCB">
<contactref element="S2" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="U$3" pad="92"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="U1" pad="P$13"/>
<contactref element="U1" pad="P$12"/>
<contactref element="U1" pad="P$16"/>
<contactref element="S3" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="C9" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U$3" pad="74"/>
<contactref element="U$3" pad="99"/>
<contactref element="U$3" pad="49"/>
<contactref element="U$3" pad="20"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="C7" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="BAT4" pad="GND"/>
<contactref element="JP12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U$2" pad="17"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$2" pad="15"/>
<contactref element="U$2" pad="19"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="9"/>
<contactref element="U$2" pad="11"/>
<contactref element="U$2" pad="13"/>
<contactref element="JP13" pad="7"/>
<contactref element="U3" pad="GND"/>
<contactref element="U3" pad="GND3"/>
<contactref element="U3" pad="GND1"/>
<contactref element="T1" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U$10" pad="P$13"/>
<contactref element="U$10" pad="P$21"/>
<contactref element="JP4" pad="4"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="U$3" pad="27"/>
<contactref element="U4" pad="EP"/>
<contactref element="U4" pad="5"/>
<contactref element="R30" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="U$12" pad="10"/>
<contactref element="U$12" pad="14"/>
<contactref element="U$12" pad="18"/>
<contactref element="U$12" pad="4"/>
<contactref element="U$12" pad="8"/>
<contactref element="U$12" pad="16"/>
<contactref element="U$12" pad="6"/>
<contactref element="U$12" pad="12"/>
<contactref element="U$12" pad="20"/>
<contactref element="U$12" pad="11"/>
<contactref element="U$11" pad="P$4"/>
<contactref element="U$11" pad="P$9"/>
<contactref element="JP14" pad="10"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$4" pad="P$12"/>
<contactref element="R20" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="U$15" pad="3"/>
<contactref element="U$15" pad="5"/>
<contactref element="JP17" pad="3"/>
<contactref element="U$1" pad="P$7"/>
<contactref element="U$6" pad="P$5"/>
<contactref element="U$6" pad="P$7"/>
<contactref element="U$6" pad="P$6"/>
<contactref element="S4" pad="6"/>
<contactref element="CN2" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="VBATT_BACKUP">
<contactref element="BAT4" pad="PWR@1"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="BOOT_MODE">
<contactref element="JP3" pad="2"/>
<contactref element="U$3" pad="94"/>
</signal>
<signal name="IMEAS_GAIN1_OUT">
<contactref element="U$1" pad="P$6"/>
<contactref element="U$3" pad="62"/>
</signal>
<signal name="IMEAS_GAIN0_OUT">
<contactref element="U$1" pad="P$5"/>
<contactref element="U$3" pad="61"/>
</signal>
<signal name="VCC">
<contactref element="U2" pad="5"/>
<contactref element="SJ1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="ACCEL_SCK">
<contactref element="U1" pad="P$4"/>
<contactref element="JP13" pad="1"/>
<contactref element="U$3" pad="30"/>
</signal>
<signal name="ACCEL_MOSI">
<contactref element="U1" pad="P$6"/>
<contactref element="JP13" pad="2"/>
<contactref element="U$3" pad="32"/>
</signal>
<signal name="ACCEL_MISO">
<contactref element="U1" pad="P$7"/>
<contactref element="JP13" pad="3"/>
<contactref element="U$3" pad="31"/>
</signal>
<signal name="ACCEL_INT1">
<contactref element="U1" pad="P$11"/>
<contactref element="JP13" pad="5"/>
<contactref element="U$3" pad="34"/>
</signal>
<signal name="ACCEL_INT2">
<contactref element="U1" pad="P$9"/>
<contactref element="JP13" pad="6"/>
<contactref element="U$3" pad="35"/>
</signal>
<signal name="ACCEL_CS">
<contactref element="U1" pad="P$8"/>
<contactref element="U$3" pad="33"/>
<contactref element="JP13" pad="4"/>
</signal>
<signal name="N$28">
<contactref element="R2" pad="2"/>
<contactref element="JP17" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R3" pad="2"/>
<contactref element="JP17" pad="2"/>
</signal>
<signal name="GPS_SECOND">
<contactref element="U$10" pad="P$3"/>
<contactref element="U$3" pad="36"/>
</signal>
<signal name="CONSOLE_TX">
<contactref element="R2" pad="1"/>
<contactref element="U$3" pad="68"/>
</signal>
<signal name="CONSOLE_RX">
<contactref element="R3" pad="1"/>
<contactref element="U$3" pad="69"/>
</signal>
<signal name="BTLE_SCK">
<contactref element="U$3" pad="78"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="BTLE_MISO">
<contactref element="U$3" pad="79"/>
<contactref element="U$4" pad="P$3"/>
</signal>
<signal name="BTLE_MOSI">
<contactref element="U$3" pad="80"/>
<contactref element="U$4" pad="P$4"/>
</signal>
<signal name="BTLE_CS">
<contactref element="U$3" pad="81"/>
<contactref element="U$4" pad="P$5"/>
</signal>
<signal name="BTLE_INT">
<contactref element="U$3" pad="82"/>
<contactref element="U$4" pad="P$6"/>
</signal>
<signal name="BTLE_DFU">
<contactref element="U$3" pad="83"/>
<contactref element="U$4" pad="P$21"/>
</signal>
<signal name="BUTTON_EXTERNAL">
<contactref element="JP12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U$3" pad="91"/>
</signal>
<signal name="DEBUG_TRACECLK">
<contactref element="U$3" pad="1"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="DEBUG_TRACE_D0">
<contactref element="U$3" pad="2"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="DEBUG_TRACE_D1">
<contactref element="U$3" pad="3"/>
<contactref element="U$2" pad="16"/>
</signal>
<signal name="DEBUG_TRACE_D2">
<contactref element="U$3" pad="4"/>
<contactref element="U$2" pad="18"/>
</signal>
<signal name="DEBUG_TRACE_D3">
<contactref element="U$3" pad="5"/>
<contactref element="U$2" pad="20"/>
</signal>
<signal name="DEBUG_SWDIO_JTMS">
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="72"/>
<contactref element="U$12" pad="7"/>
<contactref element="R41" pad="2"/>
</signal>
<signal name="DEBUG_SWCLK_JTCK">
<contactref element="U$2" pad="4"/>
<contactref element="U$3" pad="76"/>
<contactref element="U$12" pad="9"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="DEBUG_JTDI">
<contactref element="U$2" pad="8"/>
<contactref element="U$3" pad="77"/>
<contactref element="U$12" pad="5"/>
<contactref element="R40" pad="2"/>
</signal>
<signal name="DEBUG_JTDO_TRACESWO">
<contactref element="U$2" pad="6"/>
<contactref element="U$3" pad="89"/>
<contactref element="U$12" pad="13"/>
</signal>
<signal name="SDCARD_DETECT_IN">
<contactref element="U3" pad="CD2"/>
<contactref element="U$3" pad="56"/>
<contactref element="JP14" pad="6"/>
</signal>
<signal name="SDCARD_SCK">
<contactref element="U3" pad="SCLK"/>
<contactref element="U$3" pad="52"/>
<contactref element="U$11" pad="P$6"/>
<contactref element="JP14" pad="4"/>
</signal>
<signal name="SDCARD_MISO">
<contactref element="U3" pad="DO"/>
<contactref element="U$3" pad="53"/>
<contactref element="U$11" pad="P$2"/>
<contactref element="JP14" pad="3"/>
</signal>
<signal name="SDCARD_MOSI">
<contactref element="U$3" pad="54"/>
<contactref element="U$11" pad="P$5"/>
<contactref element="U3" pad="DI"/>
<contactref element="JP14" pad="2"/>
</signal>
<signal name="SDCARD_CS">
<contactref element="U3" pad="CS"/>
<contactref element="U$3" pad="51"/>
<contactref element="JP14" pad="1"/>
</signal>
<signal name="SDCARD_DETECT_OUT">
<contactref element="U3" pad="CD1"/>
<contactref element="U$3" pad="55"/>
<contactref element="JP14" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="T1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R6" pad="2"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="VIN_MEAS_A2D">
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="TP3" pad="TP"/>
<contactref element="U$3" pad="59"/>
</signal>
<signal name="SD_POWER">
<contactref element="U3" pad="VCC"/>
<contactref element="TP1" pad="TP"/>
<contactref element="U$13" pad="3"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="BTLE_POWER_EN">
<contactref element="U$3" pad="85"/>
<contactref element="U$17" pad="1"/>
</signal>
<signal name="BTLE_POWER">
<contactref element="U$4" pad="P$11"/>
<contactref element="U$17" pad="3"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$14"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="U$1" pad="P$3"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="GPS_POWER_EN">
<contactref element="U$3" pad="48"/>
<contactref element="U$18" pad="1"/>
</signal>
<signal name="GPS_POWER">
<contactref element="U$10" pad="P$24"/>
<contactref element="U$18" pad="3"/>
<contactref element="C18" pad="2"/>
</signal>
<signal name="GPS_HS_SIGN">
<contactref element="U$10" pad="P$18"/>
<contactref element="JP4" pad="1"/>
<contactref element="U$3" pad="44"/>
</signal>
<signal name="GPS_HS_CLK">
<contactref element="U$10" pad="P$17"/>
<contactref element="JP4" pad="2"/>
<contactref element="U$3" pad="43"/>
</signal>
<signal name="GPS_HS_SS">
<contactref element="U$10" pad="P$11"/>
<contactref element="JP4" pad="3"/>
<contactref element="U$3" pad="42"/>
</signal>
<signal name="GPS_TRIG_TIMESTAMP">
<contactref element="U$10" pad="P$15"/>
<contactref element="U$3" pad="45"/>
</signal>
<signal name="RCC_OSC_IN">
<contactref element="U$3" pad="12"/>
<contactref element="C12" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="IMEAS_IN+">
<contactref element="U$1" pad="P$4"/>
<contactref element="TP6" pad="TP"/>
<contactref element="U$3" pad="60"/>
</signal>
<signal name="GPS_NMEA_TX">
<contactref element="U$3" pad="26"/>
<contactref element="U$10" pad="P$12"/>
</signal>
<signal name="CHARGER_PGOOD">
<contactref element="R29" pad="2"/>
<contactref element="U$3" pad="63"/>
</signal>
<signal name="CHARGER_CE">
<contactref element="R31" pad="2"/>
<contactref element="U$3" pad="64"/>
</signal>
<signal name="GPS_PROG_TX">
<contactref element="U$3" pad="46"/>
<contactref element="U$10" pad="P$2"/>
</signal>
<signal name="GPS_PROG_RX">
<contactref element="U$3" pad="47"/>
<contactref element="U$10" pad="P$1"/>
</signal>
<signal name="SDCARD_POWER_EN">
<contactref element="U$3" pad="57"/>
<contactref element="U$13" pad="1"/>
</signal>
<signal name="USB_DM">
<contactref element="U$3" pad="70"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="USB_DP">
<contactref element="U$3" pad="71"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="RCC_OSC32_OUT">
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="4"/>
<contactref element="U$3" pad="9"/>
</signal>
<signal name="VIN_MEAS_EN">
<contactref element="R5" pad="2"/>
<contactref element="U$3" pad="41"/>
</signal>
<signal name="RCC_OSC_OUT">
<contactref element="C13" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="U$3" pad="13"/>
</signal>
<signal name="VUSB">
<contactref element="U4" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="VLIPO">
<contactref element="U4" pad="10"/>
<contactref element="C15" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="CN2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R18" pad="1"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$39">
<contactref element="R19" pad="1"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="D4" pad="C"/>
<contactref element="U4" pad="4"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="D5" pad="C"/>
<contactref element="U4" pad="3"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="CHARGER_STAT1">
<contactref element="R26" pad="2"/>
<contactref element="U$3" pad="67"/>
</signal>
<signal name="CHARGER_STAT2">
<contactref element="R27" pad="2"/>
<contactref element="U$3" pad="66"/>
</signal>
<signal name="N$42">
<contactref element="R28" pad="1"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$43">
<contactref element="D6" pad="C"/>
<contactref element="U4" pad="8"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="U4" pad="6"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="R32" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="U4" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="R33" pad="1"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="N$48">
<contactref element="R34" pad="1"/>
<contactref element="R35" pad="1"/>
<contactref element="U$6" pad="P$3"/>
</signal>
<signal name="N$49">
<contactref element="U4" pad="7"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="CHARGER_ISET2">
<contactref element="R36" pad="2"/>
<contactref element="U$3" pad="65"/>
</signal>
<signal name="N$51">
<contactref element="R37" pad="1"/>
<contactref element="U$6" pad="P$4"/>
</signal>
<signal name="DEBUG_TRST">
<contactref element="U$3" pad="90"/>
<contactref element="U$12" pad="3"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="LED_OUT0">
<contactref element="U$3" pad="93"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="DEBUG_GNDDETECT">
<contactref element="U$3" pad="88"/>
</signal>
<signal name="FLASH_POWER_EN">
<contactref element="U$3" pad="37"/>
<contactref element="U$19" pad="1"/>
</signal>
<signal name="FLASH_POWER">
<contactref element="U$11" pad="P$8"/>
<contactref element="TP2" pad="TP"/>
<contactref element="U$19" pad="3"/>
<contactref element="C19" pad="2"/>
</signal>
<signal name="FLASH_CS">
<contactref element="U$11" pad="P$1"/>
<contactref element="JP14" pad="7"/>
<contactref element="U$3" pad="40"/>
</signal>
<signal name="FLASH_WP">
<contactref element="U$11" pad="P$3"/>
<contactref element="JP14" pad="8"/>
<contactref element="U$3" pad="38"/>
</signal>
<signal name="FLASH_HOLD">
<contactref element="U$11" pad="P$7"/>
<contactref element="JP14" pad="9"/>
<contactref element="U$3" pad="39"/>
</signal>
<signal name="BTLE_MODE">
<contactref element="U$4" pad="P$15"/>
<contactref element="U$3" pad="97"/>
</signal>
<signal name="SWDIO">
<contactref element="U$4" pad="P$31"/>
<contactref element="U$15" pad="2"/>
</signal>
<signal name="BTLE_RXD">
<contactref element="U$4" pad="P$25"/>
<contactref element="U$3" pad="96"/>
</signal>
<signal name="BTLE_TX">
<contactref element="U$4" pad="P$23"/>
<contactref element="U$3" pad="95"/>
</signal>
<signal name="BTLE_RTS">
<contactref element="U$4" pad="P$22"/>
<contactref element="U$3" pad="58"/>
</signal>
<signal name="BTLE_CTS">
<contactref element="U$4" pad="P$24"/>
<contactref element="U$3" pad="73"/>
</signal>
<signal name="BTLE_FACTORY_RESET">
<contactref element="U$4" pad="P$30"/>
<contactref element="U$3" pad="84"/>
</signal>
<signal name="SWDCLK">
<contactref element="U$4" pad="P$32"/>
<contactref element="U$15" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="D9" pad="C"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="D10" pad="C"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="CONNECTED_LED">
<contactref element="D9" pad="A"/>
<contactref element="U$4" pad="P$34"/>
</signal>
<signal name="MODE_LED">
<contactref element="D10" pad="A"/>
<contactref element="U$4" pad="P$33"/>
</signal>
<signal name="REG_EN">
<contactref element="U2" pad="3"/>
<contactref element="D8" pad="C"/>
<contactref element="R9" pad="2"/>
<contactref element="S4" pad="2"/>
</signal>
<signal name="SYSTEM_POWER_LATCH">
<contactref element="D8" pad="A"/>
<contactref element="U$3" pad="86"/>
</signal>
<signal name="N$11">
<contactref element="S4" pad="5"/>
<contactref element="R9" pad="1"/>
<contactref element="D11" pad="C"/>
</signal>
<signal name="SYSTEM_POWER_SWITCH_STATE">
<contactref element="D11" pad="A"/>
<contactref element="U$3" pad="87"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
