(kicad_pcb (version 20171130) (host pcbnew "(5.0.2-5)-5")
  (general
    (thickness 1.6)
    (drawings 84)
    (tracks 240)
    (zones 0)
    (modules 29)
    (nets 24)
  )
  (page A4)
  (title_block
    (title "Train Distance Car Interconnect")
    (date 2019-03-17)
    (rev v1.2)
    (company "Timberlake Hobbies")
    (comment 1 "Version 1.2 corrects incorrect package sizes..")
    (comment 2 https://creativecommons.org/licenses/by/4.0/)
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: Eric Timberlake")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.381)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 2.7)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 "Net-(BZ1-Pad2)")
  (net 3 VBAT.5)
  (net 4 GND)
  (net 5 "Net-(F1-Pad1)")
  (net 6 +5V)
  (net 7 ENC-B)
  (net 8 ENC-A)
  (net 9 ~BUTTON1)
  (net 10 TIRQ)
  (net 11 MISO)
  (net 12 MOSI)
  (net 13 SCK)
  (net 14 "Net-(J3-Pad7)")
  (net 15 DnC)
  (net 16 ~BUTTON2)
  (net 17 ~LOBAT)
  (net 18 ~PWR_OFF)
  (net 19 VBAT)
  (net 20 ~FRCS)
  (net 21 ~TCS)
  (net 22 ~CS)
  (net 23 "Net-(R7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net +3V3)
    (add_net +5V)
    (add_net DnC)
    (add_net ENC-A)
    (add_net ENC-B)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(BZ1-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(R7-Pad2)")
    (add_net SCK)
    (add_net TIRQ)
    (add_net VBAT)
    (add_net VBAT.5)
    (add_net ~BUTTON1)
    (add_net ~BUTTON2)
    (add_net ~CS)
    (add_net ~FRCS)
    (add_net ~LOBAT)
    (add_net ~PWR_OFF)
    (add_net ~TCS)
  )
  (module teensy:Teensy30_31_32_LC_audio_only (layer F.Cu) (tedit 5C72631E)
    (at 92.71 88.9 270)
    (fp_text reference U1 (at -19.05 5.08) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 10.16 270) (layer F.Fab))
    (pad 19 thru_hole circle (at 16.51 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 SCK))
    (pad 14 thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 MISO))
    (pad 21 thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 VBAT.5))
    (pad 22 thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 ~BUTTON2))
    (pad 24 thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 ~BUTTON1))
    (pad 25 thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 ~LOBAT))
    (pad 26 thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 ENC-A))
    (pad 28 thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 ENC-B))
    (pad 29 thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 ~FRCS))
    (pad 30 thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(BZ1-Pad2)"))
    (pad 31 thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 32 thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 33 thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 +5V))
    (pad 13 thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 MOSI))
    (pad 12 thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 ~CS))
    (pad 11 thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 DnC))
    (pad 10 thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 ~TCS))
    (pad 9 thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 TIRQ))
    (pad 3 thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole rect (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.7338 77.6986)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.1016 1.9304 180) (layer F.SilkS))
    (fp_text value .1uf (at -0.127 -2.0828) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 VBAT.5))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5C8F0ED0)
    (at 109.22 95.25)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 12.7) (layer F.SilkS))
    (fp_text value "Encoder Header" (at 2.54 5.08 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 ENC-B))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 ENC-A))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C8F0EDA)
    (at 118.11 102.87)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 5.08) (layer F.SilkS))
    (fp_text value "Button Header" (at -2.54 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 ~BUTTON1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x14_P2.54mm_Vertical (layer F.Cu) (tedit 5C8F0EC9)
    (at 67.31 72.39)
    (descr "Through hole straight socket strip, 1x14, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x14 2.54mm single row")
    (fp_text reference J1 (at 0 35.814) (layer F.SilkS))
    (fp_text value "IFI9431 Header" (at 3.81 8.89 90) (layer F.Fab))
    (fp_text user %R (at 0 16.51 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 TIRQ))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 MISO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 MOSI))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 ~TCS))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 SCK))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 MISO))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 SCK))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 MOSI))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 DnC))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 ~CS))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C8F0957)
    (at 123.19 102.87)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 5.08) (layer F.SilkS))
    (fp_text value "Button Header" (at 2.54 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 ~BUTTON2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 140.97 80.01)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J5 (at 0 -2.77) (layer F.SilkS))
    (fp_text value "Adafruit 500C Header" (at 2.54 8.89 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 ~LOBAT))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 ~PWR_OFF))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VBAT))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.74 72.39 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -2.286 180) (layer F.SilkS))
    (fp_text value 100 (at 0 6.35 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 +5V))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(J3-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.11 97.79 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 2.54) (layer F.SilkS))
    (fp_text value 10k (at -3.81 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 ~BUTTON1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 76.2 86.36)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -2.54) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 ~TCS))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 76.2 91.44)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 ~CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.4722 78.5368 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0.0508 1.7018 90) (layer F.SilkS))
    (fp_text value 10k (at -3.81 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 ~FRCS))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.2408 97.8124 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -0.0224 -2.2352) (layer F.SilkS))
    (fp_text value 10k (at -3.7562 0.1524 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 ~BUTTON2))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.1552 78.3844 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0.0508 -1.8542 90) (layer F.SilkS))
    (fp_text value 10k (at -3.683 -0.0508 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5C725353)
    (at 132.334 99.06 270)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 7.62 3.302) (layer F.SilkS))
    (fp_text value EG1218 (at 2.11 3.14 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 ~PWR_OFF))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module Buzzer_Beeper:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 5C8F0884)
    (at 107.95 74.93)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference Buzzer1 (at 3.8 -7.2) (layer F.SilkS))
    (fp_text value Buzzer (at 3.81 6.604) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 7.6 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(BZ1-Pad2)"))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5C72694E)
    (at 64.008 67.31)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5C726963)
    (at 64.008 110.49)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5C726982)
    (at 142.24 105.41)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5C726928)
    (at 158.75 105.41)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5C726972)
    (at 166.0652 67.3608)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H5 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5C726913)
    (at 166.0652 110.5154)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H6 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value hole (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.686 82.042 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 VBAT))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 VBAT.5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.6576 86.0044)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 1.905) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 VBAT.5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SSOP-8_3.9x5.05mm_P1.27mm (layer F.Cu) (tedit 5B9564B2)
    (at 118.872 85.852)
    (descr "SSOP, 8 Pin (http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (attr smd)
    (fp_text reference U2 (at 0 -3.48) (layer F.SilkS))
    (fp_text value MB85RS16 (at 0 3.48) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.675 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 ~FRCS))
    (pad 2 smd roundrect (at -2.675 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 MISO))
    (pad 3 smd roundrect (at -2.675 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R7-Pad2)"))
    (pad 4 smd roundrect (at -2.675 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 5 smd roundrect (at 2.675 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 MOSI))
    (pad 6 smd roundrect (at 2.675 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 SCK))
    (pad 7 smd roundrect (at 2.675 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R7-Pad2)"))
    (pad 8 smd roundrect (at 2.675 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-8_3.9x5.05mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 76.2 104.14)
    (descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F1 (at 0 -2.65) (layer F.SilkS))
    (fp_text value "450mA Polyfuse" (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.225 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 5 "Net-(F1-Pad1)"))
    (pad 2 smd roundrect (at 2.225 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:RCGRS_sm (layer B.Cu) (tedit 0)
    (at 109.474 98.298)
    (fp_text reference RCGRS_sm (at 0 -5) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0) (layer B.SilkS))
  )
  (module Symbol:OSHW-Logo_11.4x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 155.702 87.884)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_11.4x12mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbol:OSHW-Logo_11.4x12mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 158.496 71.882)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_11.4x12mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text ~BEEP (at 114.808 77.724) (layer F.SilkS))
  (gr_text SN: (at 73.914 110.998) (layer F.SilkS))
  (gr_text 10k (at 124.206 74.422 90) (layer F.SilkS))
  (gr_text 10k (at 120.396 74.422 90) (layer F.SilkS))
  (gr_text VBAT.5 (at 96.266 102.87) (layer F.SilkS))
  (gr_text USB (at 137.668 97.79) (layer F.SilkS))
  (gr_text GND (at 137.668 95.25) (layer F.SilkS))
  (gr_text VBAT (at 137.414 92.71) (layer F.SilkS))
  (gr_text ~PWR_OFF (at 135.89 90.17) (layer F.SilkS))
  (gr_text GND (at 137.668 87.63) (layer F.SilkS))
  (gr_text ~LOBAT (at 136.906 85.09) (layer F.SilkS))
  (gr_text GND (at 137.668 82.55) (layer F.SilkS))
  (gr_text VCC (at 137.668 80.01) (layer F.SilkS))
  (gr_text ~BEEP (at 96.774 80.01) (layer F.SilkS))
  (gr_text ~FRCS (at 96.774 82.55) (layer F.SilkS))
  (gr_text GND (at 106.426 105.41) (layer F.SilkS))
  (gr_text VCC (at 106.172 97.79) (layer F.SilkS))
  (gr_text ENCA (at 105.664 100.33) (layer F.SilkS))
  (gr_text ENCB (at 105.41 95.25) (layer F.SilkS))
  (gr_text ENCB (at 96.774 85.09) (layer F.SilkS))
  (gr_text ENCA (at 96.774 87.63) (layer F.SilkS))
  (gr_text ~BUT2 (at 96.52 97.79) (layer F.SilkS))
  (gr_text ~BUT1 (at 96.774 95.25) (layer F.SilkS))
  (gr_text DAC (at 94.996 105.41) (layer F.SilkS))
  (gr_text SCK (at 103.124 105.41) (layer F.SilkS))
  (gr_text ~TCS (at 87.884 95.25) (layer F.SilkS))
  (gr_text D/C (at 88.138 97.79) (layer F.SilkS))
  (gr_text ~CS (at 87.63 100.584) (layer F.SilkS))
  (gr_text MOSI (at 88.138 102.87) (layer F.SilkS))
  (gr_text MISO (at 88.138 105.41) (layer F.SilkS))
  (gr_text TIRQ (at 87.884 80.01) (layer F.SilkS))
  (gr_text TIRQ (at 63.5 72.39) (layer F.SilkS))
  (gr_text MISO (at 63.5 74.93) (layer F.SilkS))
  (gr_text MOSI (at 63.5 77.47) (layer F.SilkS))
  (gr_text ~TCS (at 63.246 80.01) (layer F.SilkS))
  (gr_text SCK (at 63.5 82.55) (layer F.SilkS))
  (gr_text MISO (at 63.754 85.09) (layer F.SilkS))
  (gr_text LED (at 63.246 87.63) (layer F.SilkS))
  (gr_text SCK (at 63.246 90.17) (layer F.SilkS))
  (gr_text MOSI (at 63.754 92.71) (layer F.SilkS))
  (gr_text D/C (at 63.5 95.25) (layer F.SilkS))
  (gr_text ~RST (at 63.5 97.79) (layer F.SilkS))
  (gr_text ~CS (at 63.246 100.33) (layer F.SilkS))
  (gr_text GND (at 63.754 102.87) (layer F.SilkS))
  (gr_text VCC (at 63.754 105.41) (layer F.SilkS))
  (gr_text "450ma Polyfuse" (at 76.454 100.33) (layer F.SilkS))
  (gr_text 100 (at 78.74 68.834 90) (layer F.SilkS))
  (gr_text 10k (at 80.01 91.44 90) (layer F.SilkS))
  (gr_text 10k (at 80.01 86.36 90) (layer F.SilkS))
  (gr_text 10k (at 118.11 93.98 90) (layer F.SilkS))
  (gr_text 10k (at 123.19 93.98 90) (layer F.SilkS))
  (gr_text .1uf (at 127.4318 77.7748 90) (layer F.SilkS))
  (gr_text 100k (at 127.762 81.788 90) (layer F.SilkS))
  (gr_text 100k (at 127.762 86.106 90) (layer F.SilkS))
  (gr_text "Teensy 3.2" (at 91.948 87.63 90) (layer F.SilkS))
  (gr_text "IFI9341 Header" (at 70.358 89.408 90) (layer F.SilkS))
  (gr_text Encoder (at 111.76 100.838 90) (layer F.SilkS))
  (gr_text ~B2 (at 126.492 104.14 90) (layer F.SilkS))
  (gr_text ~B1 (at 115.316 104.14 90) (layer F.SilkS))
  (gr_text "Adafruit\nPower\nBoost\n500C" (at 150.114 97.536) (layer F.SilkS))
  (gr_text "Track Distance Car Interconnect\nVersion: 1.2\n2019" (at 135.4582 69.088) (layer F.SilkS))
  (gr_text OFF (at 132.334 109.22) (layer F.SilkS))
  (gr_text ON (at 132.08 93.98) (layer F.SilkS))
  (gr_text "Track Distance Car Interconnect\nVersion:  1.2\nEric Timberlake - 2019" (at 144.526 70.358 180) (layer B.SilkS))
  (dimension 112.522 (width 0.3) (layer Cmts.User)
    (gr_text "4.4300 in" (at 113.411 124.528) (layer Cmts.User))
    (feature1 (pts (xy 169.672 114.808) (xy 169.672 123.014421)))
    (feature2 (pts (xy 57.15 114.808) (xy 57.15 123.014421)))
    (crossbar (pts (xy 57.15 122.428) (xy 169.672 122.428)))
    (arrow1a (pts (xy 169.672 122.428) (xy 168.545496 123.014421)))
    (arrow1b (pts (xy 169.672 122.428) (xy 168.545496 121.841579)))
    (arrow2a (pts (xy 57.15 122.428) (xy 58.276504 123.014421)))
    (arrow2b (pts (xy 57.15 122.428) (xy 58.276504 121.841579)))
  )
  (dimension 49.87007 (width 0.3) (layer Cmts.User)
    (gr_text "49.870 mm" (at 186.60034 88.879698 270.2216512) (layer Cmts.User))
    (feature1 (pts (xy 170.372924 113.877697) (xy 185.183234 113.820402)))
    (feature2 (pts (xy 170.18 64.008) (xy 184.99031 63.950705)))
    (crossbar (pts (xy 184.403894 63.952974) (xy 184.596818 113.822671)))
    (arrow1a (pts (xy 184.596818 113.822671) (xy 184.006044 112.698444)))
    (arrow1b (pts (xy 184.596818 113.822671) (xy 185.178876 112.693907)))
    (arrow2a (pts (xy 184.403894 63.952974) (xy 183.821836 65.081738)))
    (arrow2b (pts (xy 184.403894 63.952974) (xy 184.994668 65.077201)))
  )
  (dimension 43.18 (width 0.3) (layer Cmts.User)
    (gr_text "1.7000 in" (at 177.321538 88.9 270) (layer Cmts.User))
    (feature1 (pts (xy 166.077538 110.49) (xy 175.807959 110.49)))
    (feature2 (pts (xy 166.077538 67.31) (xy 175.807959 67.31)))
    (crossbar (pts (xy 175.221538 67.31) (xy 175.221538 110.49)))
    (arrow1a (pts (xy 175.221538 110.49) (xy 174.635117 109.363496)))
    (arrow1b (pts (xy 175.221538 110.49) (xy 175.807959 109.363496)))
    (arrow2a (pts (xy 175.221538 67.31) (xy 174.635117 68.436504)))
    (arrow2b (pts (xy 175.221538 67.31) (xy 175.807959 68.436504)))
  )
  (dimension 109.728 (width 0.3) (layer Cmts.User)
    (gr_text "4.3200 in" (at 111.267033 52.376664) (layer Cmts.User))
    (feature1 (pts (xy 56.403033 67.176664) (xy 56.403033 53.890243)))
    (feature2 (pts (xy 166.131033 67.176664) (xy 166.131033 53.890243)))
    (crossbar (pts (xy 166.131033 54.476664) (xy 56.403033 54.476664)))
    (arrow1a (pts (xy 56.403033 54.476664) (xy 57.529537 53.890243)))
    (arrow1b (pts (xy 56.403033 54.476664) (xy 57.529537 55.063085)))
    (arrow2a (pts (xy 166.131033 54.476664) (xy 165.004529 53.890243)))
    (arrow2b (pts (xy 166.131033 54.476664) (xy 165.004529 55.063085)))
  )
  (dimension 16.51 (width 0.3) (layer Cmts.User)
    (gr_text "0.6500 in" (at 150.495 109.542) (layer Cmts.User))
    (feature1 (pts (xy 158.75 105.41) (xy 158.75 108.028421)))
    (feature2 (pts (xy 142.24 105.41) (xy 142.24 108.028421)))
    (crossbar (pts (xy 142.24 107.442) (xy 158.75 107.442)))
    (arrow1a (pts (xy 158.75 107.442) (xy 157.623496 108.028421)))
    (arrow1b (pts (xy 158.75 107.442) (xy 157.623496 106.855579)))
    (arrow2a (pts (xy 142.24 107.442) (xy 143.366504 108.028421)))
    (arrow2b (pts (xy 142.24 107.442) (xy 143.366504 106.855579)))
  )
  (dimension 1.27 (width 0.3) (layer Cmts.User)
    (gr_text "0.0500 in" (at 141.605 111.32) (layer Cmts.User))
    (feature1 (pts (xy 142.24 88.9) (xy 142.24 109.806421)))
    (feature2 (pts (xy 140.97 88.9) (xy 140.97 109.806421)))
    (crossbar (pts (xy 140.97 109.22) (xy 142.24 109.22)))
    (arrow1a (pts (xy 142.24 109.22) (xy 141.113496 109.806421)))
    (arrow1b (pts (xy 142.24 109.22) (xy 141.113496 108.633579)))
    (arrow2a (pts (xy 140.97 109.22) (xy 142.096504 109.806421)))
    (arrow2b (pts (xy 140.97 109.22) (xy 142.096504 108.633579)))
  )
  (dimension 16.51 (width 0.3) (layer Cmts.User)
    (gr_text "0.6500 in" (at 151.706 97.155 270) (layer Cmts.User))
    (feature1 (pts (xy 140.97 105.41) (xy 150.192421 105.41)))
    (feature2 (pts (xy 140.97 88.9) (xy 150.192421 88.9)))
    (crossbar (pts (xy 149.606 88.9) (xy 149.606 105.41)))
    (arrow1a (pts (xy 149.606 105.41) (xy 149.019579 104.283496)))
    (arrow1b (pts (xy 149.606 105.41) (xy 150.192421 104.283496)))
    (arrow2a (pts (xy 149.606 88.9) (xy 149.019579 90.026504)))
    (arrow2b (pts (xy 149.606 88.9) (xy 150.192421 90.026504)))
  )
  (dimension 5.08 (width 0.3) (layer Cmts.User)
    (gr_text "0.2000 in" (at 53.78 69.85 90) (layer Cmts.User))
    (feature1 (pts (xy 67.31 67.31) (xy 55.293579 67.31)))
    (feature2 (pts (xy 67.31 72.39) (xy 55.293579 72.39)))
    (crossbar (pts (xy 55.88 72.39) (xy 55.88 67.31)))
    (arrow1a (pts (xy 55.88 67.31) (xy 56.466421 68.436504)))
    (arrow1b (pts (xy 55.88 67.31) (xy 55.293579 68.436504)))
    (arrow2a (pts (xy 55.88 72.39) (xy 56.466421 71.263496)))
    (arrow2b (pts (xy 55.88 72.39) (xy 55.293579 71.263496)))
  )
  (dimension 3.302 (width 0.3) (layer Cmts.User)
    (gr_text "0.1300 in" (at 65.659 60.13) (layer Cmts.User))
    (feature1 (pts (xy 64.008 72.39) (xy 64.008 61.643579)))
    (feature2 (pts (xy 67.31 72.39) (xy 67.31 61.643579)))
    (crossbar (pts (xy 67.31 62.23) (xy 64.008 62.23)))
    (arrow1a (pts (xy 64.008 62.23) (xy 65.134504 61.643579)))
    (arrow1b (pts (xy 64.008 62.23) (xy 65.134504 62.816421)))
    (arrow2a (pts (xy 67.31 62.23) (xy 66.183496 61.643579)))
    (arrow2b (pts (xy 67.31 62.23) (xy 66.183496 62.816421)))
  )
  (dimension 5.08 (width 0.3) (layer Cmts.User)
    (gr_text "0.2000 in" (at 53.018 107.95 270) (layer Cmts.User))
    (feature1 (pts (xy 67.31 110.49) (xy 54.531579 110.49)))
    (feature2 (pts (xy 67.31 105.41) (xy 54.531579 105.41)))
    (crossbar (pts (xy 55.118 105.41) (xy 55.118 110.49)))
    (arrow1a (pts (xy 55.118 110.49) (xy 54.531579 109.363496)))
    (arrow1b (pts (xy 55.118 110.49) (xy 55.704421 109.363496)))
    (arrow2a (pts (xy 55.118 105.41) (xy 54.531579 106.536504)))
    (arrow2b (pts (xy 55.118 105.41) (xy 55.704421 106.536504)))
  )
  (dimension 3.302 (width 0.3) (layer Cmts.User)
    (gr_text "0.1300 in" (at 65.659 118.686) (layer Cmts.User))
    (feature1 (pts (xy 64.008 105.41) (xy 64.008 117.172421)))
    (feature2 (pts (xy 67.31 105.41) (xy 67.31 117.172421)))
    (crossbar (pts (xy 67.31 116.586) (xy 64.008 116.586)))
    (arrow1a (pts (xy 64.008 116.586) (xy 65.134504 115.999579)))
    (arrow1b (pts (xy 64.008 116.586) (xy 65.134504 117.172421)))
    (arrow2a (pts (xy 67.31 116.586) (xy 66.183496 115.999579)))
    (arrow2b (pts (xy 67.31 116.586) (xy 66.183496 117.172421)))
  )
  (gr_line (start 170.18 114.3) (end 57.15 114.3) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 170.18 63.5) (end 170.18 114.3) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 57.15 63.5) (end 170.18 63.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 57.15 114.3) (end 57.15 63.5) (layer Edge.Cuts) (width 0.0254))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.832 116.84) (xy 172.974 116.84) (xy 172.974 60.706) (xy 52.578 60.706) (xy 52.578 60.96)
        (xy 53.34 116.332)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.292 57.404) (xy 173.99 57.15) (xy 174.498 119.126) (xy 50.292 119.38)
      )
    )
  )
)
