(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "MestaRider1")
		(date "2025-06-02")
		(rev "0.1")
		(company "JHU/APL")
		(comment 1 "Gavin Granath")
		(comment 2 "Export Controlled under the EAR (15 CFR 730-744) ECCN EAR99")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask yes)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "fabOutputs/")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(A1-SDA-Pad12)")
	(net 2 "Net-(A1-VDD)")
	(net 3 "unconnected-(A1-IO1-Pad6)")
	(net 4 "Net-(A1-VBAT)")
	(net 5 "unconnected-(A1-IO2-Pad7)")
	(net 6 "unconnected-(A1-SCL-Pad11)")
	(net 7 "unconnected-(A1-AIN1-Pad5)")
	(net 8 "SOFTUARTRX")
	(net 9 "unconnected-(A1-BOOT-Pad1)")
	(net 10 "Net-(J3-Pin_2)")
	(net 11 "Net-(D1-K)")
	(net 12 "unconnected-(J1-Pad5)")
	(net 13 "unconnected-(J1-Pad9)")
	(net 14 "DIAGUARTRX")
	(net 15 "DIAGUARTTX")
	(net 16 "SOFTUARTTX")
	(net 17 "MCRXPin")
	(net 18 "unconnected-(J1-Pad4)")
	(net 19 "3V3 Ext")
	(net 20 "MCTXPin")
	(net 21 "3V3_EXT_PICO")
	(net 22 "3V3_EXT_RAK")
	(net 23 "POW_IN")
	(net 24 "GND")
	(net 25 "POW_IN_PICO")
	(net 26 "POW_IN_RAK")
	(net 27 "Net-(Q1-B)")
	(net 28 "P1")
	(net 29 "GPIO9")
	(net 30 "GPIO16")
	(net 31 "GPIO7")
	(net 32 "GPIO13")
	(net 33 "GPIO14")
	(net 34 "GPIO15")
	(net 35 "GPIO10")
	(net 36 "GPIO11")
	(net 37 "GPIO17")
	(net 38 "GPIO8")
	(net 39 "GPIO12")
	(net 40 "GPIO18")
	(net 41 "unconnected-(U2-GP28-Pad34)")
	(net 42 "unconnected-(U2-GP5-Pad7)")
	(net 43 "unconnected-(U2-GP6-Pad9)")
	(net 44 "unconnected-(U2-GND-Pad42)")
	(net 45 "unconnected-(U2-GP3-Pad5)")
	(net 46 "unconnected-(U2-GP26-Pad31)")
	(net 47 "unconnected-(U2-ADC_VREF-Pad35)")
	(net 48 "unconnected-(U2-GP4-Pad6)")
	(net 49 "unconnected-(U2-3V3(OUT)-Pad36)")
	(net 50 "unconnected-(U2-3V3_EN-Pad37)")
	(net 51 "unconnected-(U2-RUN-Pad30)")
	(net 52 "unconnected-(U2-SWDIO-Pad43)")
	(net 53 "unconnected-(U2-GP2-Pad4)")
	(net 54 "unconnected-(U2-GP27-Pad32)")
	(net 55 "unconnected-(U2-VBUS-Pad40)")
	(net 56 "unconnected-(U2-SWCLK-Pad41)")
	(net 57 "unconnected-(U3-NC-Pad4)")
	(net 58 "unconnected-(U4-NC-Pad4)")
	(net 59 "Net-(Q1-C)")
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 168.96 118)
		(descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R2"
			(at 1.27 -1.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.3k"
			(at 1.27 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -1.92 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "MCRXPin")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(Q1-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92L_Inline_Wide"
		(layer "F.Cu")
		(at 175.95 117.45)
		(descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
		(tags "TO-92L Inline Wide transistor")
		(property "Reference" "Q1"
			(at 2.54 -3.56 0)
			(layer "F.SilkS")
		)
		(property "Value" "NPN PN2222A"
			(at 2.54 2.79 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_Inline_Wide"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "open_collector")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "E")
			(pintype "open_emitter")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 163 118.54 180)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "J4"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Counter_Clockwise"
			(at 1.27 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "3V3 Ext")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "3V3 Ext")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "3V3_EXT_RAK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "3V3_EXT_PICO")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SparkFun-Jumper:Jumper_2_NO"
		(layer "F.Cu")
		(at 171.55 107.35)
		(tags "SparkFun")
		(property "Reference" "JP2"
			(at 0 -1.143 0)
			(layer "F.Fab")
		)
		(property "Value" "SHORT TO BYPASS"
			(at 0 1.143 0)
			(layer "F.Fab")
		)
		(property "Footprint" "SparkFun-Jumper:Jumper_2_NO"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 22 "3V3_EXT_RAK")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 26 "POW_IN_RAK")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SparkFun-Jumper:Jumper_3_NC-1_Trace"
		(layer "F.Cu")
		(at 188.4586 48 180)
		(tags "SparkFun")
		(property "Reference" "JP3"
			(at 0 -1.143 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 1.143 0)
			(layer "F.Fab")
		)
		(property "Footprint" "SparkFun-Jumper:Jumper_3_NC-1_Trace"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3-pole Solder Jumper, pins 1+2 closed/bridged"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr allow_soldermask_bridges)
		(net_tie_pad_groups "1,2")
		(pad "1" smd rect
			(at -1.0414 0 180)
			(size 0.6604 1.27)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(A1-VBAT)")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0 0 180)
			(size 0.6604 1.27)
			(layers "F.Cu" "F.Mask")
			(net 26 "POW_IN_RAK")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 1.0414 0)
			(size 0.6604 1.27)
			(layers "F.Cu" "F.Mask")
			(net 2 "Net-(A1-VDD)")
			(pinfunction "C")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "F.Cu")
		(at 171.55 110.35)
		(descr "SOT-363, SC-70-6")
		(tags "SOT-363 SC-70-6")
		(property "Reference" "U4"
			(at 2.45 -3.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM66100DCK"
			(at 0 2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm66100.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ideal Diode With Input Polarity Protection 1.5 - 5.5V  Input Voltage, 1.5A Output Current, Ron 141 mOhm, SC-70-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SC?70*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "3V3_EXT_RAK")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "POW_IN_RAK")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U4-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "GND")
			(pinfunction "ST")
			(pintype "open_collector")
		)
		(pad "6" smd roundrect
			(at 0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "POW_IN_RAK")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 151.5 102.5)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
		(property "Reference" "C1"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10 uF"
			(at 2.5 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "POW_IN")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 176 107.28 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at 1.27 -1.92 90)
			(layer "F.SilkS")
		)
		(property "Value" "30"
			(at 1.27 1.92 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -1.92 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(Q1-C)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "mestasRider1:Pico2"
		(layer "F.Cu")
		(at 169.11 78.61)
		(property "Reference" "U2"
			(at 0 -26.23 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pi Pico 2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "mestasRider1:Pico2"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -8.89 -24.13 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "DIAGUARTTX")
			(pinfunction "GP0")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole oval
			(at -8.89 -21.59 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "DIAGUARTRX")
			(pinfunction "GP1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole oval
			(at -8.89 -19.05 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole oval
			(at -8.89 -16.51 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(U2-GP2-Pad4)")
			(pinfunction "GP2")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole oval
			(at -8.89 -13.97 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(U2-GP3-Pad5)")
			(pinfunction "GP3")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "6" thru_hole oval
			(at -8.89 -11.43 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(U2-GP4-Pad6)")
			(pinfunction "GP4")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "7" thru_hole oval
			(at -8.89 -8.89 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U2-GP5-Pad7)")
			(pinfunction "GP5")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "8" thru_hole oval
			(at -8.89 -6.35 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "9" thru_hole oval
			(at -8.89 -3.81 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(U2-GP6-Pad9)")
			(pinfunction "GP6")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "10" thru_hole oval
			(at -8.89 -1.27 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "GPIO7")
			(pinfunction "GP7")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "11" thru_hole oval
			(at -8.89 1.27 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "SOFTUARTTX")
			(pinfunction "GP8")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "12" thru_hole oval
			(at -8.89 3.81 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "SOFTUARTRX")
			(pinfunction "GP9")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "13" thru_hole oval
			(at -8.89 6.35 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "14" thru_hole oval
			(at -8.89 8.89 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GPIO8")
			(pinfunction "GP10")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "15" thru_hole oval
			(at -8.89 11.43 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "GPIO9")
			(pinfunction "GP11")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "16" thru_hole oval
			(at -8.89 13.97 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "GPIO10")
			(pinfunction "GP12")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "17" thru_hole oval
			(at -8.89 16.51 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "MCTXPin")
			(pinfunction "GP13")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "18" thru_hole oval
			(at -8.89 19.05 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "19" thru_hole oval
			(at -8.89 21.59 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "MCRXPin")
			(pinfunction "GP14")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "20" thru_hole oval
			(at -8.89 24.13 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "GPIO11")
			(pinfunction "GP15")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "21" thru_hole oval
			(at 8.89 24.13 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "GPIO12")
			(pinfunction "GP16")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "22" thru_hole oval
			(at 8.89 21.59 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "GPIO13")
			(pinfunction "GP17")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "23" thru_hole oval
			(at 8.89 19.05 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "24" thru_hole oval
			(at 8.89 16.51 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "GPIO14")
			(pinfunction "GP18")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "25" thru_hole oval
			(at 8.89 13.97 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "GPIO15")
			(pinfunction "GP19")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "26" thru_hole oval
			(at 8.89 11.43 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "GPIO16")
			(pinfunction "GP20")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "27" thru_hole oval
			(at 8.89 8.89 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "GPIO17")
			(pinfunction "GP21")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "28" thru_hole oval
			(at 8.89 6.35 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "29" thru_hole oval
			(at 8.89 3.81 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "GPIO18")
			(pinfunction "GP22")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "30" thru_hole oval
			(at 8.89 1.27 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(U2-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "31" thru_hole oval
			(at 8.89 -1.27 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(U2-GP26-Pad31)")
			(pinfunction "GP26")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "32" thru_hole oval
			(at 8.89 -3.81 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(U2-GP27-Pad32)")
			(pinfunction "GP27")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "33" thru_hole oval
			(at 8.89 -6.35 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "34" thru_hole oval
			(at 8.89 -8.89 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(U2-GP28-Pad34)")
			(pinfunction "GP28")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "35" thru_hole oval
			(at 8.89 -11.43 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(U2-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "36" thru_hole oval
			(at 8.89 -13.97 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(U2-3V3(OUT)-Pad36)")
			(pinfunction "3V3(OUT)")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "37" thru_hole oval
			(at 8.89 -16.51 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(U2-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "38" thru_hole oval
			(at 8.89 -19.05 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "39" thru_hole oval
			(at 8.89 -21.59 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "POW_IN_PICO")
			(pinfunction "VSYS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "40" thru_hole oval
			(at 8.89 -24.13 270)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(U2-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "41" thru_hole oval
			(at -2.54 23.9)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(U2-SWCLK-Pad41)")
			(pinfunction "SWCLK")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "42" thru_hole oval
			(at 0 23.9)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(U2-GND-Pad42)")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "43" thru_hole oval
			(at 2.54 23.9)
			(size 1.2 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(U2-SWDIO-Pad43)")
			(pinfunction "SWDIO")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH-12mm"
		(layer "F.Cu")
		(at 185 111.5)
		(descr "Generic SW PUSH 12mm, e.g https://sten-eswitch-13110800-production.s3.amazonaws.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
		(tags "tact sw push 12mm")
		(property "Reference" "SW1"
			(at 5.83 -5.41 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_SPST"
			(at 6.37 10.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH-12mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.25 2.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 3.2 1.9)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "MCTXPin")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" thru_hole oval
			(at 12.5 0)
			(size 3.2 1.9)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "MCTXPin")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 5)
			(size 3.2 1.9)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.5 5)
			(size 3.2 1.9)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 155 114.08 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "U1"
			(at 2.54 -4.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "LM1086CT-3-3"
			(at 2.54 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1117fd.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "800mA Low-Dropout Linear Regulator, 3.3V fixed output, SOT-223/TO-263"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223* TO?263*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_2)")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "POW_IN")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D1.8mm_W3.3mm_H2.4mm"
		(layer "F.Cu")
		(at 180 107 -90)
		(descr "LED, Round,  Rectangular size 3.3x2.4mm^2 diameter 1.8mm, 2 pins")
		(tags "LED Round  Rectangular size 3.3x2.4mm^2 diameter 1.8mm 2 pins")
		(property "Reference" "D1"
			(at 1.27 -2.26 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.26 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D1.8mm_W3.3mm_H2.4mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "3V3 Ext")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D1.8mm_W3.3mm_H2.4mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm"
		(layer "F.Cu")
		(at 147.42 84.46 -90)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
		(property "Reference" "J1"
			(at 5.54 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "DE9_Plug"
			(at 5.54 20.64 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Dsub:DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "9-pin male plug pin D-SUB connector"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Male*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.54 16.14 90)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -6.96 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 18.04 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "P1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.77 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.54 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "DIAGUARTRX")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 8.31 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J1-Pad4)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 11.08 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J1-Pad5)")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 1.385 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "DIAGUARTTX")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 4.155 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "POW_IN")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 6.925 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 9.695 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J1-Pad9)")
			(pinfunction "9")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 155.5 95.46 -90)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "J2"
			(at 1.27 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Counter_Clockwise"
			(at 1.27 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "MCTXPin")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "MCRXPin")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "P1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "P1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "mestasRider1:RAKBoardRaw"
		(layer "F.Cu")
		(at 136.500009 72.121035)
		(property "Reference" "A1"
			(at 3.999991 0.378965 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "mestasRider1:RAKBoardRaw"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 3.999992 -4.229992)
			(size 1.524 1.524)
			(drill 2.154)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 55.999989 -4.229992)
			(size 1.524 1.524)
			(drill 2.154)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 57.999982 -28.229993)
			(size 1.524 1.524)
			(drill 2.5)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at 35.500054 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(A1-BOOT-Pad1)")
			(pinfunction "BOOT")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 38.040054 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at 40.580054 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "SOFTUARTRX")
			(pinfunction "TX1")
			(pintype "output")
		)
		(pad "4" thru_hole circle
			(at 43.120057 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "SOFTUARTTX")
			(pinfunction "RX1")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 45.660057 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(A1-AIN1-Pad5)")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 48.200057 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(A1-IO1-Pad6)")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 50.740057 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(A1-IO2-Pad7)")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 53.280057 -28.730069)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(A1-VBAT)")
			(pinfunction "VBAT")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at 35.500055 -26.19007)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(A1-VDD)")
			(pinfunction "VDD")
			(pintype "power_out")
		)
		(pad "10" thru_hole circle
			(at 38.040055 -26.19007)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(zone_connect 0)
		)
		(pad "11" thru_hole circle
			(at 40.580055 -26.19007)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(A1-SCL-Pad11)")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 43.120058 -26.19007)
			(size 1.524 1.524)
			(drill 0.813)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(A1-SDA-Pad12)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "F.Cu")
		(at 166.5 110.35)
		(descr "SOT-363, SC-70-6")
		(tags "SOT-363 SC-70-6")
		(property "Reference" "U3"
			(at 2.5 -3.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM66100DCK"
			(at 0 2.15 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm66100.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ideal Diode With Input Polarity Protection 1.5 - 5.5V  Input Voltage, 1.5A Output Current, Ron 141 mOhm, SC-70-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SC?70*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "3V3_EXT_PICO")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "POW_IN_PICO")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U3-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "GND")
			(pinfunction "ST")
			(pintype "open_collector")
		)
		(pad "6" smd roundrect
			(at 0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "POW_IN_PICO")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 160.5 110.54 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Power Output Isolate Jumper"
			(at 4.63 -14 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "3V3 Ext")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SparkFun-Jumper:Jumper_2_NO"
		(layer "F.Cu")
		(at 166.55 107.35)
		(tags "SparkFun")
		(property "Reference" "JP1"
			(at 0 -1.143 0)
			(layer "F.Fab")
		)
		(property "Value" "SHORT TO BYPASS"
			(at 0 1.143 0)
			(layer "F.Fab")
		)
		(property "Footprint" "SparkFun-Jumper:Jumper_2_NO"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(pad "1" smd rect
			(at -0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 21 "3V3_EXT_PICO")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 0.4064 0)
			(size 0.635 1.27)
			(layers "F.Cu" "F.Mask")
			(net 25 "POW_IN_PICO")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 151.5 119.5)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
		(property "Reference" "C2"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10 uF"
			(at 2.5 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_DIP_SPSTx12_Slide_6.7x32.04mm_W7.62mm_P2.54mm_LowProfile"
		(layer "F.Cu")
		(at 197.8 100.45 180)
		(descr "12x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x32.04mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile")
		(tags "DIP Switch SPST Slide 7.62mm 300mil LowProfile")
		(property "Reference" "SW2"
			(at 3.81 -3.11 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_DIP_x12"
			(at 3.81 31.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_DIP_SPSTx12_Slide_6.7x32.04mm_W7.62mm_P2.54mm_LowProfile"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "12x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW?DIP?x12*")
		(sheetname "Root")
		(sheetfile "mestasRider1.kicad_sch")
		(attr through_hole)
		(fp_text user "on"
			(at 4.485 -1.3425 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 6.39 13.97 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "GND")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 7.62 27.94 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "GPIO18")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 7.62 25.4 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "GPIO17")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 7.62 22.86 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "GPIO16")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 7.62 20.32 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "GPIO15")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 7.62 17.78 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "GPIO14")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 7.62 15.24 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "GPIO13")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 7.62 12.7 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "GPIO12")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 7.62 10.16 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "GPIO11")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 7.62 7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "GPIO10")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "GPIO9")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GPIO8")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "GPIO7")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx12_Slide_6.7x32.04mm_W7.62mm_P2.54mm_LowProfile.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(gr_line
		(start 200 120.5)
		(end 198 122.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149 121)
		(end 149 113.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196 41)
		(end 200 45)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.5 65)
		(end 168.5 41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.5 108)
		(end 143.5 108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.5 106)
		(end 134.5 68.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138 65)
		(end 134.5 68.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149 113.5)
		(end 143.5 108)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.5 122.5)
		(end 149 121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 198 122.5)
		(end 150.5 122.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200 45)
		(end 200 120.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.5 41)
		(end 196 41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.5 65)
		(end 138 65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.5 106)
		(end 136.5 108)
		(layer "Edge.Cuts")
	)
	(zone
		(net 24)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 207.5 37) (xy 208.5 130) (xy 132.5 130) (xy 133 38.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174.5 46) (xy 174.5 47.5) (xy 172.5 47.5) (xy 172 44.5) (xy 173.5 43.5) (xy 175.5 43.5) (xy 175.5 45.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177 44.5) (xy 175.5 43.5) (xy 173.5 43.5) (xy 172 44.5) (xy 173.5 46) (xy 175.5 46)
			)
		)
	)
	(zone
		(net 24)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 133 38.5) (xy 207.5 37) (xy 208.5 130) (xy 132.5 130)
			)
		)
	)
)
