<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="76.2" y2="0" width="0.1524" layer="20"/>
<wire x1="76.2" y1="0" x2="76.2002" y2="0" width="0.1524" layer="20"/>
<wire x1="76.2" y1="38.1" x2="76.2" y2="53.3298" width="0.1524" layer="20"/>
<wire x1="76.2" y1="53.3298" x2="76.2002" y2="53.33" width="0.1524" layer="20"/>
<wire x1="76.2002" y1="53.33" x2="0" y2="53.33" width="0.1524" layer="20"/>
<wire x1="0" y1="53.33" x2="0" y2="33.02" width="0.1524" layer="20"/>
<wire x1="0" y1="20.32" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="20.32" x2="12.5476" y2="20.32" width="0.1524" layer="20"/>
<wire x1="12.5476" y1="20.32" x2="12.5476" y2="33.02" width="0.1524" layer="20"/>
<wire x1="12.5476" y1="33.02" x2="0" y2="33.02" width="0.1524" layer="20"/>
<wire x1="76.2" y1="15.24" x2="60.96" y2="15.24" width="0.1524" layer="20"/>
<wire x1="60.96" y1="15.24" x2="60.96" y2="38.1" width="0.1524" layer="20"/>
<wire x1="60.96" y1="38.1" x2="76.2" y2="38.1" width="0.1524" layer="20"/>
<hole x="2.54" y="2.54" drill="3.302"/>
<hole x="2.54" y="50.8" drill="3.302"/>
<hole x="73.66" y="2.54" drill="3.302"/>
<hole x="73.66" y="50.8" drill="3.302"/>
<wire x1="76.2" y1="15.24" x2="76.2" y2="0" width="0.1524" layer="20"/>
<wire x1="44.45" y1="30.3784" x2="44.45" y2="22.9616" width="0.1524" layer="20"/>
<wire x1="44.45" y1="22.9616" x2="41.9354" y2="20.3708" width="0.1524" layer="20"/>
<wire x1="41.9354" y1="20.3708" x2="34.3154" y2="20.3708" width="0.1524" layer="20"/>
<wire x1="34.3154" y1="20.3708" x2="31.7246" y2="22.9362" width="0.1524" layer="20"/>
<wire x1="31.7246" y1="22.9362" x2="31.75" y2="30.4546" width="0.1524" layer="20"/>
<wire x1="31.75" y1="30.4546" x2="34.2646" y2="32.9184" width="0.1524" layer="20"/>
<wire x1="34.2646" y1="32.9184" x2="41.8846" y2="32.9184" width="0.1524" layer="20"/>
<wire x1="41.8846" y1="32.9184" x2="44.45" y2="30.3784" width="0.1524" layer="20"/>
<text>Supply
12V</text>
<text>Supply
GND</text>
<text>Output
LOW</text>
<text>Output
HIGH</text>
<text>Cathode</text>
<text>Anode</text>
<text>Learning</text>
<text>Power Switch</text>
<text>Mode Switch</text>
<text>AutoOff Switch</text>
<text>Delay</text>
<text>RV-Project.Com</text>
<text>SC1 (Self Contained) Dimmer</text>
<text>V1.2    5/29/2019</text>
<text>cut out</text>
<text>Offset to allow for 
switch clearance</text>
<text>C</text>
<text>L</text>
<text>C</text>
<text>L</text>
<text>Offset to allow for 
switch clearance</text>
<text>1/2" Standoff (13mm)</text>
<text>Option: Mount from
reverse side, add
Slot in panel for
DiP switch access.</text>
<text>When laying out panel,
remember top of PCB
is on backside.</text>
<text>1 Oz Copper = 2A Load 
2 Oz Copper = 4A Load</text>
<text>+</text>
<text>-</text>
<text>LED</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="GENERIC_0100_DEVICE_150_SPACING">
<description>Pitch: 0.15" (3.81mm)</description>
</package>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor.&lt;br&gt;Pitch:0.1&lt;br&gt;
Dia: 0.2"Dia (5.08mm)</description>
</package>
<package name="D041-3.5MIL">
<description>Pitch: 0.35"</description>
</package>
<package name="251SMALL">
<description>Pitch: 0.45"&lt;br&gt;
Drill: 0.027" dia</description>
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;Pitch: 0.35"</description>
</package>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="1X02_HEADER">
<description>Pitch: 0.1" (2.54mm)&lt;br&gt;Drill: 0.040" dia</description>
</package>
<package name="KEYSTONE8191">
</package>
<package name="1X01_HEADER">
<description>Drill: 0.039" dia</description>
</package>
</packages>
</library>
<library name="a-lib_Modules">
<packages>
<package name="MICRO_RECEIVER_1">
<description>Pitch: 2mm</description>
</package>
</packages>
</library>
<library name="a-lib_Actives">
<description>Thru-Hole Actives (Transistors, Diodes, MPUs)</description>
<packages>
<package name="TO-220-HEATSINK_MOSFET">
<description>IGO TO-220 with small horizontal heatsink.</description>
</package>
<package name="IPAK_HORIZONTAL(TO251)">
<description>IPAK (TO252).</description>
</package>
</packages>
</library>
<library name="a-lib_Switches">
<description>Thru-Hole Switches, Relays</description>
<packages>
<package name="2PINTACT">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_SMALL">
</package>
<package name="USA">
</package>
<package name="CREATIVECOMMONS_SMALL">
</package>
</packages>
</library>
<library name="a-lib_Passives">
<description>Thru-Hole Passives (Resistors, Capacitors)</description>
<packages>
<package name="GENERIC_0100_DEVICE_150_SPACING">
<description>Pitch: 0.15" (3.81mm)</description>
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;Pitch: 0.35"</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="a-lib" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="a-lib" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="F1" library="a-lib" package="251SMALL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="a-lib_Actives" package="TO-220-HEATSINK_MOSFET" value="IRLZ44">
<attribute name="NAME"/>
</element>
<element name="R3" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE" value="22k"/>
</element>
<element name="R2" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE" value="33k"/>
</element>
<element name="R1" library="a-lib_Passives" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R4" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="10k">
<attribute name="NAME"/>
</element>
<element name="R5" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="10k">
<attribute name="NAME"/>
</element>
<element name="S2" library="a-lib" package="DIL04" value="DIPSWITCH-2"/>
<element name="U1" library="a-lib" package="DIP08" value="TINY85-20-DIP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="U2" library="a-lib_Actives" package="IPAK_HORIZONTAL(TO251)" value="78XX">
<attribute name="NAME"/>
</element>
<element name="C2" library="a-lib" package="GENERIC_0100_DEVICE_150_SPACING" value="0.33uF">
<attribute name="NAME"/>
</element>
<element name="R7" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="D1" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="D2" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="J1" library="a-lib_Connectors" package="1X02_HEADER" value="M2HEADER"/>
<element name="J2" library="a-lib_Connectors" package="1X02_HEADER" value="M2HEADER"/>
<element name="RX1" library="a-lib_Modules" package="MICRO_RECEIVER_1" value="ASK-OOK_MICRO_RECEIVER(RELAY)_1CHANNEL"/>
<element name="TB3" library="a-lib_Connectors" package="KEYSTONE8191" value="">
<attribute name="VALUE"/>
</element>
<element name="TB4" library="a-lib_Connectors" package="KEYSTONE8191" value="">
<attribute name="VALUE"/>
</element>
<element name="TB2" library="a-lib_Connectors" package="KEYSTONE8191" value="">
<attribute name="VALUE"/>
</element>
<element name="TB1" library="a-lib_Connectors" package="KEYSTONE8191" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="a-lib_Connectors" package="1X02_HEADER" value="M2HEADER"/>
<element name="S1" library="a-lib_Switches" package="2PINTACT" value=""/>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_SMALL" value=""/>
<element name="U$2" library="a-lib_Asthetics" package="USA" value=""/>
<element name="U$4" library="a-lib_Asthetics" package="CREATIVECOMMONS_SMALL" value=""/>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
</element>
<element name="TB5" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="TB6" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="TB7" library="a-lib_Connectors" package="1X01_HEADER" value="">
<attribute name="VALUE"/>
</element>
<element name="C5" library="a-lib_Passives" package="GENERIC_0100_DEVICE_150_SPACING" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="O"/>
<contactref element="TB7" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="G"/>
<contactref element="C4" pad="2"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="S"/>
<contactref element="R7" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="RX1" pad="GND1"/>
<contactref element="RX1" pad="COM1"/>
<contactref element="TB4" pad="P$3"/>
<contactref element="TB4" pad="P$1"/>
<contactref element="TB4" pad="P$2"/>
<contactref element="TB4" pad="P$4"/>
<contactref element="R6" pad="2"/>
<contactref element="TB6" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="2"/>
<contactref element="RX1" pad="NO1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="6"/>
<contactref element="Q1" pad="G"/>
<contactref element="R7" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="12V">
<contactref element="U2" pad="I"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="F1" pad="P$1"/>
<contactref element="D2" pad="C"/>
<contactref element="RX1" pad="12V1"/>
<contactref element="TB2" pad="P$3"/>
<contactref element="TB2" pad="P$1"/>
<contactref element="TB2" pad="P$2"/>
<contactref element="TB2" pad="P$4"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="7"/>
<contactref element="TB5" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="J2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$5">
</signal>
<signal name="N$9">
</signal>
<signal name="N$17">
</signal>
<signal name="N$10">
</signal>
<signal name="N$23">
</signal>
<signal name="N$6">
</signal>
<signal name="N$27">
</signal>
<signal name="N$25">
<contactref element="Q1" pad="D"/>
<contactref element="D2" pad="A"/>
<contactref element="TB3" pad="P$3"/>
<contactref element="TB3" pad="P$1"/>
<contactref element="TB3" pad="P$2"/>
<contactref element="TB3" pad="P$4"/>
</signal>
<signal name="N$26">
</signal>
<signal name="N$22">
<contactref element="F1" pad="P$2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="N$12">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="TB1" pad="P$3"/>
<contactref element="TB1" pad="P$1"/>
<contactref element="TB1" pad="P$2"/>
<contactref element="TB1" pad="P$4"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="RX1" pad="L2"/>
<contactref element="S1" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="RX1" pad="L1"/>
<contactref element="S1" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="LED1" pad="K"/>
<contactref element="R6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
