(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 161)
    (no_connects 0)
    (area 142.170999 96.454099 160.101001 132.164101)
    (thickness 1.6)
    (drawings 90)
    (tracks 899)
    (zones 0)
    (modules 45)
    (nets 71)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1)
    (user_trace_width 0.1)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (trace_clearance 0.1)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.5)
    (via_drill 0.2)
    (via_min_size 0.5)
    (via_min_drill 0.2)
    (user_via 0.5 0.2)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.25 0.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 151.13 99.314)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory TinyFPGA_BX_Rev11/))
  )
  (net 0 "")
  (net 1 CDONE)
  (net 2 VPP_FAST)
  (net 3 224)
  (net 4 221)
  (net 5 185)
  (net 6 174)
  (net 7 116)
  (net 8 3A)
  (net 9 3B)
  (net 10 148)
  (net 11 10A)
  (net 12 212)
  (net 13 115)
  (net 14 119)
  (net 15 10B)
  (net 16 24B)
  (net 17 26A)
  (net 18 24A)
  (net 19 81_GBIN5)
  (net 20 54)
  (net 21 26B)
  (net 22 55)
  (net 23 177)
  (net 24 "Net-(J3-Pad1)")
  (net 25 "Net-(J3-Pad2)")
  (net 26 "Net-(J3-Pad3)")
  (net 27 "Net-(J3-Pad4)")
  (net 28 "Net-(U4-Pad4)")
  (net 29 +5V)
  (net 30 CLK)
  (net 31 +1V2)
  (net 32 SCK)
  (net 33 CRESET_B)
  (net 34 SDI)
  (net 35 SS)
  (net 36 GND)
  (net 37 +3V3)
  (net 38 SDO)
  (net 39 USB_P)
  (net 40 USB_N)
  (net 41 "Net-(C6-Pad1)")
  (net 42 "Net-(C6-Pad2)")
  (net 43 "Net-(U1-PadF3)")
  (net 44 "Net-(U1-PadC3)")
  (net 45 "Net-(U1-PadC4)")
  (net 46 "Net-(U1-PadC5)")
  (net 47 "Net-(U1-PadD3)")
  (net 48 "Net-(U1-PadD7)")
  (net 49 "Net-(U1-PadE7)")
  (net 50 USB_PU)
  (net 51 2A)
  (net 52 13A)
  (net 53 183)
  (net 54 7A)
  (net 55 180)
  (net 56 170)
  (net 57 141)
  (net 58 111)
  (net 59 LED)
  (net 60 140)
  (net 61 110)
  (net 62 57)
  (net 63 112)
  (net 64 70)
  (net 65 109)
  (net 66 "Net-(D1-Pad1)")
  (net 67 "Net-(D2-Pad1)")
  (net 68 82)
  (net 69 "Net-(U1-PadG5)")
  (net 70 56)
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.1)
    (via_dia 0.5)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V2)
    (add_net +3V3)
    (add_net +5V)
    (add_net 109)
    (add_net 10A)
    (add_net 10B)
    (add_net 110)
    (add_net 111)
    (add_net 112)
    (add_net 115)
    (add_net 116)
    (add_net 119)
    (add_net 13A)
    (add_net 140)
    (add_net 141)
    (add_net 148)
    (add_net 170)
    (add_net 174)
    (add_net 177)
    (add_net 180)
    (add_net 183)
    (add_net 185)
    (add_net 212)
    (add_net 221)
    (add_net 224)
    (add_net 24A)
    (add_net 24B)
    (add_net 26A)
    (add_net 26B)
    (add_net 2A)
    (add_net 3A)
    (add_net 3B)
    (add_net 54)
    (add_net 55)
    (add_net 56)
    (add_net 57)
    (add_net 70)
    (add_net 7A)
    (add_net 81_GBIN5)
    (add_net 82)
    (add_net CDONE)
    (add_net CLK)
    (add_net CRESET_B)
    (add_net GND)
    (add_net LED)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(U1-PadC3)")
    (add_net "Net-(U1-PadC4)")
    (add_net "Net-(U1-PadC5)")
    (add_net "Net-(U1-PadD3)")
    (add_net "Net-(U1-PadD7)")
    (add_net "Net-(U1-PadE7)")
    (add_net "Net-(U1-PadF3)")
    (add_net "Net-(U1-PadG5)")
    (add_net "Net-(U4-Pad4)")
    (add_net SCK)
    (add_net SDI)
    (add_net SDO)
    (add_net SS)
    (add_net USB_N)
    (add_net USB_P)
    (add_net USB_PU)
    (add_net VPP_FAST)
  )
  (net_class large ""
    (clearance 0.1)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class xlarge ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module tinyfpga:CM81 (layer F.Cu) (tedit 5A43F366)
    (at 151.13 114.114)
    (attr smd)
    (fp_text reference U1 (at 0 1.2091) (layer F.Fab))
    (fp_text value iCE40-LP8K-CM81 (at 0.006 -0.4909) (layer F.Fab))
    (pad A1 smd oval (at -1.6 -1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 3 224) (solder_mask_margin 0.05))
    (pad A2 smd oval (at -1.2 -1.6) (size 0.1 0.33) (layers F.Cu F.Paste F.Mask)
      (net 4 221) (solder_mask_margin 0.05))
    (pad A3 smd oval (at -0.8 -1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 50 USB_PU) (solder_mask_margin 0.05))
    (pad A4 smd oval (at -0.4 -1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 40 USB_N) (solder_mask_margin 0.05))
    (pad A5 smd circle (at 0 -1.6) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad A6 smd oval (at 0.4 -1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 5 185) (solder_mask_margin 0.05))
    (pad A7 smd oval (at 0.8 -1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 23 177) (solder_mask_margin 0.05))
    (pad A8 smd oval (at 1.2 -1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 6 174) (solder_mask_margin 0.05))
    (pad A9 smd oval (at 1.6 -1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 7 116) (solder_mask_margin 0.05))
    (pad B1 smd oval (at -1.6 -1.2) (size 0.33 0.1) (layers F.Cu F.Paste F.Mask)
      (net 8 3A) (solder_mask_margin 0.05))
    (pad B2 smd circle (at -1.2 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 30 CLK) (solder_mask_margin 0.05))
    (pad B3 smd circle (at -0.8 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 59 LED) (solder_mask_margin 0.05))
    (pad B4 smd circle (at -0.4 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 39 USB_P) (solder_mask_margin 0.05))
    (pad B5 smd circle (at 0 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad B6 smd circle (at 0.4 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 53 183) (solder_mask_margin 0.05))
    (pad B7 smd circle (at 0.8 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 55 180) (solder_mask_margin 0.05))
    (pad B8 smd circle (at 1.2 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 56 170) (solder_mask_margin 0.05))
    (pad B9 smd circle (at 1.6 -1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad C1 smd oval (at -1.6 -0.8) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 9 3B) (solder_mask_margin 0.05))
    (pad C2 smd circle (at -1.2 -0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 51 2A) (solder_mask_margin 0.05))
    (pad C3 smd circle (at -0.8 -0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-PadC3)") (solder_mask_margin 0.05))
    (pad C4 smd circle (at -0.4 -0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-PadC4)") (solder_mask_margin 0.05))
    (pad C5 smd circle (at 0 -0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-PadC5)") (solder_mask_margin 0.05))
    (pad C6 smd circle (at 0.4 -0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad C7 smd circle (at 0.8 -0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VPP_FAST) (solder_mask_margin 0.05))
    (pad C8 smd circle (at 1.2 -0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad C9 smd oval (at 1.6 -0.8) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 10 148) (solder_mask_margin 0.05))
    (pad D1 smd oval (at -1.6 -0.4) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 11 10A) (solder_mask_margin 0.05))
    (pad D2 smd circle (at -1.2 -0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 54 7A) (solder_mask_margin 0.05))
    (pad D3 smd circle (at -0.8 -0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-PadD3)") (solder_mask_margin 0.05))
    (pad D4 smd circle (at -0.4 -0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2) (solder_mask_margin 0.05))
    (pad D5 smd circle (at 0 -0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 12 212) (solder_mask_margin 0.05))
    (pad D6 smd circle (at 0.4 -0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 13 115) (solder_mask_margin 0.05))
    (pad D7 smd circle (at 0.8 -0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-PadD7)") (solder_mask_margin 0.05))
    (pad D8 smd circle (at 1.2 -0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 57 141) (solder_mask_margin 0.05))
    (pad D9 smd oval (at 1.6 -0.4) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 14 119) (solder_mask_margin 0.05))
    (pad E1 smd oval (at -1.6 0) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 15 10B) (solder_mask_margin 0.05))
    (pad E2 smd circle (at -1.2 0) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 52 13A) (solder_mask_margin 0.05))
    (pad E3 smd circle (at -0.8 0) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2) (solder_mask_margin 0.05))
    (pad E4 smd circle (at -0.4 0) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad E5 smd circle (at 0 0) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad E6 smd circle (at 0.4 0) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 CDONE) (solder_mask_margin 0.05))
    (pad E7 smd circle (at 0.8 0) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-PadE7)") (solder_mask_margin 0.05))
    (pad E8 smd circle (at 1.2 0) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 60 140) (solder_mask_margin 0.05))
    (pad E9 smd oval (at 1.6 0) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2) (solder_mask_margin 0.05))
    (pad F1 smd circle (at -1.6 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2) (solder_mask_margin 0.05))
    (pad F2 smd circle (at -1.2 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2) (solder_mask_margin 0.05))
    (pad F3 smd circle (at -0.8 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-PadF3)") (solder_mask_margin 0.05))
    (pad F4 smd circle (at -0.4 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad F5 smd circle (at 0 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad F6 smd circle (at 0.4 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad F7 smd circle (at 0.8 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 35 SS) (solder_mask_margin 0.05))
    (pad F8 smd circle (at 1.2 0.4) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 35 SS) (solder_mask_margin 0.05))
    (pad F9 smd oval (at 1.6 0.4) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad G1 smd oval (at -1.6 0.8) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 16 24B) (solder_mask_margin 0.05))
    (pad G2 smd circle (at -1.2 0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 17 26A) (solder_mask_margin 0.05))
    (pad G3 smd circle (at -0.8 0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 18 24A) (solder_mask_margin 0.05))
    (pad G4 smd circle (at -0.4 0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 19 81_GBIN5) (solder_mask_margin 0.05))
    (pad G5 smd circle (at 0 0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-PadG5)") (solder_mask_margin 0.05))
    (pad G6 smd circle (at 0.4 0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 38 SDO) (solder_mask_margin 0.05))
    (pad G7 smd circle (at 0.8 0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 32 SCK) (solder_mask_margin 0.05))
    (pad G8 smd circle (at 1.2 0.8) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 32 SCK) (solder_mask_margin 0.05))
    (pad G9 smd oval (at 1.6 0.8) (size 0.335 0.1) (layers F.Cu F.Paste F.Mask)
      (net 63 112) (solder_mask_margin 0.05))
    (pad H1 smd oval (at -1.6 1.2) (size 0.33 0.1) (layers F.Cu F.Paste F.Mask)
      (net 20 54) (solder_mask_margin 0.05))
    (pad H2 smd circle (at -1.2 1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 21 26B) (solder_mask_margin 0.05))
    (pad H3 smd circle (at -0.8 1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad H4 smd circle (at -0.4 1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 68 82) (solder_mask_margin 0.05))
    (pad H5 smd circle (at 0 1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 38 SDO) (solder_mask_margin 0.05))
    (pad H6 smd circle (at 0.4 1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 33 CRESET_B) (solder_mask_margin 0.05))
    (pad H7 smd circle (at 0.8 1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 34 SDI) (solder_mask_margin 0.05) (clearance 0.1))
    (pad H8 smd circle (at 1.2 1.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad H9 smd oval (at 1.6 1.2) (size 0.33 0.1) (layers F.Cu F.Paste F.Mask)
      (net 58 111) (solder_mask_margin 0.05))
    (pad J1 smd oval (at -1.6 1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 22 55) (solder_mask_margin 0.05) (clearance 0.1))
    (pad J2 smd oval (at -1.2 1.6) (size 0.1 0.33) (layers F.Cu F.Paste F.Mask)
      (net 70 56) (solder_mask_margin 0.05))
    (pad J3 smd oval (at -0.8 1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 62 57) (solder_mask_margin 0.05))
    (pad J4 smd oval (at -0.4 1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 64 70) (solder_mask_margin 0.05))
    (pad J5 smd oval (at 0 1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad J6 smd oval (at 0.4 1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C6-Pad1)") (solder_mask_margin 0.05))
    (pad J7 smd oval (at 0.8 1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad2)") (solder_mask_margin 0.05))
    (pad J8 smd oval (at 1.2 1.6) (size 0.1 0.33) (layers F.Cu F.Paste F.Mask)
      (net 65 109) (solder_mask_margin 0.05))
    (pad J9 smd oval (at 1.6 1.6) (size 0.1 0.335) (layers F.Cu F.Paste F.Mask)
      (net 61 110) (solder_mask_margin 0.05))
    (model ../../../../../../Users/lvale/Documents/TinyFPGA/repos/TinyFPGA-B-Series/board/tinyfpga.pretty/UCBGA-81_9x9_4x4mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer F.Cu) (tedit 5923D90A)
    (at 143.516 97.7991)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.Fab) hide)
    (fp_text value CONN_01X14 (at 0 35.35) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 221))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 224))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 3A))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 2A))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 3B))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 7A))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 10A))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 13A))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 10B))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 26A))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 54))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 55))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 26B))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 -0.075))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm_SMD (layer B.Cu) (tedit 5A9C67A9)
    (at 152.431 121.9291 180)
    (descr "surface-mounted straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x08 2.54mm double row")
    (attr smd)
    (fp_text reference J4 (at 0 11.22 180) (layer B.SilkS) hide)
    (fp_text value Conn_02x08_Odd_Even (at 0 -11.22 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -2.525 8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 60 140))
    (pad 2 smd rect (at 2.525 8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 16 24B))
    (pad 3 smd rect (at -2.525 6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 37 +3V3))
    (pad 4 smd rect (at 2.525 6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 36 GND))
    (pad 5 smd rect (at -2.525 3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 61 110))
    (pad 6 smd rect (at 2.525 3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 62 57))
    (pad 7 smd rect (at -2.525 1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 63 112))
    (pad 8 smd rect (at 2.525 1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 64 70))
    (pad 9 smd rect (at -2.525 -1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 65 109))
    (pad 10 smd rect (at 2.525 -1.27 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 68 82))
    (pad 11 smd rect (at -2.525 -3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 32 SCK))
    (pad 12 smd rect (at 2.525 -3.81 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 34 SDI))
    (pad 13 smd rect (at -2.525 -6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 38 SDO))
    (pad 14 smd rect (at 2.525 -6.35 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SS))
    (pad 15 smd rect (at -2.525 -8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 36 GND))
    (pad 16 smd rect (at 2.525 -8.89 180) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 591F8EE7)
    (at 151.136 124.2581)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 0) (layer F.Fab))
    (fp_text value AT25SF081-SSHD-B (at 0 1.4) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 SS))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 SDI))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 82))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 SDO))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 SCK))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 109))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer B.Cu) (tedit 5A3BF6DE)
    (at 149.851 102.8791)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J5 (at 0 4.87) (layer B.Fab) hide)
    (fp_text value Conn_02x03_Odd_Even (at 0 -4.87) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.525 2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 30 CLK))
    (pad 2 smd rect (at 2.525 2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 70 56))
    (pad 3 smd rect (at -2.525 0) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 59 LED))
    (pad 4 smd rect (at 2.525 0) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 50 USB_PU))
    (pad 5 smd rect (at -2.525 -2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 39 USB_P))
    (pad 6 smd rect (at 2.525 -2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 40 USB_N))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5A3B4713)
    (at 155.962 110.4991)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP3 (at 0 0.9) (layer B.SilkS) hide)
    (fp_text value TEST (at 0 -0.9) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 31 +1V2))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 5A3AFAB9)
    (at 151.009 109.1021 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5A3A12FD)
    (at 154.536 130.3731 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -0.875 0 270) (layer F.Fab))
    (fp_text value R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 CRESET_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A3A12EC)
    (at 151.736 120.1231 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 1.1 0 270) (layer F.Fab))
    (fp_text value 10uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A3A12E0)
    (at 156.036 100.9231 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -1.275 0 90) (layer F.Fab))
    (fp_text value 10uF (at 0 0.025 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 5A3A12D1)
    (at 153.886 102.4231 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 0 180) (layer F.Fab))
    (fp_text value Bead (at 0 0.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (model Inductors_SMD.3dshapes\L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 5A39FA77)
    (at 146.183 105.6731 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 0.7 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 5A39FA48)
    (at 148.215 105.6731 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 0.7 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A3BFA18)
    (at 148.215 103.3871 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 0 0.635 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5A3BFA0D)
    (at 146.183 103.3871 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.25 90) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 0 0.635 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 59 LED))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_Molex:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 595DDA79)
    (at 151.136 97.9731 180)
    (descr http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)
    (tags "Micro-USB SMD")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference J3 (at 0 4.55 360) (layer F.Fab))
    (fp_text value USB_OTG (at -0.005637 3.079657 360) (layer F.Fab))
    (fp_text user "PCB Front Edge" (at 7.65 1.5 360) (layer Dwgs.User))
    (pad 1 smd rect (at -1.3 -2.675 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -0.65 -2.675 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0 -2.675 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 0.65 -2.675 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 1.3 -2.675 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 6 smd rect (at -3.1 -2.55 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 6 smd rect (at 3.1 -2.55 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 6 smd rect (at -3.8 0 270) (size 1.9 1.8) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 6 smd rect (at 3.8 0 270) (size 1.9 1.8) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 6 smd rect (at -1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 6 smd rect (at 1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ../../../../../../Users/lvale/Documents/TinyFPGA/repos/TinyFPGA-B-Series/board/tinyfpga.pretty/USB-Micro.wrl
      (at (xyz 0 0.01 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module tinyfpga:CDFN3225-4LD-PL-1 (layer F.Cu) (tedit 595DCA31)
    (at 148.039614 109.364854 180)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference U3 (at 0 -0.6 180) (layer F.Fab))
    (fp_text value DSC6001CI2A-016.0000T (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.046386 0.941754 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 4 smd rect (at -1.046386 -0.958246 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 3 smd rect (at 1.053614 -0.958246 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 CLK))
    (pad 2 smd rect (at 1.053614 0.941754 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ../../../../../../Users/lvale/Documents/TinyFPGA/repos/TinyFPGA-B-Series/board/tinyfpga.pretty/DFN-4_2x2_2.5x3.2mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 59227DE2)
    (at 146.31 129.5491)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 0 0.425) (layer B.Fab))
    (fp_text value TEST (at 0 -0.375) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 68 82))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5923CDF4)
    (at 146.31 124.4691)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP2 (at 0 0.425) (layer B.Fab))
    (fp_text value TEST (at 0 -0.475) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 33 CRESET_B))
  )
  (module tinyfpga:SC-70-C5 (layer F.Cu) (tedit 593651E8)
    (at 153.636 105.1731)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference U2 (at 0 -0.1) (layer F.Fab))
    (fp_text value MIC5504-3.3YM5-TR (at 0 0.3) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.3) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 3 smd rect (at -0.95 -1.3) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 29 +5V))
    (pad 1 smd rect (at 0.95 -1.3) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 29 +5V))
    (pad 4 smd rect (at -0.95 1.3) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 5 smd rect (at 0.95 1.3) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (model ../../../../../../Users/lvale/Documents/TinyFPGA/repos/TinyFPGA-B-Series/board/tinyfpga.pretty/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59227D88)
    (at 146.9 126.954)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at -0.875 0.05) (layer F.Fab))
    (fp_text value 10k (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 82))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer F.Cu) (tedit 5923D90E)
    (at 158.756 97.7991)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.Fab) hide)
    (fp_text value CONN_01X14 (at 0 35.35) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 +3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 185))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 183))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 177))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 180))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 174))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 170))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 116))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 148))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 141))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 119))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 111))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 -0.075))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E97BE)
    (at 150.555 118.414 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 0.9 0 270) (layer F.Fab))
    (fp_text value 100nF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 5A43ECB6)
    (at 153.93 115.464 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -0.875 0 90) (layer F.Fab))
    (fp_text value 10k (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.38 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.38 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 SS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E94D1)
    (at 154.38 114.164)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 0.9 0) (layer F.Fab))
    (fp_text value 10nF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E9451)
    (at 151.13 110.964 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference C15 (at 0.9 0 90) (layer F.Fab))
    (fp_text value 10nF (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E93FE)
    (at 154.105 112.439)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 0.9 0) (layer F.Fab))
    (fp_text value 10nF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E9370)
    (at 147.436 114.9231 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0.9 0 180) (layer F.Fab))
    (fp_text value 10nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E931C)
    (at 147.436 114.1231 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0.9 0 180) (layer F.Fab))
    (fp_text value 100nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E92B2)
    (at 148.5198 107.3495 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0.9 0 180) (layer F.Fab))
    (fp_text value 100nF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E9218)
    (at 153.255 117.514 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0.85 0 270) (layer F.Fab))
    (fp_text value 100nF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591E91DB)
    (at 148.836 117.8231 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0.85 0 270) (layer F.Fab))
    (fp_text value 100nF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591D48CF)
    (at 151.736 117.6731 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0.9 0 270) (layer F.Fab))
    (fp_text value 100nF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 591D4866)
    (at 152.936 120.4231 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -0.8 0 90) (layer F.Fab))
    (fp_text value 100 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk locked (layer F.Cu) (tedit 591D47FF)
    (at 155.336 122.9231 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0.85 0 270) (layer F.Fab))
    (fp_text value 100nF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 591D2795)
    (at 149.636 102.7231 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0.8 0 270) (layer F.Fab))
    (fp_text value 1.5k (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 USB_PU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 591D270C)
    (at 150.636 102.7231 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -0.8 0 90) (layer F.Fab))
    (fp_text value 68 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 USB_P))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 591D26E3)
    (at 151.636 102.7231 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -0.8 0 90) (layer F.Fab))
    (fp_text value 68 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 USB_N))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tinyfpga:SC-70-C5 (layer F.Cu) (tedit 5ABAF6E7)
    (at 153.936 108.7231)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference U4 (at 0 0) (layer F.Fab))
    (fp_text value MIC5365-1.2YC5-TR (at 0 1) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.1) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 3 smd rect (at -0.65 -1.1) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 1 smd rect (at 0.65 -1.1) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3) (solder_mask_margin 0.05))
    (pad 4 smd rect (at -0.65 1.1) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at 0.65 1.1) (size 0.45 0.95) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2))
    (model ../../../../../../Users/lvale/Documents/TinyFPGA/repos/TinyFPGA-B-Series/board/tinyfpga.pretty/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591BE6A8)
    (at 155.936 109.9231)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0.9 0) (layer F.Fab))
    (fp_text value 1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 +1V2))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591BE6A0)
    (at 155.936 103.9231)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0.9 0) (layer F.Fab))
    (fp_text value 1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 +5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591BE664)
    (at 155.936 106.3231)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0.9 0) (layer F.Fab))
    (fp_text value 1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 591BE66E)
    (at 155.936 107.5231)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0.9 0) (layer F.Fab))
    (fp_text value 1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tinyfpga:PTS_810_SMT_Switch (layer F.Cu) (tedit 591BDDCE)
    (at 151.136 129.7231)
    (attr smd)
    (fp_text reference SW1 (at 0 0) (layer F.Fab))
    (fp_text value SW_Push (at 0 -3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.075 -1.075) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at 2.075 -1.075) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd rect (at 2.075 1.075) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 CRESET_B))
    (pad 2 smd rect (at -2.075 1.075) (size 1.05 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 CRESET_B))
    (model ../../../../../../Users/lvale/Documents/TinyFPGA/repos/TinyFPGA-B-Series/board/tinyfpga.pretty/Y97M01810FP.wrl
      (at (xyz 0 0 0.055))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 5ABAFCB4)
    (at 155.14 127.064)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at -0.01 -0.47) (layer F.Fab) hide)
    (fp_text value 10k (at 0.004 0.469899) (layer F.Fab))
    (fp_text user %R (at -0.01 -0.470101) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 109))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text IO0 (at 152.655 128.2791 270) (layer B.SilkS))
  (gr_text G (at 147.58 115.5791 270) (layer B.SilkS))
  (gr_text 31 (at 154.692 105.4191 270) (layer B.SilkS))
  (gr_text CLK (at 149.612 105.4191 270) (layer B.SilkS))
  (gr_text 1.2v (at 155.962 109.4831 270) (layer B.SilkS))
  (gr_text RST (at 146.31 123.4531 270) (layer B.SilkS))
  (gr_text WP (at 146.31 128.5331 270) (layer B.SilkS))
  (gr_text "TinyFPGA Bx" (at 151.13 98.439) (layer B.SilkS))
  (gr_text Pwr (at 149.225 106.1085 90) (layer F.SilkS))
  (gr_text Boot (at 147.193 106.1085 90) (layer F.SilkS))
  (gr_text PU (at 154.692 102.8791 270) (layer B.SilkS))
  (gr_text U- (at 154.692 100.3391 270) (layer B.SilkS))
  (gr_text LED (at 149.612 102.8791 270) (layer B.SilkS))
  (gr_text U+ (at 149.612 100.3391 270) (layer B.SilkS))
  (gr_text GND (at 145.04 97.7991 270) (layer B.SilkS))
  (gr_text Vin (at 157.232 97.7991 270) (layer B.SilkS))
  (gr_text GND (at 157.232 100.3391 270) (layer B.SilkS))
  (gr_text 3.3v (at 157.232 102.8791 270) (layer B.SilkS))
  (gr_text 30 (at 152.66 113.0391 270) (layer B.SilkS))
  (gr_text 29 (at 152.66 118.1191 270) (layer B.SilkS))
  (gr_text 28 (at 152.66 120.6591 270) (layer B.SilkS))
  (gr_text IO3 (at 152.66 123.1991 270) (layer B.SilkS))
  (gr_text SCK (at 152.66 125.7391 270) (layer B.SilkS))
  (gr_text G (at 152.66 130.8191 270) (layer B.SilkS))
  (gr_text G (at 147.58 130.8191 270) (layer B.SilkS))
  (gr_text 3v (at 152.66 115.5791 270) (layer B.SilkS))
  (gr_text SS (at 147.58 128.2791 270) (layer B.SilkS))
  (gr_text IO1 (at 147.58 125.7391 270) (layer B.SilkS))
  (gr_text IO2 (at 147.58 123.1991 270) (layer B.SilkS))
  (gr_text 27 (at 147.58 120.6591 270) (layer B.SilkS))
  (gr_text 26 (at 147.58 118.1191 270) (layer B.SilkS))
  (gr_text 25 (at 147.58 113.0391 270) (layer B.SilkS))
  (gr_text 1 (at 145.04 100.3391 270) (layer B.SilkS))
  (gr_text 2 (at 145.04 102.8791 270) (layer B.SilkS))
  (gr_text 3 (at 145.04 105.4191 270) (layer B.SilkS))
  (gr_text 4 (at 145.04 107.9591 270) (layer B.SilkS))
  (gr_text 5 (at 145.04 110.4991 270) (layer B.SilkS))
  (gr_text 6 (at 145.04 113.0391 270) (layer B.SilkS))
  (gr_text 7 (at 145.04 115.5791 270) (layer B.SilkS))
  (gr_text 8 (at 145.04 118.1191 270) (layer B.SilkS))
  (gr_text 9 (at 145.04 120.6591 270) (layer B.SilkS))
  (gr_text 10 (at 145.04 123.1991 270) (layer B.SilkS))
  (gr_text 11 (at 145.04 125.7391 270) (layer B.SilkS))
  (gr_text 12 (at 145.04 128.2791 270) (layer B.SilkS))
  (gr_text 13 (at 145.04 130.8191 270) (layer B.SilkS))
  (gr_text 24 (at 157.232 105.4191 270) (layer B.SilkS))
  (gr_text 23 (at 157.232 107.9591 270) (layer B.SilkS))
  (gr_text 22 (at 157.232 110.4991 270) (layer B.SilkS))
  (gr_text 21 (at 157.232 113.0391 270) (layer B.SilkS))
  (gr_text 20 (at 157.232 115.5791 270) (layer B.SilkS))
  (gr_text 19 (at 157.232 118.1191 270) (layer B.SilkS))
  (gr_text 18 (at 157.232 120.6591 270) (layer B.SilkS))
  (gr_text 17 (at 157.232 123.1991 270) (layer B.SilkS))
  (gr_text 16 (at 157.232 125.7391 270) (layer B.SilkS))
  (gr_text 15 (at 157.232 128.2791 270) (layer B.SilkS))
  (gr_text G (at 156.718 100.33) (layer F.SilkS))
  (gr_text "Tiny\nFPGA" (at 146.1262 120.0658) (layer F.SilkS))
  (gr_text Bx (at 149.606 108.458) (layer F.SilkS))
  (gr_text 14 (at 157.232 130.8191 270) (layer B.SilkS))
  (gr_text Vin (at 157.73 97.464) (layer F.SilkS))
  (gr_text 3.3v (at 157.48 102.87) (layer F.SilkS))
  (gr_text 24 (at 157.48 105.156) (layer F.SilkS))
  (gr_text 23 (at 157.48 108.712) (layer F.SilkS))
  (gr_text 22 (at 157.48 110.998) (layer F.SilkS))
  (gr_text 21 (at 157.48 113.03) (layer F.SilkS))
  (gr_text 20 (at 157.48 115.57) (layer F.SilkS))
  (gr_text 19 (at 157.48 118.11) (layer F.SilkS))
  (gr_text 18 (at 157.48 120.65) (layer F.SilkS))
  (gr_text 17 (at 157.48 123.19) (layer F.SilkS))
  (gr_text 16 (at 157.48 125.73) (layer F.SilkS))
  (gr_text 15 (at 157.48 128.27) (layer F.SilkS))
  (gr_text 14 (at 157.48 130.81) (layer F.SilkS))
  (gr_text 13 (at 144.78 130.81) (layer F.SilkS))
  (gr_text 12 (at 144.78 128.27) (layer F.SilkS))
  (gr_text 11 (at 144.78 125.73) (layer F.SilkS))
  (gr_text 10 (at 144.78 123.19) (layer F.SilkS))
  (gr_text 9 (at 144.78 120.65) (layer F.SilkS))
  (gr_text 8 (at 144.78 118.11) (layer F.SilkS))
  (gr_text 7 (at 144.78 115.57) (layer F.SilkS))
  (gr_text 6 (at 144.78 113.03) (layer F.SilkS))
  (gr_text 5 (at 144.78 110.49) (layer F.SilkS))
  (gr_text 4 (at 144.78 107.95) (layer F.SilkS))
  (gr_text 3 (at 144.78 105.41) (layer F.SilkS))
  (gr_text 2 (at 144.78 102.87) (layer F.SilkS))
  (gr_text 1 (at 144.78 100.33) (layer F.SilkS))
  (gr_text G (at 144.78 97.79) (layer F.SilkS))
  (gr_line (start 142.246 132.0891) (end 142.246 96.5291) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.026 132.0891) (end 142.246 132.0891) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.026 96.5291) (end 160.026 132.0891) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.246 96.5291) (end 160.026 96.5291) (layer Edge.Cuts) (width 0.15))
  (zone (net 36) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 142.621 96.8375) (xy 159.639 96.8375) (xy 159.639 131.826) (xy 142.621 131.826)
      )
    )
  )
  (zone (net 37) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 159.639 116.332) (xy 159.639 131.826) (xy 142.621 131.826) (xy 142.621 96.8375) (xy 159.639 96.8375)
      )
    )
    (polygon
      (pts        (xy 154.1145 108.712) (xy 154.1145 112.776) (xy 153.162 112.776) (xy 153.162 112.014) (xy 148.336 112.014)
        (xy 148.336 116.332) (xy 151.003 116.332) (xy 151.003 121.539) (xy 153.67 121.539) (xy 153.67 116.332)
        (xy 156.0195 116.332) (xy 156.0195 108.712)
      )
    )
  )
  (zone (net 31) (net_name +1V2) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 155.7655 108.966) (xy 154.3685 108.966) (xy 154.3685 113.03) (xy 152.908 113.03) (xy 152.908 112.268)
        (xy 148.59 112.268) (xy 148.59 116.078) (xy 151.257 116.078) (xy 151.257 121.285) (xy 153.416 121.285)
        (xy 153.416 116.078) (xy 155.7655 116.078)
      )
    )
  )
)
