(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 20)
    (no_connects 1)
    (area 45.644999 34.214999 71.195001 59.765001)
    (thickness 1.6)
    (drawings 34)
    (tracks 97)
    (zones 0)
    (modules 3)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 GND)
  (net 3 IINT)
  (net 4 GPIO9)
  (net 5 GPIO8)
  (net 6 GPIO7)
  (net 7 GPIO6)
  (net 8 SCL)
  (net 9 VIN)
  (net 10 VCC_SYSTEM)
  (net 11 SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GPIO6)
    (add_net GPIO7)
    (add_net GPIO8)
    (add_net GPIO9)
    (add_net IINT)
    (add_net "Net-(P1-Pad1)")
    (add_net SCL)
    (add_net SDA)
    (add_net VCC_SYSTEM)
    (add_net VIN)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 52.07 55.88)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 IINT))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 VCC_SYSTEM))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 SDA))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 SCL))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module KiCAD_EXAMPLE:boardConnector_back (layer F.Cu) (tedit 57CF4177)
    (at 68.58 46.99 270)
    (fp_text reference J2 (at -5.08 -3.81 270) (layer F.SilkS))
    (fp_text value connector (at -2.54 -5.08 270) (layer F.Fab))
    (pad 10 smd rect (at -4 -0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 3 IINT))
    (pad 9 smd rect (at -2 -0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 4 GPIO9))
    (pad 8 smd rect (at 0 -0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 5 GPIO8))
    (pad 7 smd rect (at 2 -0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 6 GPIO7))
    (pad 6 smd rect (at 4 -0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 7 GPIO6))
    (pad 5 smd rect (at -4 -0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (pad 4 smd rect (at -2 -0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 11 SDA))
    (pad 1 smd rect (at 4 -0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC_SYSTEM))
    (pad 2 smd rect (at 2 -0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 9 VIN))
    (pad 3 smd rect (at 0 -0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCAD_EXAMPLE:BoardConnectorFront (layer F.Cu) (tedit 57CF422B)
    (at 48.26 46.99 270)
    (fp_text reference J1 (at -1.27 -6.35 270) (layer F.SilkS))
    (fp_text value connector (at -8.89 -3.81 270) (layer F.Fab))
    (pad 10 smd rect (at -4 0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 3 IINT))
    (pad 9 smd rect (at -2 0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 4 GPIO9))
    (pad 8 smd rect (at 0 0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 5 GPIO8))
    (pad 7 smd rect (at 2 0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 6 GPIO7))
    (pad 6 smd rect (at 4 0.4 270) (size 1 3.4) (layers B.Cu B.Paste B.Mask)
      (net 7 GPIO6))
    (pad 3 smd rect (at 0 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 9 VIN))
    (pad 1 smd rect (at 4 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC_SYSTEM))
    (pad 4 smd rect (at -2 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 11 SDA))
    (pad 5 smd rect (at -4 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (pad 5 smd rect (at -4 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (pad 4 smd rect (at -2 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 11 SDA))
    (pad 1 smd rect (at 4 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC_SYSTEM))
    (pad 2 smd rect (at 2 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 9 VIN))
    (pad 3 smd rect (at 0 0.4 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_text "KICAD EXAMPLE BREAKOUT" (at 58.42 36.83) (layer F.SilkS))
  (gr_text NC (at 52.07 58.42 90) (layer F.SilkS))
  (gr_text "INT\n" (at 54.61 58.42 90) (layer F.SilkS))
  (gr_text "GND\n" (at 57.15 58.42 90) (layer F.SilkS))
  (gr_text "VCC\n" (at 59.69 58.42 90) (layer F.SilkS))
  (gr_text "SDA\n" (at 62.23 58.42 90) (layer F.SilkS))
  (gr_text SCL (at 64.77 58.42 90) (layer F.SilkS))
  (dimension 2.54 (width 0.3) (layer Eco1.User)
    (gr_text "0.1000 in" (at 89.488 58.42 270) (layer Eco1.User))
    (feature1 (pts (xy 72.39 59.69) (xy 90.838 59.69)))
    (feature2 (pts (xy 72.39 57.15) (xy 90.838 57.15)))
    (crossbar (pts (xy 88.138 57.15) (xy 88.138 59.69)))
    (arrow1a (pts (xy 88.138 59.69) (xy 87.551579 58.563496)))
    (arrow1b (pts (xy 88.138 59.69) (xy 88.724421 58.563496)))
    (arrow2a (pts (xy 88.138 57.15) (xy 87.551579 58.276504)))
    (arrow2b (pts (xy 88.138 57.15) (xy 88.724421 58.276504)))
  )
  (dimension 25.4 (width 0.3) (layer Eco1.User)
    (gr_text "1.0000 in" (at 58.42 27.352) (layer Eco1.User))
    (feature1 (pts (xy 71.12 33.02) (xy 71.12 26.002)))
    (feature2 (pts (xy 45.72 33.02) (xy 45.72 26.002)))
    (crossbar (pts (xy 45.72 28.702) (xy 71.12 28.702)))
    (arrow1a (pts (xy 71.12 28.702) (xy 69.993496 29.288421)))
    (arrow1b (pts (xy 71.12 28.702) (xy 69.993496 28.115579)))
    (arrow2a (pts (xy 45.72 28.702) (xy 46.846504 29.288421)))
    (arrow2b (pts (xy 45.72 28.702) (xy 46.846504 28.115579)))
  )
  (dimension 25.4 (width 0.3) (layer Eco1.User)
    (gr_text "1.0000 in" (at 32.686 46.99 90) (layer Eco1.User))
    (feature1 (pts (xy 41.402 34.29) (xy 31.336 34.29)))
    (feature2 (pts (xy 41.402 59.69) (xy 31.336 59.69)))
    (crossbar (pts (xy 34.036 59.69) (xy 34.036 34.29)))
    (arrow1a (pts (xy 34.036 34.29) (xy 34.622421 35.416504)))
    (arrow1b (pts (xy 34.036 34.29) (xy 33.449579 35.416504)))
    (arrow2a (pts (xy 34.036 59.69) (xy 34.622421 58.563496)))
    (arrow2b (pts (xy 34.036 59.69) (xy 33.449579 58.563496)))
  )
  (gr_line (start 68.072 48.514) (end 68.326 48.514) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.12 48.514) (end 68.072 48.514) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.12 59.69) (end 71.12 48.514) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 45.72 59.69) (end 71.12 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 45.72 48.514) (end 45.72 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.768 48.514) (end 45.72 48.514) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 48.768 48.006) (end 49.276 48.006) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 48.768 48.006) (end 48.768 47.498) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 45.72 47.498) (end 48.768 47.498) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 45.72 34.29) (end 45.72 47.498) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.12 34.29) (end 45.72 34.29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.12 47.498) (end 71.12 34.29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.072 47.498) (end 71.12 47.498) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 68.072 48.006) (end 67.564 48.006) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 68.072 48.006) (end 68.072 48.514) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 2.54 (width 0.3) (layer Eco1.User)
    (gr_text "2.540 mm" (at 83.9 58.42 90) (layer Eco1.User))
    (feature1 (pts (xy 71.12 57.15) (xy 85.25 57.15)))
    (feature2 (pts (xy 71.12 59.69) (xy 85.25 59.69)))
    (crossbar (pts (xy 82.55 59.69) (xy 82.55 57.15)))
    (arrow1a (pts (xy 82.55 57.15) (xy 83.136421 58.276504)))
    (arrow1b (pts (xy 82.55 57.15) (xy 81.963579 58.276504)))
    (arrow2a (pts (xy 82.55 59.69) (xy 83.136421 58.563496)))
    (arrow2b (pts (xy 82.55 59.69) (xy 81.963579 58.563496)))
  )
  (dimension 25.4 (width 0.3) (layer Eco1.User)
    (gr_text "25.400 mm" (at 38.02 46.99 270) (layer Eco1.User))
    (feature1 (pts (xy 45.72 59.69) (xy 36.67 59.69)))
    (feature2 (pts (xy 45.72 34.29) (xy 36.67 34.29)))
    (crossbar (pts (xy 39.37 34.29) (xy 39.37 59.69)))
    (arrow1a (pts (xy 39.37 59.69) (xy 38.783579 58.563496)))
    (arrow1b (pts (xy 39.37 59.69) (xy 39.956421 58.563496)))
    (arrow2a (pts (xy 39.37 34.29) (xy 38.783579 35.416504)))
    (arrow2b (pts (xy 39.37 34.29) (xy 39.956421 35.416504)))
  )
  (dimension 25.4 (width 0.3) (layer Eco1.User)
    (gr_text "25.400 mm" (at 58.42 33.099999) (layer Eco1.User))
    (feature1 (pts (xy 71.12 27.94) (xy 71.12 34.449999)))
    (feature2 (pts (xy 45.72 27.94) (xy 45.72 34.449999)))
    (crossbar (pts (xy 45.72 31.749999) (xy 71.12 31.749999)))
    (arrow1a (pts (xy 71.12 31.749999) (xy 69.993496 32.33642)))
    (arrow1b (pts (xy 71.12 31.749999) (xy 69.993496 31.163578)))
    (arrow2a (pts (xy 45.72 31.749999) (xy 46.846504 32.33642)))
    (arrow2b (pts (xy 45.72 31.749999) (xy 46.846504 31.163578)))
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.866 41.402) (xy 66.294 41.402) (xy 66.294 52.578) (xy 70.866 52.578) (xy 70.866 59.436)
        (xy 45.974 59.436) (xy 45.974 52.578) (xy 50.546 52.578) (xy 50.546 41.148) (xy 45.974 41.148)
        (xy 45.974 34.544) (xy 70.866 34.544)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.866 41.402) (xy 66.294 41.402) (xy 66.294 52.578) (xy 70.866 52.578) (xy 70.866 59.436)
        (xy 45.974 59.436) (xy 45.974 52.578) (xy 50.546 52.578) (xy 50.546 41.148) (xy 45.974 41.148)
        (xy 45.974 34.544) (xy 70.866 34.544)
      )
    )
  )
)
