(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(Cdelay1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(Ctantalumbypass1-Pad1)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(Rfreq1-Pad1)")
  (net 6 "Net-(U3-Pad1)")
  (net 7 "Net-(U2-Pad8)")
  (net 8 "Net-(Rpwm1-Pad1)")
  (net 9 "Net-(Cdelay2-Pad1)")
  (net 10 "Net-(J1-Pad6)")
  (net 11 "Net-(J1-Pad7)")
  (net 12 "Net-(Rfreq2-Pad1)")
  (net 13 "Net-(Rlimiting2-Pad2)")
  (net 14 "Net-(Rpulldown2-Pad1)")
  (net 15 "Net-(Rpwm2-Pad1)")
  (net 16 "Net-(J1-Pad4)")
  (net 17 "unconnected-(U2-Pad7)")
  (net 18 "unconnected-(U4-Pad7)")
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 216.8 91.9 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cdelay1" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100 nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "Net-(Cdelay1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-8-3.5-H_1x08_P3.50mm_Horizontal" (layer "F.Cu")
    (tedit 5B294F44)
    (at 216.05 113.9 180)
    (descr "Terminal Block Phoenix PT-1,5-8-3.5-H, 8 pins, pitch 3.5mm, size 28x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-8-3.5-H pitch 3.5mm size 28x7.6mm^2 drill 1.2mm pad 2.4mm")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 12.25 -4.16 180) (layer "F.SilkS") hide)
    (fp_text value "Screw_Terminal_01x08" (at 12.25 5.56 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.25 2.4 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 10.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 14 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 17.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 21 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 24.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-8-3.5-H_1x08_P3.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drv103:DRV103U" (layer "F.Cu")
    (tedit 0)
    (at 215.16505 98.4 -90)
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 0 -270) (layer "F.SilkS") hide)
    (fp_text value "DRV103U" (at 0 3.8 -270) (layer "F.SilkS") hide)
    (fp_text user ".022in/.559mm" (at 5.5118 -1.905 -270) (layer "Cmts.User"))
    (fp_text user ".194in/4.928mm" (at 0 -4.9149 -270) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 -270) (layer "Cmts.User"))
    (fp_text user ".078in/1.981mm" (at -2.4638 4.9149 -270) (layer "Cmts.User"))
    (fp_text user ".05in/1.27mm" (at -5.5118 -1.27 -270) (layer "Cmts.User"))
    (fp_text user "*" (at -2.7178 -3.6068 -270) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 -270) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(Rpwm1-Pad1)") (pinfunction "DUTYCYCLEADJ") (pintype "input"))
    (pad "2" smd rect (at -2.4638 -0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(Cdelay1-Pad1)") (pinfunction "DELAYADJ") (pintype "output"))
    (pad "3" smd rect (at -2.4638 0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(Rfreq1-Pad1)") (pinfunction "OSCFREQADJ") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-Pad3)") (pinfunction "OUT") (pintype "output"))
    (pad "6" smd rect (at 2.4638 0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "VS+") (pintype "power_in"))
    (pad "7" smd rect (at 2.4638 -0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(U2-Pad7)") (pinfunction "STATUSOKFLAG") (pintype "unspecified"))
    (pad "8" smd rect (at 2.4638 -1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(U2-Pad8)") (pinfunction "INPUT") (pintype "input"))
    (pad "9" thru_hole roundrect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 216.1 104.8)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Ctantalumbypass1" (at 0 -1.85) (layer "F.SilkS") hide)
    (fp_text value "22 uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.4 98.3)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rpullup1" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "R2.2k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(U3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 191.9 92.1 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rfreq2" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text value "R205k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 12 "Net-(Rfreq2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 185.5 113.5)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 221.5 96.1)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rpulldown1" (at 0 -1.82) (layer "F.SilkS") hide)
    (fp_text value "R4.7k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "Net-(U2-Pad8)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "diode:CDBA360-G" (layer "F.Cu")
    (tedit 0)
    (at 222.3982 119.5 180)
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Uflyback1" (at 0.5982 -2.7) (layer "F.SilkS") hide)
    (fp_text value "CDBA360-G" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (pad "1" smd rect (at -1.7018 0 270) (size 1.651 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at 1.7018 0 270) (size 1.651 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-Pad3)") (pinfunction "2") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 200.4 98.6 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SIGINV2" (at 0 1.9) (layer "F.SilkS"))
    (fp_text value "9999999999999999" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(J1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(Rpulldown2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 221.5 100 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SIGINV1" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "9999999999999999" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "Net-(U2-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.4 107.8)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rlimiting2" (at 0 -1.82) (layer "F.SilkS") hide)
    (fp_text value "R10k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(J1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(Rlimiting2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "transistor:BC857B-7-F" (layer "F.Cu")
    (tedit 0)
    (at 208.4 102.6)
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -2.755 -0.5) (layer "F.SilkS") hide)
    (fp_text value "BC857B-7-F" (at 0 3.412) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0 3.412) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 3.412) (layer "Cmts.User"))
    (fp_text user "*" (at 0 3.412) (layer "F.Fab"))
    (pad "1" smd rect (at -1.024999 0.944999) (size 0.8128 0.889) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(U3-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect (at 1.024999 0.944999) (size 0.8128 0.889) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect (at 0 -0.945) (size 0.8128 0.889) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(U2-Pad8)") (pinfunction "C") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.4 104.9)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rpullup2" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "R2.2k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(J1-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 208.4 106.6 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rlimiting1" (at 0 -1.82) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(U3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 221.5 93.3)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rpwm1" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "R95.3k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 8 "Net-(Rpwm1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "transistor:BC857B-7-F" (layer "F.Cu")
    (tedit 0)
    (at 200.9 106.1)
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 2.855 0.1) (layer "F.SilkS") hide)
    (fp_text value "BC857B-7-F" (at 0 3.412) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0 3.412) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 3.412) (layer "Cmts.User"))
    (fp_text user "*" (at 0 3.412) (layer "F.Fab"))
    (pad "1" smd rect (at -1.024999 0.944999) (size 0.8128 0.889) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(Rlimiting2-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect (at 1.024999 0.944999) (size 0.8128 0.889) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect (at 0 -0.945) (size 0.8128 0.889) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(Rpulldown2-Pad1)") (pinfunction "C") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 195.8 92.1 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cdelay2" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text value "100 nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 9 "Net-(Cdelay2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 222.1 113.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 213.2 91.9 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rfreq1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R205k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(Rfreq1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 200.4 93.3)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rpwm2" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text value "R95.3k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 15 "Net-(Rpwm2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 200.4 101.1)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rpulldown2" (at 0 -1.82) (layer "F.SilkS") hide)
    (fp_text value "R4.7k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(Rpulldown2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "diode:CDBA360-G" (layer "F.Cu")
    (tedit 0)
    (at 185.5 119.6 180)
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Uflyback2" (at 0.2982 2.5) (layer "F.SilkS") hide)
    (fp_text value "CDBA360-G" (at 9.8982 0.8) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (pad "1" smd rect (at -1.7018 0 270) (size 1.651 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at 1.7018 0 270) (size 1.651 2.1844) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(J1-Pad6)") (pinfunction "2") (pintype "unspecified"))
  )
  (footprint "drv103:DRV103U" (layer "F.Cu")
    (tedit 0)
    (at 194.16505 98.6 -90)
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0 0 -270) (layer "F.SilkS") hide)
    (fp_text value "DRV103U" (at 0 3.788 -270) (layer "F.SilkS") hide)
    (fp_text user ".022in/.559mm" (at 5.5118 -1.905 -270) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 -270) (layer "Cmts.User"))
    (fp_text user ".05in/1.27mm" (at -5.5118 -1.27 -270) (layer "Cmts.User"))
    (fp_text user ".194in/4.928mm" (at 0 -4.9149 -270) (layer "Cmts.User"))
    (fp_text user ".078in/1.981mm" (at -2.4638 4.9149 -270) (layer "Cmts.User"))
    (fp_text user "*" (at -2.7178 -3.6068 -270) (layer "F.Fab"))
    (fp_text user "*" (at -2.7178 -3.6068 -270) (layer "F.Fab"))
    (pad "1" smd rect (at -2.4638 -1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(Rpwm2-Pad1)") (pinfunction "DUTYCYCLEADJ") (pintype "input"))
    (pad "2" smd rect (at -2.4638 -0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(Cdelay2-Pad1)") (pinfunction "DELAYADJ") (pintype "output"))
    (pad "3" smd rect (at -2.4638 0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(Rfreq2-Pad1)") (pinfunction "OSCFREQADJ") (pintype "input"))
    (pad "4" smd rect (at -2.4638 1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.4638 1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(J1-Pad6)") (pinfunction "OUT") (pintype "output"))
    (pad "6" smd rect (at 2.4638 0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pinfunction "VS+") (pintype "power_in"))
    (pad "7" smd rect (at 2.4638 -0.635 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(U4-Pad7)") (pinfunction "STATUSOKFLAG") (pintype "unspecified"))
    (pad "8" smd rect (at 2.4638 -1.905 270) (size 1.9812 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(Rpulldown2-Pad1)") (pinfunction "INPUT") (pintype "input"))
    (pad "9" thru_hole roundrect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 194.2 104.8 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "drv103 pwm economizer.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Ctantalumbypass2" (at 0 -1.85) (layer "F.SilkS") hide)
    (fp_text value "22 uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "Net-(Ctantalumbypass1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 182 121.7) (end 226 89.1) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "12V+\nCC1+\nCC1-\nCC1S\nCC2+\nCC2-\nCC2S\nGND" (at 203.8 121.7 -90) (layer "F.SilkS"))
  (gr_text "RB DESIGNS \nPWM ECONOMIZER\nREV 1.2" (at 185.2 100.9 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.9 121.6)
        (xy 182.1 121.6)
        (xy 182.1 89.2)
        (xy 225.9 89.2)
      )
    )
  )
)
