<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="8.89" y1="26.416" x2="33.302" y2="26.416" width="0" layer="20"/>
<wire x1="33.302" y1="26.416" x2="33.302" y2="50" width="0" layer="20"/>
<wire x1="33.302" y1="50" x2="8.89" y2="50" width="0" layer="20"/>
<wire x1="8.89" y1="50" x2="8.89" y2="26.416" width="0" layer="20"/>
<text>Miny85LEDC 0.2</text>
<text>1</text>
<text>+</text>
<text>GND</text>
<text>LED</text>
<text>VCC</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-tact">
<description>&lt;b&gt;Diptronics THMD &amp; SMD tact switches&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;DTS-3: 3.5x6mm THMD tact switch
&lt;li&gt;DTS-6, DTS-64: 6x6mm THMD tact switch
&lt;li&gt;DTSM-3: 3.5x6mm SMD tact switch
&lt;li&gt;DTSM-6, DTSM-64: 6x6mm SMD tact switch
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DTS-3">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P762X533-8">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
</packages>
</library>
<library name="ZZFlowerpad">
<packages>
<package name="FLOWERPIN">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP3" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-tact" package="DTS-3" value="DTS-3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP10" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP5" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP6" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP27" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP32" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP37" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP40" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP42" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP43" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP50" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP53" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP54" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP60" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="TP75" library="ZZFlowerpad" package="FLOWERPIN" value="FLOWERPIN"/>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-8" value="ATTINY85-20PU">
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="OC_NEWARK" value="58M3796"/>
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="switch-tact" package="DTS-3" value="DTS-3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+3.3V">
<contactref element="JP3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="TP50" pad="P$1"/>
<contactref element="CN1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP3" pad="6"/>
<contactref element="S1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="TP53" pad="P$1"/>
<contactref element="CN1" pad="2"/>
</signal>
<signal name="JP2">
<contactref element="JP3" pad="5"/>
<contactref element="S1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="JP3" pad="4"/>
<contactref element="U1" pad="5"/>
<contactref element="TP40" pad="P$1"/>
</signal>
<signal name="N$18">
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="N$17">
</signal>
<signal name="N$5">
</signal>
<signal name="N$12">
</signal>
<signal name="N$16">
</signal>
<signal name="N$37">
</signal>
<signal name="N$53">
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$79">
</signal>
<signal name="N$1">
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP3" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="S2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="U1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
