<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="100" y1="38.2" x2="100" y2="3.81" width="0.254" layer="20"/>
<wire x1="100" y1="3.81" x2="99.06" y2="1.27" width="0.254" layer="20"/>
<wire x1="99.06" y1="1.27" x2="99.06" y2="1" width="0.254" layer="20"/>
<wire x1="99.06" y1="1" x2="98.06" y2="0" width="0.254" layer="20" curve="-90"/>
<wire x1="98.06" y1="0" x2="1" y2="0" width="0.254" layer="20"/>
<wire x1="1" y1="0" x2="0" y2="1" width="0.254" layer="20" curve="-90"/>
<wire x1="0" y1="1" x2="0" y2="52.3" width="0.254" layer="20"/>
<text>ADDRESS</text>
<text>AREF</text>
<text>GND</text>
<text>TX0</text>
<text>RX0</text>
<text>RESET</text>
<text>3V</text>
<text>5V</text>
<text>VI</text>
<text>/WRAM</text>
<text>REFSH</text>
<text>EXPD</text>
<text>/CS</text>
<text>/IRQ</text>
<text>/WR</text>
<text>/RD</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>SDA</text>
<text>SCL</text>
<text>A8</text>
<text>A9</text>
<text>A10</text>
<text>A11</text>
<text>A12</text>
<text>A13</text>
<text>A14</text>
<text>A15</text>
<text>RESET</text>
<text>/PARD</text>
<text>/PAWR</text>
<text>GND</text>
<text>P0</text>
<text>P2</text>
<text>P4</text>
<text>P6</text>
<text>D7</text>
<text>D5</text>
<text>D3</text>
<text>D1</text>
<text>BTN</text>
<text>CIC</text>
<text>B7</text>
<text>B5</text>
<text>B3</text>
<text>B1</text>
<text>BANK</text>
<text>IOREF</text>
<text>SDA</text>
<text>SCL</text>
<wire x1="1" y1="53.3" x2="0" y2="52.3" width="0.254" layer="20" curve="90"/>
<text>DATA</text>
<text>SD</text>
<text>G</text>
<text>G</text>
<text>5V</text>
<text>CLK
EXP
PA6
PAR


GND
A11
A10
A9
A8
A7
A6
A5
A4
A3
A2
A1
A0
IRQ
D0
D1
D2
D3
RD
CIC1
RIN
RESET
VCC


PA0
PA2
PA4
LAUD</text>
<text>WRM
REF
PA7
PAW


GND
A12
A13
A14
A15
BA0
BA1
BA2
BA3
BA4
BA5
BA6
BA7
CS
D4
D5
D6
D7
WR
CIC2
CICCLK
CPUCLK
VCC


PA1
PA3
PA5
RAUD</text>
<text>5V</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>CLK2</text>
<text>CLK1</text>
<text>CLK0</text>
<wire x1="96.6" y1="53.3" x2="99" y2="50.9" width="0.254" layer="20"/>
<wire x1="99" y1="50.9" x2="99" y2="40.6" width="0.254" layer="20"/>
<wire x1="99" y1="40.6" x2="100" y2="38.2" width="0.254" layer="20"/>
<text>FLASH</text>
<text>CLK1</text>
<text>RX1</text>
<text>TX1</text>
<text>VCC</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>MISO</text>
<text>SCK</text>
<text>MOSI</text>
<text>CS</text>
<text>5V</text>
<wire x1="1" y1="53.3" x2="96.6" y2="53.3" width="0.254" layer="20"/>
<text>CPUCLK</text>
<text>Red</text>
<text>Green</text>
<text>Blue</text>
<text>CA</text>
<text>PA</text>
<text>38</text>
<text>41</text>
<text>40</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>20</text>
<text>21</text>
<text>22</text>
<text>24</text>
<text>26</text>
<text>28</text>
<text>30</text>
<text>32</text>
<text>34</text>
<text>36</text>
<text>38</text>
<text>40</text>
<text>42</text>
<text>44</text>
<text>46</text>
<text>50</text>
<text>48</text>
<text>52</text>
<text>LED</text>
<text>5V
CLK
ROH
RIN</text>
<text>GND
CIC0
CIC1
R0S</text>
<text>FLA</text>
<text>SNES CART READER SHIELD</text>
<text>CLOCK</text>
</plain>
<libraries>
<library name="SmartPrj">
<packages>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X18">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="snes_div">
<packages>
<package name="PIC12F629">
</package>
</packages>
</library>
<library name="pinhead2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED5MMRGB">
</package>
<package name="1X04-BIG">
</package>
<package name="1X04-CLEANBIG">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="snes_div_mod">
<packages>
<package name="SNESCART_CONN">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
</packages>
</library>
<library name="!sanni">
<packages>
<package name="1X03-CLEANBIG">
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PWML" library="SmartPrj" package="1X08" value="8x1F-H8.5"/>
<element name="ADCL" library="SmartPrj" package="1X08" value="8x1F-H8.5"/>
<element name="COMMUNICATION" library="SmartPrj" package="1X08" value="8x1F-H8.5"/>
<element name="ADCH" library="SmartPrj" package="1X08" value="8x1F-H8.5"/>
<element name="XIO" library="SmartPrj" package="2X18" value="18x2F-H8.5"/>
<element name="PINS" library="SmartPrj" package="1X10" value="10x1F-H8.5"/>
<element name="POWER" library="SmartPrj" package="1X08" value="8x1F-H8.5">
<attribute name="NAME"/>
</element>
<element name="SDCARD" library="pinhead2" package="2X08" value="">
<attribute name="VALUE"/>
</element>
<element name="BUTTON" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="10K" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CA_RGB_LED" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM"/>
<element name="220R" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="220R1" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="220R2" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="I2CCLOCKGEN" library="pinhead2" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ_2" value="">
<attribute name="VALUE"/>
</element>
<element name="CIC" library="snes_div" package="PIC12F629" value="PIC12F629_SIMPLE">
<attribute name="NAME"/>
</element>
<element name="SERIAL2" library="pinhead2" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="snes_div_mod" package="SNESCART_CONN" value="SNESCART_CONN"/>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL-KIT" value="">
<attribute name="PROD_ID" value="CAP-08370"/>
</element>
<element name="LCD" library="adafruit" package="1X04-BIG" value="1X4-BIG">
<attribute name="NAME"/>
</element>
<element name="CN1" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN2" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN3" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN4" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN5" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN6" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN7" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN9" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN10" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN11" library="adafruit" package="1X04-CLEANBIG" value="1X4-CLEANBIG"/>
<element name="CN8" library="!sanni" package="1X03-CLEANBIG" value="1X3-CLEANBIG"/>
<element name="CN13" library="!sanni" package="1X03-CLEANBIG" value="1X3-CLEANBIG"/>
<element name="CN14" library="!sanni" package="1X03-CLEANBIG" value="1X3-CLEANBIG"/>
<element name="CN15" library="!sanni" package="1X03-CLEANBIG" value="1X3-CLEANBIG"/>
<element name="5V" library="!sanni" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="!sanni" package="SJ" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="PINS" pad="4"/>
<contactref element="XIO" pad="36"/>
<contactref element="POWER" pad="6"/>
<contactref element="SDCARD" pad="1"/>
<contactref element="SDCARD" pad="2"/>
<contactref element="SDCARD" pad="15"/>
<contactref element="SDCARD" pad="16"/>
<contactref element="BUTTON" pad="3"/>
<contactref element="I2CCLOCKGEN" pad="2"/>
<contactref element="CIC" pad="8"/>
<contactref element="POWER" pad="7"/>
<contactref element="XIO" pad="35"/>
<contactref element="U$1" pad="84"/>
<contactref element="U$1" pad="36"/>
<contactref element="U$1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="LCD" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="PINS" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="POWER" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="POWER" pad="8"/>
</signal>
<signal name="ADC0">
<contactref element="ADCL" pad="1"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="ADC2">
<contactref element="ADCL" pad="3"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="ADC1">
<contactref element="ADCL" pad="2"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="ADC3">
<contactref element="ADCL" pad="4"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="ADC4">
<contactref element="ADCL" pad="5"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="ADC5">
<contactref element="ADCL" pad="6"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="ADC6">
<contactref element="ADCL" pad="7"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="ADC7">
<contactref element="ADCL" pad="8"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="+3V3">
<contactref element="POWER" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="COMMUNICATION" pad="2"/>
<contactref element="PINS" pad="2"/>
<contactref element="I2CCLOCKGEN" pad="3"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="COMMUNICATION" pad="1"/>
<contactref element="PINS" pad="1"/>
<contactref element="I2CCLOCKGEN" pad="4"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="ADC9">
<contactref element="ADCH" pad="2"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="ADC8">
<contactref element="ADCH" pad="1"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="ADC10">
<contactref element="ADCH" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="ADC11">
<contactref element="ADCH" pad="4"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="ADC12">
<contactref element="ADCH" pad="5"/>
<contactref element="U$1" pad="85"/>
<contactref element="U$1" pad="37"/>
</signal>
<signal name="ADC13">
<contactref element="ADCH" pad="6"/>
<contactref element="U$1" pad="80"/>
<contactref element="U$1" pad="38"/>
</signal>
<signal name="ADC14">
<contactref element="ADCH" pad="7"/>
<contactref element="U$1" pad="79"/>
<contactref element="U$1" pad="39"/>
</signal>
<signal name="ADC15">
<contactref element="ADCH" pad="8"/>
<contactref element="U$1" pad="78"/>
<contactref element="U$1" pad="40"/>
</signal>
<signal name="PB3">
<contactref element="XIO" pad="31"/>
<contactref element="SDCARD" pad="13"/>
<contactref element="SDCARD" pad="14"/>
</signal>
<signal name="PB2">
<contactref element="XIO" pad="32"/>
<contactref element="SDCARD" pad="9"/>
<contactref element="SDCARD" pad="10"/>
</signal>
<signal name="PB1">
<contactref element="XIO" pad="33"/>
<contactref element="SDCARD" pad="11"/>
<contactref element="SDCARD" pad="12"/>
</signal>
<signal name="PB5">
<contactref element="PINS" pad="7"/>
<contactref element="220R1" pad="P$1"/>
</signal>
<signal name="PB4">
<contactref element="PINS" pad="8"/>
<contactref element="220R" pad="P$1"/>
</signal>
<signal name="PE5">
<contactref element="PWML" pad="4"/>
<contactref element="U$1" pad="88"/>
<contactref element="U$1" pad="33"/>
</signal>
<signal name="PE4">
<contactref element="PWML" pad="3"/>
<contactref element="U$1" pad="89"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="PE3">
<contactref element="PWML" pad="6"/>
</signal>
<signal name="PE1">
<contactref element="PWML" pad="2"/>
</signal>
<signal name="PE0">
<contactref element="PWML" pad="1"/>
</signal>
<signal name="PB6">
<contactref element="PINS" pad="6"/>
<contactref element="220R2" pad="P$1"/>
</signal>
<signal name="PH3">
<contactref element="PWML" pad="7"/>
<contactref element="U$1" pad="69"/>
<contactref element="U$1" pad="49"/>
</signal>
<signal name="PH4">
<contactref element="PWML" pad="8"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="PH5">
<contactref element="PINS" pad="10"/>
<contactref element="U$1" pad="74"/>
<contactref element="U$1" pad="54"/>
</signal>
<signal name="PH6">
<contactref element="PINS" pad="9"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="PG5">
<contactref element="PWML" pad="5"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="RXD1">
<contactref element="COMMUNICATION" pad="3"/>
<contactref element="SERIAL2" pad="2"/>
</signal>
<signal name="TXD1">
<contactref element="COMMUNICATION" pad="4"/>
<contactref element="SERIAL2" pad="1"/>
</signal>
<signal name="PJ0">
<contactref element="COMMUNICATION" pad="7"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="PH1">
<contactref element="COMMUNICATION" pad="6"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="PJ1">
<contactref element="COMMUNICATION" pad="8"/>
<contactref element="U$1" pad="86"/>
<contactref element="U$1" pad="35"/>
</signal>
<signal name="PC0">
<contactref element="XIO" pad="18"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="PC1">
<contactref element="XIO" pad="17"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="PC2">
<contactref element="XIO" pad="16"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="PC3">
<contactref element="XIO" pad="15"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="PC4">
<contactref element="XIO" pad="14"/>
<contactref element="U$1" pad="50"/>
<contactref element="U$1" pad="70"/>
</signal>
<signal name="PC5">
<contactref element="XIO" pad="13"/>
<contactref element="U$1" pad="51"/>
<contactref element="U$1" pad="71"/>
</signal>
<signal name="PC6">
<contactref element="XIO" pad="12"/>
<contactref element="U$1" pad="72"/>
<contactref element="U$1" pad="52"/>
</signal>
<signal name="PC7">
<contactref element="XIO" pad="11"/>
<contactref element="U$1" pad="53"/>
<contactref element="U$1" pad="73"/>
</signal>
<signal name="PB0">
<contactref element="XIO" pad="34"/>
<contactref element="SDCARD" pad="7"/>
<contactref element="SDCARD" pad="8"/>
</signal>
<signal name="PG0">
<contactref element="XIO" pad="22"/>
<contactref element="CIC" pad="3"/>
</signal>
<signal name="PG1">
<contactref element="XIO" pad="21"/>
<contactref element="CIC" pad="4"/>
</signal>
<signal name="PG2">
<contactref element="XIO" pad="20"/>
</signal>
<signal name="PD7">
<contactref element="XIO" pad="19"/>
<contactref element="BUTTON" pad="1"/>
<contactref element="10K" pad="P$1"/>
</signal>
<signal name="PA0">
<contactref element="XIO" pad="3"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="PA1">
<contactref element="XIO" pad="4"/>
<contactref element="U$1" pad="59"/>
<contactref element="U$1" pad="90"/>
</signal>
<signal name="PA2">
<contactref element="XIO" pad="5"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="PA3">
<contactref element="XIO" pad="6"/>
<contactref element="U$1" pad="91"/>
<contactref element="U$1" pad="60"/>
</signal>
<signal name="PA4">
<contactref element="XIO" pad="7"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="PA5">
<contactref element="XIO" pad="8"/>
<contactref element="U$1" pad="61"/>
<contactref element="U$1" pad="92"/>
</signal>
<signal name="PA6">
<contactref element="XIO" pad="9"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="PA7">
<contactref element="XIO" pad="10"/>
<contactref element="U$1" pad="87"/>
<contactref element="U$1" pad="34"/>
</signal>
<signal name="PL0">
<contactref element="XIO" pad="30"/>
<contactref element="U$1" pad="77"/>
<contactref element="U$1" pad="41"/>
</signal>
<signal name="PL1">
<contactref element="XIO" pad="29"/>
<contactref element="U$1" pad="42"/>
<contactref element="U$1" pad="76"/>
</signal>
<signal name="PL2">
<contactref element="XIO" pad="28"/>
<contactref element="U$1" pad="67"/>
<contactref element="U$1" pad="43"/>
</signal>
<signal name="PL3">
<contactref element="XIO" pad="27"/>
<contactref element="U$1" pad="66"/>
<contactref element="U$1" pad="44"/>
</signal>
<signal name="PL4">
<contactref element="XIO" pad="26"/>
<contactref element="U$1" pad="65"/>
<contactref element="U$1" pad="45"/>
</signal>
<signal name="PL5">
<contactref element="XIO" pad="25"/>
<contactref element="U$1" pad="46"/>
<contactref element="U$1" pad="64"/>
</signal>
<signal name="PL6">
<contactref element="XIO" pad="24"/>
<contactref element="U$1" pad="47"/>
<contactref element="U$1" pad="63"/>
</signal>
<signal name="PL7">
<contactref element="XIO" pad="23"/>
<contactref element="U$1" pad="48"/>
<contactref element="U$1" pad="68"/>
</signal>
<signal name="PB7">
<contactref element="PINS" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="XIO" pad="2"/>
<contactref element="POWER" pad="2"/>
<contactref element="SDCARD" pad="5"/>
<contactref element="SDCARD" pad="6"/>
<contactref element="10K" pad="P$2"/>
<contactref element="CA_RGB_LED" pad="2"/>
<contactref element="I2CCLOCKGEN" pad="1"/>
<contactref element="XIO" pad="1"/>
<contactref element="POWER" pad="5"/>
<contactref element="LCD" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="5V" pad="1"/>
</signal>
<signal name="PH0">
<contactref element="COMMUNICATION" pad="5"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="N$2">
<contactref element="SDCARD" pad="3"/>
<contactref element="SDCARD" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="CA_RGB_LED" pad="4"/>
<contactref element="220R" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="CA_RGB_LED" pad="3"/>
<contactref element="220R1" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="CA_RGB_LED" pad="1"/>
<contactref element="220R2" pad="P$2"/>
</signal>
<signal name="CLK2">
<contactref element="I2CCLOCKGEN" pad="5"/>
<contactref element="CIC" pad="2"/>
<contactref element="U$1" pad="81"/>
<contactref element="U$1" pad="56"/>
</signal>
<signal name="CLK1">
<contactref element="I2CCLOCKGEN" pad="6"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="CLK0">
<contactref element="I2CCLOCKGEN" pad="7"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="SJ1" pad="2"/>
<contactref element="U$1" pad="57"/>
<contactref element="U$1" pad="82"/>
</signal>
<signal name="CICDATA0">
<contactref element="CIC" pad="7"/>
<contactref element="U$1" pad="75"/>
<contactref element="U$1" pad="55"/>
</signal>
<signal name="CICDATA1">
<contactref element="CIC" pad="6"/>
<contactref element="U$1" pad="24"/>
</signal>
<signal name="CICRSTSO">
<contactref element="CIC" pad="5"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="27"/>
<contactref element="5V" pad="2"/>
<contactref element="U$1" pad="58"/>
<contactref element="U$1" pad="83"/>
</signal>
<signal name="N$7">
<contactref element="CIC" pad="1"/>
<contactref element="SJ3" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
