(kicad_pcb (version 20171130) (host pcbnew 5.1.0-060a0da~80~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 187)
    (zones 0)
    (modules 27)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.381)
    (via_drill 0.254)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (user_via 0.4 0.254)
    (user_via 0.6 0.4)
    (user_via 0.8 0.6)
    (user_via 1 0.8)
    (user_via 1.3 1)
    (user_via 1.5 1.2)
    (user_via 1.7 1.4)
    (user_via 1.9 1.6)
    (uvia_size 0.381)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.381)
    (uvia_min_drill 0.254)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1)
    (solder_mask_min_width 0.05)
    (pad_to_paste_clearance_ratio -0.15)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "OSH_Park_2_layer_plots"))
  )
  (net 0 "")
  (net 1 /VSS)
  (net 2 "Net-(C1-Pad1)")
  (net 3 /VBUS)
  (net 4 /VDD)
  (net 5 /VDDIO)
  (net 6 /VDD_33V)
  (net 7 "Net-(C9-Pad2)")
  (net 8 "Net-(C10-Pad2)")
  (net 9 "Net-(J1-Pad4)")
  (net 10 /USB_DP)
  (net 11 /USB_DM)
  (net 12 /CTSI)
  (net 13 /TXO)
  (net 14 /RXI)
  (net 15 /RTSO)
  (net 16 "Net-(D1-Pad2)")
  (net 17 "Net-(FB1-Pad2)")
  (net 18 /VDDCONN)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.381)
    (uvia_drill 0.254)
    (add_net /CTSI)
    (add_net /RTSO)
    (add_net /RXI)
    (add_net /TXO)
    (add_net /USB_DM)
    (add_net /USB_DP)
    (add_net /VBUS)
    (add_net /VDD)
    (add_net /VDDCONN)
    (add_net /VDDIO)
    (add_net /VDD_33V)
    (add_net /VSS)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(FB1-Pad2)")
    (add_net "Net-(J1-Pad4)")
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 144.2 91.2 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference N1 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OHWLOGO (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module SquantorLabels:Label_version (layer B.Cu) (tedit 5B5A1E49)
    (at 148.2 92.3 270)
    (fp_text reference N2 (at 0 -1.4 270) (layer B.Fab) hide)
    (fp_text value 20190401 (at -0.4 0.1 270) (layer B.SilkS))
    (fp_text user V: (at -4.8 0.1 270) (layer B.SilkS))
  )
  (module SquantorRcl:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 143.7 96.9)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.1 1.7) (layer F.SilkS))
    (fp_text value 100n (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 155.9 93.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.4 0 270) (layer F.SilkS))
    (fp_text value 1u (at 2.4 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /VDDCONN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 147.8 84.9 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.1 1.6 90) (layer F.SilkS))
    (fp_text value 10u (at 0.9 1.6 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 153.95 87.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0.45 -1.3 180) (layer F.SilkS))
    (fp_text value 1u (at 0.55 -1.3 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /VDD_33V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0603_hand (layer F.Cu) (tedit 587552B0)
    (at 146 84.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB1 (at -2.2 -2.2 180) (layer F.SilkS))
    (fp_text value 600 (at -2.2 -2.3 180) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(FB1-Pad2)"))
    (pad 1 smd rect (at -0.85 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorUsb:USB-muB-SMD_TH (layer F.Cu) (tedit 5B3D26BA)
    (at 143.7 91.2 270)
    (fp_text reference J1 (at 5.6 -2.7) (layer F.SilkS))
    (fp_text value USB-ID (at 5.4 -2.6 270) (layer F.Fab))
    (pad S thru_hole circle (at -3.575 -1.725 270) (size 1.2 1.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad S thru_hole circle (at 3.575 -1.725 270) (size 1.2 1.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad S thru_hole circle (at -3.575 1.725 270) (size 1.2 1.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad "" np_thru_hole circle (at -2 -0.575 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu))
    (pad 5 smd rect (at 1.3 -1.3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 4 smd rect (at 0.65 -1.3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -1.3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 10 /USB_DP))
    (pad 2 smd rect (at -0.65 -1.3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 11 /USB_DM))
    (pad 1 smd rect (at -1.3 -1.3 270) (size 0.4 1.85) (layers F.Cu F.Paste F.Mask)
      (net 3 /VBUS))
    (pad "" np_thru_hole circle (at 2 -0.575 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu))
    (pad S thru_hole circle (at 3.575 1.725 270) (size 1.2 1.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module SquantorIC:SOT23-3-Microchip-TT (layer F.Cu) (tedit 5C6B2141)
    (at 153.1 93.9 90)
    (fp_text reference U1 (at -1.1 -1.1 180) (layer F.SilkS))
    (fp_text value MCP1702-CB (at -4.6 2.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.15 90) (size 0.65 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 2 smd rect (at 0.95 1.15 90) (size 0.65 1.05) (layers F.Cu F.Paste F.Mask)
      (net 18 /VDDCONN))
    (pad 3 smd rect (at 0 -1.15 90) (size 0.65 1.05) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
  )
  (module SquantorIC:MSOP-10 (layer F.Cu) (tedit 5C993A76)
    (at 152.4 90.1 180)
    (fp_text reference U2 (at 3.2 2.4 180) (layer F.SilkS))
    (fp_text value HT42B534-MSOP10 (at 0.2 5.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.3 -1 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 2 smd rect (at -2.3 -0.5 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /VDD_33V))
    (pad 3 smd rect (at -2.3 0 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 4 smd rect (at -2.3 0.5 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /CTSI))
    (pad 5 smd rect (at -2.3 1 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /TXO))
    (pad 6 smd rect (at 2.3 1 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDDIO))
    (pad 7 smd rect (at 2.3 0.5 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /RXI))
    (pad 8 smd rect (at 2.3 0 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /RTSO))
    (pad 9 smd rect (at 2.3 -0.5 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad2)"))
    (pad 10 smd rect (at 2.3 -1 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad2)"))
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 143 84.3 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0.3 -1.2 90) (layer F.SilkS))
    (fp_text value 100n (at 0.3 -1.2 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /VBUS) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 151.3 87.7)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0.6 -1.5 180) (layer F.SilkS))
    (fp_text value 100n (at 0.9 -1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS) (solder_mask_margin 0.1))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDDIO) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 156 90.55 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 2.15 0.1 90) (layer F.SilkS))
    (fp_text value 100n (at 2.25 0.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 148.2 88.9)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at -1.2 -1.2) (layer F.SilkS))
    (fp_text value 47p (at -1.1 -1.2) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad2)") (solder_mask_margin 0.1))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:C_0402 (layer F.Cu) (tedit 58D18F8A)
    (at 148.2 92.8)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at -0.7 2.7) (layer F.SilkS))
    (fp_text value 47p (at -0.6 2.8) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad2)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 148.2 94.1)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 2 0.9) (layer F.SilkS))
    (fp_text value 0 (at 1.9 0.9) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 148.2 91.5)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 2 2.3) (layer F.SilkS))
    (fp_text value 33 (at 2 2.3) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /USB_DP))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 148.2 90.2)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 2 2.3) (layer F.SilkS))
    (fp_text value 33 (at 2 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /USB_DM))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 148.45 97.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0.05 -1.3 180) (layer F.SilkS))
    (fp_text value 1K (at 0.05 -1.3 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0603_hand (layer F.Cu) (tedit 587552B0)
    (at 144.4 84.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 1.4 2.6 270) (layer F.SilkS))
    (fp_text value Fuse (at 1.2 2.6 270) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(FB1-Pad2)"))
    (pad 2 smd rect (at 0.85 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VBUS))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorRcl:R_0402_hand (layer F.Cu) (tedit 5921FEA0)
    (at 155.9 85.6 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 2 0 270) (layer F.SilkS))
    (fp_text value 10K (at 2 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /TXO))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDDIO))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorDiodes:SOD-523 (layer F.Cu) (tedit 5C9BDEC5)
    (at 149.9 85.4)
    (fp_text reference D2 (at 1 -1.6 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 4.7 -1.8) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 2 smd rect (at 0.7 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDDIO))
  )
  (module SquantorSpecial:solder_jumper_2way_noconn (layer B.Cu) (tedit 5C9BE0F0)
    (at 154.6 85.4 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference SJ1 (at -2.6 -0.4 90) (layer B.SilkS))
    (fp_text value vddio=vddconn (at -2.4 -3.9 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Mask)
      (net 18 /VDDCONN))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Mask)
      (net 5 /VDDIO))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorSpecial:solder_jumper_2way_conn (layer B.Cu) (tedit 5C9BE3F7)
    (at 153.3 85.4 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference SJ3 (at 2.6 0.4 90) (layer B.SilkS))
    (fp_text value vddio=3.3v (at 1.2 3.7 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Mask)
      (net 5 /VDDIO))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Mask)
      (net 6 /VDD_33V))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorSpecial:solder_jumper_2way_conn (layer B.Cu) (tedit 5C9BE3F7)
    (at 153.5 93.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference SJ2 (at 0.3 2.1 270) (layer B.SilkS))
    (fp_text value vddconn=vdd (at 1.6 -0.5 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Mask)
      (net 18 /VDDCONN))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Mask)
      (net 4 /VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SquantorDiodes:D_0603_hand (layer F.Cu) (tedit 5CA1F802)
    (at 151.1 97.4 180)
    (descr "Diode SMD 0603, reflow soldering, general purpose")
    (tags "Diode 0603")
    (attr smd)
    (fp_text reference D1 (at -2.7 0 180) (layer F.SilkS))
    (fp_text value RED (at -2.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /VSS))
    (pad 2 smd rect (at 0.85 0 180) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad2)"))
  )
  (module SquantorConnectorsNamed:Molex_KK-254_AE-6410-06A_1x06_P2.54mm_Vertical_FTDI_UART (layer F.Cu) (tedit 5CA1FE89)
    (at 160.1 97.3 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-06A example for new part number: 22-27-2061, 6 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator. Now with FTDI pinout labels")
    (tags "connector Molex KK-254 side entry FTDI UART")
    (fp_text reference J2 (at -0.9 -4.2 90) (layer F.SilkS))
    (fp_text value FTDI_PINS_1X06_input (at 6.35 4.08 90) (layer F.Fab))
    (fp_text user %R (at 6.35 -2.22 90) (layer F.Fab))
    (fp_text user GND (at 0 -4.3) (layer B.SilkS))
    (fp_text user CTS# (at 2.54 -4.5) (layer B.SilkS))
    (fp_text user VCC (at 5.08 -4.3) (layer B.SilkS))
    (fp_text user TXD (at 7.62 -4.3) (layer B.SilkS))
    (fp_text user RXD (at 10.16 -4.3) (layer B.SilkS))
    (fp_text user RTS# (at 13.6 -4.5) (layer B.SilkS))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 /VSS))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 /CTSI))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /VDDCONN))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 /TXO))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 /RXI))
    (pad 6 thru_hole oval (at 12.7 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /RTSO))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-06A_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 141 82.6) (end 163.7 82.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141 99.3) (end 141 82.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.7 99.3) (end 141 99.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.7 82.6) (end 163.7 99.3) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name /VSS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 141 82.6) (xy 163.7 82.6) (xy 163.7 99.3) (xy 141 99.3)
      )
    )
  )
)
