(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "-12V")
  (net 4 "Net-(D1-COM)")
  (net 5 "Net-(D2-COM)")
  (net 6 "/FACE")
  (net 7 "Net-(J1-Pin_1)")
  (net 8 "Net-(J1-Pin_10)")
  (net 9 "/IN0")
  (net 10 "unconnected-(J2-PadTN)")
  (net 11 "/OUT0")
  (net 12 "unconnected-(J3-PadTN)")
  (net 13 "/OUT1")
  (net 14 "unconnected-(J4-PadTN)")
  (net 15 "/OUT2")
  (net 16 "unconnected-(J5-PadTN)")
  (net 17 "/IN1")
  (net 18 "/OUT3")
  (net 19 "unconnected-(J7-PadTN)")
  (net 20 "/OUT4")
  (net 21 "unconnected-(J8-PadTN)")
  (net 22 "/OUT5")
  (net 23 "unconnected-(J9-PadTN)")
  (net 24 "Net-(U1A-+)")
  (net 25 "Net-(U1B-+)")
  (net 26 "Net-(U1B--)")
  (net 27 "Net-(U1C--)")
  (net 28 "Net-(U1D--)")
  (net 29 "Net-(U2A-+)")
  (net 30 "Net-(U2B-+)")
  (net 31 "Net-(U2B--)")
  (net 32 "Net-(U2C--)")
  (net 33 "Net-(U2D--)")
  (net 34 "/GND'")
  (net 35 "/IN0'")
  (net 36 "/IN1'")
  (net 37 "/OUT0'")
  (net 38 "/OUT1'")
  (net 39 "/OUT2'")
  (net 40 "/OUT3'")
  (net 41 "/OUT4'")
  (net 42 "/OUT5'")
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 125.73 107.844 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J7" (at 5.842 -4.424 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 18 "/OUT3") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J7-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 125.73 141.459 180)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H10" (at -3.302 -4.064 180 unlocked) (layer "F.Fab"))
    (fp_text value "out 2" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 149.86 107.844 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J9" (at 5.842 -4.424 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 22 "/OUT5") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(J9-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 106.68 74.168)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J13" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "/IN0'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "/IN1'") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 125.73 96.668 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J3" (at 5.842 4.466 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "/OUT0") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(J3-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 137.795 96.668 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J4" (at 5.842 4.466 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 13 "/OUT1") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(J4-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 109.305 119.3)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H1" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount0" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "output"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 109.305 152.95)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H4" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount3" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 149.86 141.459 180)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H12" (at -3.302 -4.064 180 unlocked) (layer "F.Fab"))
    (fp_text value "out 2" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 149.86 130.283)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H9" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "out 1" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (at 113.665 141.457)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H6" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "in 2" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole" (layer "F.Cu")
    (at 113.665 130.283)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H5" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "in 1" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 154.855 119.3)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H2" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 113.665 96.668 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J2" (at 5.842 4.466 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "/IN0") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(J2-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 157.48 68.58)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J14" (at 0 7.366) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/OUT0'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/OUT1'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/OUT2'") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 149.86 96.668 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J5" (at 5.842 4.466 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 15 "/OUT2") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J5-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 137.795 141.459 180)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H11" (at -3.302 -4.064 180 unlocked) (layer "F.Fab"))
    (fp_text value "out 2" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 125.73 130.283)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H7" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "out 1" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 157.48 81.28)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J15" (at 0 -2.286) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "/OUT3'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "/OUT4'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "/OUT5'") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 137.795 130.283)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H8" (at -3.302 -4.064 unlocked) (layer "F.Fab"))
    (fp_text value "out 1" (at 0 -6.858 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 155.08 152.95)
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H3" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount2" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 113.665 107.842 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J6" (at 5.842 -4.426 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "/IN1") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "/IN0") (pintype "passive"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 137.795 107.844 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J8" (at 5.842 -4.424 unlocked) (layer "F.SilkS"))
    (fp_text value "AudioJack2_SwitchT" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 20 "/OUT4") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(J8-PadTN)") (pintype "passive+no_connect"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 149.86 77.396 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 33 "Net-(U2D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 42 "/OUT5'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 122.1613 73.1669 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 1.7653 1.65) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(D1-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 136.398 81.5455 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0.0115 -1.778 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 136.398 73.329 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(U1A-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 25 "Net-(U1B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 149.733 85.3555 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 1.651 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 36 "/IN1'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 29 "Net-(U2A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (at 143.383 71.424 -90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14")
    (property "ki_keywords" "quad opamp")
    (attr smd)
    (fp_text reference "U1" (at 0 5.28 90) (layer "B.SilkS"))
    (fp_text value "TL074" (at 0 -5.08 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1B-+)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 -1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1B-+)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 -2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 -3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1B--)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1C--)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 -2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1C--)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 -1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1B-+)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1B-+)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U1D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U1D--)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 141.478 77.396 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 32 "Net-(U2C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 41 "/OUT4'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 123.4313 79.5169 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D2" (at 0 2.4 90) (layer "B.SilkS"))
    (fp_text value "BAT54S" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 122.1613 75.7069 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 1.7653 -1.7631) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 5 "Net-(D2-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(J1-Pin_10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (at 123.4313 69.3569 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D1" (at 0 2.4 90) (layer "B.SilkS"))
    (fp_text value "BAT54S" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (at 142.748 83.4505 90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14")
    (property "ki_keywords" "quad opamp")
    (attr smd)
    (fp_text reference "U2" (at 0 5.28 90) (layer "B.SilkS"))
    (fp_text value "TL074" (at 0 -5.28 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U2B-+)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U2A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U2B-+)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U2B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U2B--)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U2C--)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U2C--)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U2B-+)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U2B-+)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(U2D--)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(U2D--)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 149.733 69.519 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.651 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(U1B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 37 "/OUT0'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 115.824 72.57 180)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "PartNum" "A-2939")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -4.4323 4.4831) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at -2.3114 -5.0502 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 138.938 77.396 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 28 "Net-(U1D--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 39 "/OUT2'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 136.398 85.3555 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.778 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 31 "Net-(U2B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 40 "/OUT3'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 106.68 99.223 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J10" (at 0.508 2.33) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "/GND'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/IN0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/IN1") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 149.733 81.5455 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 29 "Net-(U2A-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 30 "Net-(U2B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 147.32 77.396 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "1K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 27 "Net-(U1C--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 38 "/OUT1'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 122.7963 83.9619 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at -1.905 2.54) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 136.398 69.519 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.905 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 35 "/IN0'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(U1A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 128.5113 86.5019 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 4.445 -1.905) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 149.733 73.329 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0.077 -1.651 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 157.48 106.305 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J12" (at 0 2.165) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/OUT3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/OUT4") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/OUT5") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 157.48 93.605 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "mult.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 0 -7.233) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/OUT0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/OUT1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/OUT2") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 104.305 66.22) (end 159.855 88.72)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 104.305 116.3) (end 159.855 155.95)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 104.305 91.26) (end 159.855 113.76)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "thismatters/mult/v0" (at 129.032 94.742 90) (layer "B.SilkS"))
  (gr_text "thismatters/mult/v0" (at 133.096 70.104 90) (layer "B.SilkS"))
  (gr_text "POWER" (at 125.9713 71.8969 90) (layer "B.SilkS"))
  (gr_text "N" (at 113.665 136.652) (layer "F.SilkS"))
  (gr_text "thismatters/mult/v0" (at 159.258 149.352 90) (layer "F.SilkS"))
  (gr_text "mult" (at 131.826 155.702) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 161.29 65.86)
        (xy 102.87 65.86)
        (xy 102.87 89.99)
        (xy 161.29 89.99)
      )
    )
  )
  (zone (net 34) (net_name "/GND'") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 161.29 114.12)
        (xy 102.87 114.12)
        (xy 102.87 89.99)
        (xy 161.29 89.99)
      )
    )
  )
  (zone (net 6) (net_name "/FACE") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 161.29 115.39)
        (xy 102.87 115.39)
        (xy 102.87 157.3)
        (xy 161.29 157.3)
      )
    )
  )
)
