(kicad_pcb (version 20171130) (host pcbnew 5.0.1-33cea8e~68~ubuntu16.04.1)
  (general
    (thickness 0.8)
    (drawings 8)
    (tracks 167)
    (zones 0)
    (modules 28)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu jumper)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.1524)
    (zone_clearance 0.381)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GNDD)
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(DM1-Pad1)")
  (net 8 "Net-(R2-Pad2)")
  (net 9 "Net-(R3-Pad1)")
  (net 10 "Net-(12V1-Pad1)")
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(5V1-Pad1)")
  (net 13 "Net-(U4-Pad1)")
  (net 14 "Net-(U5-Pad1)")
  (net 15 "Net-(U1-Pad7)")
  (net 16 "Net-(U1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GNDD)
    (add_net "Net-(12V1-Pad1)")
    (add_net "Net-(5V1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(DM1-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U5-Pad1)")
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 155.575 104.14 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 47uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(5V1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 149.225 113.665 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.5 180) (layer F.SilkS) hide)
    (fp_text value MP1580 (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad8)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyKiCAD:VIA-0.8-1.6x2.5sq (layer F.Cu) (tedit 5BF2431F)
    (at 146.685 99.06)
    (fp_text reference DM1 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.6 2.5) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(DM1-Pad1)") (zone_connect 2))
  )
  (module MyKiCAD:VIA-0.8-1.6x2.5sq (layer F.Cu) (tedit 5BF2431F)
    (at 144.145 99.06)
    (fp_text reference VFB1 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.6 2.5) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(R3-Pad1)") (zone_connect 2))
  )
  (module MyKiCAD:VIA-0.8-1.6x2.5sq (layer F.Cu) (tedit 5BF2431F)
    (at 149.225 99.06)
    (fp_text reference DP1 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.6 2.5) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(DM1-Pad1)") (zone_connect 2))
  )
  (module MyKiCAD:VIA-0.8-1.6x2.5sq (layer F.Cu) (tedit 5BF2431F)
    (at 151.765 99.06)
    (fp_text reference 5V1 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.6 2.5) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(5V1-Pad1)") (zone_connect 2))
  )
  (module MyKiCAD:VIA-1.2-2.5MM (layer F.Cu) (tedit 5BF231A4)
    (at 154.94 99.06)
    (fp_text reference GND3 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 GNDD) (zone_connect 2))
  )
  (module MyKiCAD:VIA-1.2-2.5MM (layer F.Cu) (tedit 5BF231A4)
    (at 151.13 118.745)
    (fp_text reference 12V1 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(12V1-Pad1)") (zone_connect 2))
  )
  (module MyKiCAD:VIA-1.2-2.5MM (layer F.Cu) (tedit 5BF231A4)
    (at 157.48 118.745)
    (fp_text reference GND2 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 GNDD) (zone_connect 2))
  )
  (module MyKiCAD:VIA-1.2-2.5MM (layer F.Cu) (tedit 5BF231A4)
    (at 147.955 118.745)
    (fp_text reference 12V2 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(12V1-Pad1)") (zone_connect 2))
  )
  (module MyKiCAD:VIA-1.2-2.5MM (layer F.Cu) (tedit 5BF231A4)
    (at 141.605 118.745)
    (fp_text reference GND1 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 GNDD) (zone_connect 2))
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5BF8C8FB)
    (at 153.67 111.76)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 1.75) (layer B.SilkS) hide)
    (fp_text value 10uF/35V (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 140.97 112.395 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.524 90) (layer F.SilkS) hide)
    (fp_text value 4n7 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 154.432 114.3 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 142.875 114.935 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.524 180) (layer F.SilkS) hide)
    (fp_text value 4n7 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB (layer B.Cu) (tedit 5BF8C8F5)
    (at 144.78 113.665 180)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D1 (at 0 3 180) (layer B.SilkS) hide)
    (fp_text value S3JB (at 0 -3.1 180) (layer B.Fab))
    (fp_text user %R (at 0 3 180) (layer B.Fab))
    (pad 1 smd rect (at -2.15 0 180) (size 2.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.15 0 180) (size 2.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA (layer B.Cu) (tedit 5BF8C8FF)
    (at 154.4 114.935)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D2 (at 0 2.5) (layer B.SilkS) hide)
    (fp_text value TPSMA6L16A (at 0 -2.6) (layer B.Fab))
    (fp_text user %R (at 0 2.5) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 58645DF3)
    (at 154.559 108.585)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D4 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value B230ADICT-ND (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -3) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyKiCAD:L_Taiyo-Yuden_NR10050 (layer B.Cu) (tedit 5BF8C903)
    (at 149.225 106.045)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-5050, 5.0mmx5.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 10uH (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 4 0) (size 2.6 4.5) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(5V1-Pad1)"))
    (pad 1 smd rect (at -4 0) (size 2.6 4.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_MD-5050.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 140.97 115.316 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.127 0.127 180) (layer F.SilkS) hide)
    (fp_text value 15k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 140.97 109.601 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.159 0 270) (layer F.SilkS) hide)
    (fp_text value "10k2 1%" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 142.875 109.601 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.651 270) (layer F.SilkS) hide)
    (fp_text value "34k 1%" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 144.792 95.504 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 56 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(5V1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 154.432 95.885 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 68k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(5V1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(DM1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 144.78 97.028 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 22k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(DM1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyKiCAD:VIA-0.6MM-1.6MM (layer F.Cu) (tedit 5A6924B4)
    (at 148.209 96.012)
    (fp_text reference U4 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.6) (layers *.Cu)
      (net 13 "Net-(U4-Pad1)") (zone_connect 2))
  )
  (module MyKiCAD:VIA-0.6MM-1.6MM (layer F.Cu) (tedit 5A6924B4)
    (at 150.876 96.012)
    (fp_text reference U5 (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.6) (layers *.Cu)
      (net 14 "Net-(U5-Pad1)") (zone_connect 2))
  )
  (module "MyKiCAD:LittleFuse Fast Fuse Axial" (layer F.Cu) (tedit 5BF8C876)
    (at 144.78 118.745)
    (fp_text reference F1 (at 5.08 -3.175) (layer F.SilkS) hide)
    (fp_text value "5A Fast Blow" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2 2) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D1-Pad2)"))
    (pad 2 thru_hole roundrect (at 9.525 0) (size 2 2) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(12V1-Pad1)"))
  )
  (gr_line (start 142.24 104.775) (end 142.24 94.615) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.7 104.775) (end 142.24 104.775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.7 120.65) (end 139.7 104.775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.385 120.65) (end 139.7 120.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.385 104.775) (end 159.385 120.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.845 104.775) (end 159.385 104.775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.845 94.615) (end 156.845 104.775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.24 94.615) (end 156.845 94.615) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads no (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 120.65) (xy 159.385 120.65) (xy 159.385 104.775) (xy 156.845 104.775) (xy 156.845 94.615)
        (xy 142.24 94.615) (xy 142.24 104.775) (xy 139.7 104.775) (xy 139.7 120.015)
      )
    )
  )
  (zone (net 2) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads no (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 94.615) (xy 156.845 94.615) (xy 156.845 104.775) (xy 159.385 104.775) (xy 159.385 120.65)
        (xy 139.7 120.65) (xy 139.7 104.775) (xy 142.24 104.775)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 103.505) (xy 146.685 100.965) (xy 151.765 100.965) (xy 154.305 103.505) (xy 154.305 108.585)
        (xy 151.765 111.125) (xy 146.685 111.125) (xy 144.145 108.585)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 103.505) (xy 146.685 100.965) (xy 151.765 100.965) (xy 154.305 103.505) (xy 154.305 108.585)
        (xy 151.765 111.125) (xy 146.685 111.125) (xy 144.145 108.585)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.765 111.125) (xy 151.765 112.395) (xy 148.59 112.395) (xy 148.59 111.125)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.575 94.996) (xy 152.654 94.996) (xy 152.654 96.393) (xy 155.575 96.393)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.32 111.125) (xy 151.13 111.125) (xy 151.13 116.205) (xy 147.32 116.205)
      )
    )
  )
)
