(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1)
  (general
    (links 66)
    (no_connects 0)
    (area 9.470317 12.914999 58.395 37.05086)
    (thickness 1.6)
    (drawings 5)
    (tracks 334)
    (zones 0)
    (modules 36)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (trace_clearance 0.2)
    (zone_clearance 0.16)
    (zone_45_only yes)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.686)
    (via_min_drill 0.33)
    (user_via 0.8 0.4)
    (uvia_size 0.8)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /DVDD5V)
  (net 2 GND)
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C8-Pad1)")
  (net 6 /TCK)
  (net 7 /TMS)
  (net 8 /TDI)
  (net 9 "Net-(J1-Pad6)")
  (net 10 /CSYNC_i)
  (net 11 /MCLK_EXT_i)
  (net 12 /MCLK_SEL_i)
  (net 13 "Net-(Q1-Pad2)")
  (net 14 /TDO)
  (net 15 /CSYNC_o)
  (net 16 /GCLK_o)
  (net 17 "Net-(U1-Pad2)")
  (net 18 "Net-(U1-Pad3)")
  (net 19 "Net-(U1-Pad5)")
  (net 20 "Net-(U1-Pad6)")
  (net 21 "Net-(U1-Pad8)")
  (net 22 "Net-(U1-Pad10)")
  (net 23 "Net-(U1-Pad11)")
  (net 24 "Net-(U1-Pad12)")
  (net 25 "Net-(U1-Pad13)")
  (net 26 "Net-(U1-Pad14)")
  (net 27 "Net-(U1-Pad19)")
  (net 28 "Net-(U1-Pad20)")
  (net 29 "Net-(U1-Pad21)")
  (net 30 "Net-(U1-Pad22)")
  (net 31 "Net-(U1-Pad23)")
  (net 32 "Net-(U1-Pad25)")
  (net 33 "Net-(U1-Pad27)")
  (net 34 "Net-(U1-Pad28)")
  (net 35 "Net-(U1-Pad30)")
  (net 36 "Net-(U1-Pad31)")
  (net 37 "Net-(U1-Pad33)")
  (net 38 "Net-(U1-Pad35)")
  (net 39 "Net-(U1-Pad42)")
  (net 40 "Net-(U1-Pad43)")
  (net 41 "Net-(U1-Pad44)")
  (net 42 "Net-(J9-Pad1)")
  (net 43 "Net-(R7-Pad2)")
  (net 44 "Net-(Q1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (add_net /CSYNC_i)
    (add_net /CSYNC_o)
    (add_net /DVDD5V)
    (add_net /GCLK_o)
    (add_net /MCLK_EXT_i)
    (add_net /MCLK_SEL_i)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 5A3E8DE0)
    (at 18.99 14.66 90)
    (attr smd)
    (fp_text reference C1 (at 0.84 1.54 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 5A3E90B6)
    (at 36.77 35.78)
    (attr smd)
    (fp_text reference C2 (at 1.86 0.02 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 24.12 32.77 270)
    (attr smd)
    (fp_text reference C3 (at -1.8288 0 360) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 5A3D2F54)
    (at 41.46 28.99 270)
    (attr smd)
    (fp_text reference C4 (at 1.79 0.01 360) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 14.28 23.67 90)
    (attr smd)
    (fp_text reference C5 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value 12p (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 14.27 20.74 270)
    (attr smd)
    (fp_text reference C6 (at -1.8288 0 360) (layer F.SilkS))
    (fp_text value 12p (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 5A3EEE05)
    (at 34.1 18.9)
    (attr smd)
    (fp_text reference C7 (at -1.82 0.23 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 5A3E92E2)
    (at 54.38 34.39 270)
    (attr smd)
    (fp_text reference C8 (at 1.77 -0.03 360) (layer F.SilkS))
    (fp_text value 330p (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A3EED02)
    (at 46.42 31.68 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2 2.53 90) (layer F.SilkS))
    (fp_text value BC847 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 29.27 35.79)
    (attr smd)
    (fp_text reference R1 (at -1.8288 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 /TDI))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3E908E)
    (at 32.55 35.79 180)
    (attr smd)
    (fp_text reference R2 (at -1.93 -0.03 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 /TMS))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3D31A3)
    (at 34.05 16.53 90)
    (attr smd)
    (fp_text reference R3 (at 1.84 0.01 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 /TCK))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3D3172)
    (at 29.33 18.39 90)
    (attr smd)
    (fp_text reference R4 (at 1.78 -0.05 180) (layer F.SilkS))
    (fp_text value 1.8k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 /TDO))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3EAA08)
    (at 31.2 16.86 90)
    (attr smd)
    (fp_text reference R5 (at -1.81 -0.13 180) (layer F.SilkS))
    (fp_text value 3.3k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3E8CA6)
    (at 14.29 27.35 90)
    (attr smd)
    (fp_text reference R6 (at -0.89 1.48 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 /MCLK_SEL_i))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 23.76 24.18 90)
    (attr smd)
    (fp_text reference R7 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value 1M (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R7-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 23.76 20.53 90)
    (attr smd)
    (fp_text reference R8 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3D2E9B)
    (at 43.46 30.78 270)
    (attr smd)
    (fp_text reference R9 (at 1.84 -0.02 360) (layer F.SilkS))
    (fp_text value 1.8k (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 /CSYNC_o))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Q1-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3D2E97)
    (at 41.45 32.64 270)
    (attr smd)
    (fp_text reference R10 (at 1.86 0.01 360) (layer F.SilkS))
    (fp_text value 3.3k (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3E92DF)
    (at 49.35 34.55 270)
    (attr smd)
    (fp_text reference R11 (at 1.77 -0.06 360) (layer F.SilkS))
    (fp_text value 300 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3EA887)
    (at 51.79 33.55 180)
    (attr smd)
    (fp_text reference R12 (at -0.83 -1.66 270) (layer F.SilkS))
    (fp_text value 100 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 42.36 26.57 180)
    (attr smd)
    (fp_text reference R13 (at -1.8288 0 270) (layer F.SilkS))
    (fp_text value 39 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 /GCLK_o))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 5A3E8A7B)
    (at 45.79 27.33 270)
    (attr smd)
    (fp_text reference R14 (at 0.88 -1.69 360) (layer F.SilkS))
    (fp_text value 210 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J9-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5A3EEDA6)
    (at 19.03 24.68 90)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at -3.8 2.49 180) (layer F.SilkS))
    (fp_text value 21.477272MHz (at 2.44 3.525 90) (layer F.Fab))
    (fp_text user %R (at 2.44 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3E8F53)
    (at 14.34 15.84)
    (fp_text reference J2 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value 5V (at 2.22 0.01) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 1 /DVDD5V))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3EA890)
    (at 55.55 31.79)
    (fp_text reference J10 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value CSYNC_o (at -3.3 -0.08) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 5 "Net-(C8-Pad1)"))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3D2FDD)
    (at 55.55 27.08)
    (fp_text reference J9 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value MCLK_o (at -3 -0.05) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 42 "Net-(J9-Pad1)"))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3D2FE9)
    (at 55.55 29)
    (fp_text reference J8 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value GND (at -2.51 0.02) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3E8ED7)
    (at 14.35 30.09)
    (fp_text reference J7 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value CLK_SEL_i (at 3.55 -0.02) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 12 /MCLK_SEL_i))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3E8ED1)
    (at 14.35 33.81)
    (fp_text reference J6 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value MCLK_EXT_i (at 3.88 -0.02) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 11 /MCLK_EXT_i))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3E8ED4)
    (at 14.35 31.95)
    (fp_text reference J5 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value CSYNC_i (at 3.2 0.02) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 10 /CSYNC_i))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3D2D05)
    (at 14.35 35.69)
    (fp_text reference J4 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value GND (at 2.5 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module custom_components:SMD_PAD (layer F.Cu) (tedit 5A3D2D05)
    (at 14.34 14)
    (fp_text reference J3 (at -3.81254 0) (layer F.SilkS) hide)
    (fp_text value GND (at 2.5 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module custom_components:JTAG_Header_Angled_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A3EAF74)
    (at 42.35 23.69 90)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value JTAG_CONN (at 4.385 14.97 90) (layer F.Fab))
    (fp_text user TDO (at 7.47268 12.7381 90) (layer F.SilkS))
    (fp_text user TDI (at 7.25932 10.20318 90) (layer F.SilkS))
    (fp_text user TMS (at 7.38124 7.66318 90) (layer F.SilkS))
    (fp_text user TCK (at 7.31266 5.11048 90) (layer F.SilkS))
    (fp_text user GND (at 7.22122 2.54254 90) (layer F.SilkS))
    (fp_text user 5V (at 7.21106 0.07366 90) (layer F.SilkS))
    (fp_text user %R (at 2.77 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /DVDD5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /TCK))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /TMS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /TDI))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SMD_JUMPER (layer F.Cu) (tedit 5A3EED8D)
    (at 22.36 34.71 270)
    (attr smd)
    (fp_text reference JP1 (at -1.8288 0 360) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers F.Cu F.Mask)
      (net 1 /DVDD5V))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers F.Cu F.Mask)
      (net 12 /MCLK_SEL_i))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:TQFP-44_10x10mm_Pitch0.8mm_Handsoldering (layer F.Cu) (tedit 5A3EEDEF)
    (at 32.51 27.37 90)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 6.02 5.83 180) (layer F.SilkS))
    (fp_text value ATF1502AS-7AX44 (at 0 7.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.8 -4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /TDI))
    (pad 2 smd rect (at -5.8 -3.2 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -5.8 -2.4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -5.8 -1.6 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -5.8 -0.8 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -5.8 0 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -5.8 0.8 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /TMS))
    (pad 8 smd rect (at -5.8 1.6 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -5.8 2.4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 10 smd rect (at -5.8 3.2 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -5.8 4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -4 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -3.2 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at -2.4 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -1.6 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /CSYNC_o))
    (pad 16 smd rect (at -0.8 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 0 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 18 smd rect (at 0.8 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /GCLK_o))
    (pad 19 smd rect (at 1.6 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.4 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 3.2 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 4 5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 5.8 4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 5.8 3.2 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 5.8 2.4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 5.8 1.6 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /TCK))
    (pad 27 smd rect (at 5.8 0.8 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 5.8 0 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 5.8 -0.8 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 30 smd rect (at 5.8 -1.6 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 5.8 -2.4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad31)"))
    (pad 32 smd rect (at 5.8 -3.2 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /TDO))
    (pad 33 smd rect (at 5.8 -4 90) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad33)"))
    (pad 34 smd rect (at 4 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R7-Pad2)"))
    (pad 35 smd rect (at 3.2 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad35)"))
    (pad 36 smd rect (at 2.4 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 1.6 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 38 smd rect (at 0.8 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /MCLK_SEL_i))
    (pad 39 smd rect (at 0 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /CSYNC_i))
    (pad 40 smd rect (at -0.8 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /MCLK_EXT_i))
    (pad 41 smd rect (at -1.6 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /DVDD5V))
    (pad 42 smd rect (at -2.4 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -3.2 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad43)"))
    (pad 44 smd rect (at -4 -5.8 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad44)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "snes_dejitter\nv1.0" (at 26.6 15.32) (layer F.SilkS))
  (gr_line (start 57 13.02) (end 57 36.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 12.9 36.7) (end 12.9 13.02) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 57 36.7) (end 12.9 36.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 12.9 13.02) (end 57 13.02) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 36.7) (xy 12.9 36.7) (xy 12.9 13.02) (xy 57 13.02)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 36.7) (xy 12.9 36.7) (xy 12.9 13.02) (xy 57 13.02)
      )
    )
  )
)
