(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 78)
    (no_connects 0)
    (area 35.924999 64.924999 86.075001 137.075001)
    (thickness 1.6)
    (drawings 45)
    (tracks 308)
    (zones 0)
    (modules 21)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 /SCL)
  (net 3 /~INT)
  (net 4 /SDA)
  (net 5 /~RESET)
  (net 6 /IO0)
  (net 7 /IO1)
  (net 8 /IO2)
  (net 9 /IO3)
  (net 10 /IO4)
  (net 11 /IO5)
  (net 12 /IO6)
  (net 13 /IO7)
  (net 14 /IO8)
  (net 15 /IO9)
  (net 16 /IO10)
  (net 17 /IO11)
  (net 18 /IO12)
  (net 19 /IO13)
  (net 20 /IO14)
  (net 21 /IO15)
  (net 22 /V3)
  (net 23 /G3)
  (net 24 /G5)
  (net 25 /V5)
  (net 26 "Net-(M1-Pad1)")
  (net 27 "Net-(M1-Pad6)")
  (net 28 "Net-(M1-Pad11)")
  (net 29 "Net-(M1-Pad21)")
  (net 30 "Net-(M1-Pad26)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /G3)
    (add_net /G5)
    (add_net /IO0)
    (add_net /IO1)
    (add_net /IO10)
    (add_net /IO11)
    (add_net /IO12)
    (add_net /IO13)
    (add_net /IO14)
    (add_net /IO15)
    (add_net /IO2)
    (add_net /IO3)
    (add_net /IO4)
    (add_net /IO5)
    (add_net /IO6)
    (add_net /IO7)
    (add_net /IO8)
    (add_net /IO9)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /V3)
    (add_net /V5)
    (add_net /~INT)
    (add_net /~RESET)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad11)")
    (add_net "Net-(M1-Pad21)")
    (add_net "Net-(M1-Pad26)")
    (add_net "Net-(M1-Pad6)")
  )
  (module "0 My SparkFun:SparkFun_SX1509" (layer F.Cu) (tedit 5A105259)
    (at 61.595 100.965 90)
    (fp_text reference M1 (at 0 -19.05 90) (layer F.SilkS))
    (fp_text value SparkFun_SX1509 (at -1.905 0.635 180) (layer F.SilkS))
    (fp_text user ~INT (at -6.35 -13.97 180) (layer F.SilkS))
    (fp_text user ~RST (at -3.81 -13.97 180) (layer F.SilkS))
    (fp_text user SCL (at 6.35 -13.97 180) (layer F.SilkS))
    (fp_text user SDA (at 3.81 -13.97 180) (layer F.SilkS))
    (fp_text user 3.3V (at 1.27 -13.716 180) (layer F.SilkS))
    (fp_text user GND (at -1.27 -13.97 180) (layer F.SilkS))
    (fp_text user SCL (at 6.35 13.97 180) (layer F.SilkS))
    (fp_text user SDA (at 3.81 13.97 180) (layer F.SilkS))
    (fp_text user 3.3V (at 1.27 13.716 180) (layer F.SilkS))
    (fp_text user GND (at -1.27 13.97 180) (layer F.SilkS))
    (fp_text user ~RST (at -3.81 13.97 180) (layer F.SilkS))
    (fp_text user OSC (at -6.35 13.97 180) (layer F.SilkS))
    (fp_text user GND (at 4.826 -11.43 90) (layer F.SilkS))
    (fp_text user 15 (at 5.08 -8.89 90) (layer F.SilkS))
    (fp_text user 14 (at 5.08 -6.35 90) (layer F.SilkS))
    (fp_text user 13 (at 5.08 -3.81 90) (layer F.SilkS))
    (fp_text user 12 (at 5.08 -1.27 90) (layer F.SilkS))
    (fp_text user VCC2 (at 3.81 1.27 90) (layer F.SilkS))
    (fp_text user 11 (at 5.08 3.81 90) (layer F.SilkS))
    (fp_text user 10 (at 5.08 6.35 90) (layer F.SilkS))
    (fp_text user 9 (at 5.08 8.89 90) (layer F.SilkS))
    (fp_text user 8 (at 5.08 11.43 90) (layer F.SilkS))
    (fp_text user GND (at -4.064 -11.43 90) (layer F.SilkS))
    (fp_text user 7 (at -5.08 11.43 90) (layer F.SilkS))
    (fp_text user 6 (at -5.08 8.89 90) (layer F.SilkS))
    (fp_text user 5 (at -5.08 6.35 90) (layer F.SilkS))
    (fp_text user 4 (at -5.08 3.81 90) (layer F.SilkS))
    (fp_text user VCC1 (at -3.81 1.27 90) (layer F.SilkS))
    (fp_text user 3 (at -5.08 -1.27 90) (layer F.SilkS))
    (fp_text user 2 (at -5.08 -3.81 90) (layer F.SilkS))
    (fp_text user 1 (at -5.08 -6.35 90) (layer F.SilkS))
    (fp_text user 0 (at -5.08 -8.89 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 -11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(M1-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /IO0))
    (pad 3 thru_hole circle (at -7.62 -6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /IO1))
    (pad 4 thru_hole circle (at -7.62 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /IO2))
    (pad 5 thru_hole circle (at -7.62 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 /IO3))
    (pad 6 thru_hole circle (at -7.62 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(M1-Pad6)"))
    (pad 7 thru_hole circle (at -7.62 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 /IO4))
    (pad 8 thru_hole circle (at -7.62 6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /IO5))
    (pad 9 thru_hole circle (at -7.62 8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 /IO6))
    (pad 10 thru_hole circle (at -7.62 11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /IO7))
    (pad 11 thru_hole circle (at -6.35 16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(M1-Pad11)"))
    (pad 12 thru_hole circle (at -3.81 16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /~RESET))
    (pad 13 thru_hole circle (at -1.27 16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /G3))
    (pad 14 thru_hole circle (at 1.27 16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /V3))
    (pad 15 thru_hole circle (at 3.81 16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 16 thru_hole circle (at 6.35 16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /SCL))
    (pad 17 thru_hole circle (at 7.62 11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 /IO8))
    (pad 18 thru_hole circle (at 7.62 8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /IO9))
    (pad 19 thru_hole circle (at 7.62 6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /IO10))
    (pad 20 thru_hole circle (at 7.62 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /IO11))
    (pad 21 thru_hole circle (at 7.62 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(M1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /IO12))
    (pad 23 thru_hole circle (at 7.62 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /IO13))
    (pad 24 thru_hole circle (at 7.62 -6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /IO14))
    (pad 25 thru_hole circle (at 7.62 -8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 /IO15))
    (pad 26 thru_hole circle (at 7.62 -11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(M1-Pad26)"))
    (pad 27 thru_hole circle (at 6.35 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /SCL))
    (pad 28 thru_hole circle (at 3.81 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 29 thru_hole circle (at 1.27 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /V3))
    (pad 30 thru_hole circle (at -1.27 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /G3))
    (pad 31 thru_hole circle (at -3.81 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /~RESET))
    (pad 32 thru_hole circle (at -6.35 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 /~INT))
  )
  (module w_conn_strip:vasch_strip_5x2 (layer F.Cu) (tedit 5A0F0D0B)
    (at 49.53 81.28 180)
    (descr "Box header 5x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P1 (at 9.525 -5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_ELEXOL (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 9 thru_hole oval (at 5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 6 /IO0))
    (pad 10 thru_hole oval (at 5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 23 /G3))
    (pad 8 thru_hole oval (at 2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /IO1))
    (pad 7 thru_hole oval (at 2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 8 /IO2))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 22 /V3))
    (pad 2 thru_hole oval (at -5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 13 /IO7))
    (pad 3 thru_hole oval (at -2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 12 /IO6))
    (pad 4 thru_hole oval (at -2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 11 /IO5))
    (pad 5 thru_hole oval (at 0 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 10 /IO4))
    (pad 6 thru_hole oval (at 0 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 9 /IO3))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_5x2 (layer F.Cu) (tedit 5A0F0D10)
    (at 72.39 81.28 180)
    (descr "Box header 5x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P2 (at -9.525 -5.715 180) (layer F.SilkS))
    (fp_text value MY_CONN_ELEXOL (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 9 thru_hole oval (at 5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 14 /IO8))
    (pad 10 thru_hole oval (at 5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 23 /G3))
    (pad 8 thru_hole oval (at 2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 15 /IO9))
    (pad 7 thru_hole oval (at 2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 16 /IO10))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 22 /V3))
    (pad 2 thru_hole oval (at -5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 21 /IO15))
    (pad 3 thru_hole oval (at -2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 20 /IO14))
    (pad 4 thru_hole oval (at -2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 19 /IO13))
    (pad 5 thru_hole oval (at 0 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 18 /IO12))
    (pad 6 thru_hole oval (at 0 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 17 /IO11))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A0F0C9F)
    (at 50.8 125.73 270)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P3 (at -10.16 0 360) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 270) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 24 /G5))
    (pad 7 thru_hole oval (at 3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 23 /G3))
    (pad 1 thru_hole rect (at -3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 22 /V3))
    (pad 2 thru_hole oval (at -3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /V5))
    (pad 3 thru_hole oval (at -1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SCL))
    (pad 4 thru_hole oval (at -1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~INT))
    (pad 5 thru_hole oval (at 1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA))
    (pad 6 thru_hole oval (at 1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 5 /~RESET))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 (layer F.Cu) (tedit 5A0F0CA3)
    (at 71.12 125.73 270)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P4 (at -10.16 0 360) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 270) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 24 /G5))
    (pad 7 thru_hole oval (at 3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 23 /G3))
    (pad 1 thru_hole rect (at -3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 22 /V3))
    (pad 2 thru_hole oval (at -3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /V5))
    (pad 3 thru_hole oval (at -1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SCL))
    (pad 4 thru_hole oval (at -1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 /~INT))
    (pad 5 thru_hole oval (at 1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SDA))
    (pad 6 thru_hole oval (at 1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 5 /~RESET))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 81.915 125.73 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /G3))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0EE17A)
    (at 41 71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0EE398)
    (at 81 71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0EE459)
    (at 81 131)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0EE076)
    (at 41 131)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5A0F112A)
    (at 81.915 92.075 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 /V3))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_details:testpoint_1mm5 (layer F.Cu) (tedit 5A0F0756)
    (at 59.055 116.84)
    (descr "TestPoint 1.5mm")
    (fp_text reference TP1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value V3 (at -1.905 1.905) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.50114 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 22 /V3))
    (model walter/details/testpoint.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_details:testpoint_1mm5 (layer F.Cu) (tedit 5A0F0759)
    (at 62.865 116.84)
    (descr "TestPoint 1.5mm")
    (fp_text reference TP2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value V5 (at 1.905 1.905) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.50114 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 25 /V5))
    (model walter/details/testpoint.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_details:testpoint_1mm5 (layer F.Cu) (tedit 5A0F06C2)
    (at 59.055 134.62)
    (descr "TestPoint 1.5mm")
    (fp_text reference TP3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value G3 (at -1.905 -1.905) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.50114 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 23 /G3))
    (model walter/details/testpoint.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_details:testpoint_1mm5 (layer F.Cu) (tedit 5A0F06CA)
    (at 62.865 134.62)
    (descr "TestPoint 1.5mm")
    (fp_text reference TP4 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value G5 (at 1.905 -1.905) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.50114 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 24 /G5))
    (model walter/details/testpoint.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 61.595 99.06 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A104D18)
    (at 45.085 94.615)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P6 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 15.03) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /G3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /~RESET))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /~INT))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 5A104D1E)
    (at 50.165 108.585 90)
    (descr "Through hole straight socket strip, 1x10, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x10 2.54mm single row")
    (fp_text reference P7 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_10 (at 0 25.19 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(M1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /IO0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /IO1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /IO2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /IO3))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(M1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /IO4))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /IO5))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IO6))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IO7))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 5A104D22)
    (at 73.025 93.345 270)
    (descr "Through hole straight socket strip, 1x10, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x10 2.54mm single row")
    (fp_text reference P8 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_10 (at 0 25.19 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IO8))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IO9))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IO10))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IO11))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(M1-Pad21)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /IO12))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /IO13))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /IO14))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IO15))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(M1-Pad26)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A104D26)
    (at 78.105 107.315 180)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P9 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 15.03 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(M1-Pad11)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /~RESET))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /G3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /V3))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /SCL))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 60.96 125.73)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference LIC1 (at 0.3 -1.4) (layer F.SilkS) hide)
    (fp_text value CC-BY-NC-SA-icon (at 0.3 0.5) (layer F.SilkS) hide)
  )
  (gr_text 2 (at 69.85 67.945) (layer F.SilkS))
  (gr_text "3V only" (at 60.96 74.93) (layer F.SilkS))
  (gr_text 15 (at 77.47 87.63) (layer F.SilkS))
  (gr_text 14 (at 74.93 74.93) (layer F.SilkS))
  (gr_text 13 (at 74.93 87.63) (layer F.SilkS))
  (gr_text 12 (at 72.39 74.93) (layer F.SilkS))
  (gr_text 11 (at 72.39 87.63) (layer F.SilkS))
  (gr_text 10 (at 69.85 74.93) (layer F.SilkS))
  (gr_text 9 (at 69.85 87.63) (layer F.SilkS))
  (gr_text 8 (at 67.31 74.93) (layer F.SilkS))
  (gr_text 3V (at 77.47 74.93) (layer F.SilkS))
  (gr_text G (at 67.31 87.63) (layer F.SilkS))
  (gr_text 3V (at 54.61 74.93) (layer F.SilkS))
  (gr_text G (at 44.45 87.63) (layer F.SilkS))
  (gr_text 7 (at 54.61 87.63) (layer F.SilkS))
  (gr_text 5 (at 52.07 87.63) (layer F.SilkS))
  (gr_text 3 (at 49.53 87.63) (layer F.SilkS))
  (gr_text 1 (at 46.99 87.63) (layer F.SilkS))
  (gr_text 6 (at 52.07 74.93) (layer F.SilkS))
  (gr_text 4 (at 49.53 74.93) (layer F.SilkS))
  (gr_text 2 (at 46.99 74.93) (layer F.SilkS))
  (gr_text 0 (at 44.45 74.93) (layer F.SilkS))
  (gr_text v1 (at 60.325 70.485) (layer F.SilkS))
  (gr_text "by jeditekunum" (at 60.325 72.39) (layer F.SilkS))
  (gr_text "SX1509 Adapter" (at 60.325 68.58) (layer F.SilkS))
  (dimension 60 (width 0.3) (layer Cmts.User)
    (gr_text "60.000 mm" (at 29.65 101 90) (layer Cmts.User))
    (feature1 (pts (xy 35 71) (xy 28.3 71)))
    (feature2 (pts (xy 35 131) (xy 28.3 131)))
    (crossbar (pts (xy 31 131) (xy 31 71)))
    (arrow1a (pts (xy 31 71) (xy 31.586421 72.126504)))
    (arrow1b (pts (xy 31 71) (xy 30.413579 72.126504)))
    (arrow2a (pts (xy 31 131) (xy 31.586421 129.873496)))
    (arrow2b (pts (xy 31 131) (xy 30.413579 129.873496)))
  )
  (gr_line (start 37 137) (end 85 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 85 66) (end 85 65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 37 65) (end 85 65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 40 (width 0.3) (layer Cmts.User)
    (gr_text "40.000 mm" (at 61 57.65) (layer Cmts.User))
    (feature1 (pts (xy 81 64) (xy 81 56.3)))
    (feature2 (pts (xy 41 64) (xy 41 56.3)))
    (crossbar (pts (xy 41 59) (xy 81 59)))
    (arrow1a (pts (xy 81 59) (xy 79.873496 59.586421)))
    (arrow1b (pts (xy 81 59) (xy 79.873496 58.413579)))
    (arrow2a (pts (xy 41 59) (xy 42.126504 59.586421)))
    (arrow2b (pts (xy 41 59) (xy 42.126504 58.413579)))
  )
  (dimension 50 (width 0.3) (layer Cmts.User)
    (gr_text "50.000 mm" (at 61 50.65) (layer Cmts.User))
    (feature1 (pts (xy 86 64) (xy 86 49.3)))
    (feature2 (pts (xy 36 64) (xy 36 49.3)))
    (crossbar (pts (xy 36 52) (xy 86 52)))
    (arrow1a (pts (xy 86 52) (xy 84.873496 52.586421)))
    (arrow1b (pts (xy 86 52) (xy 84.873496 51.413579)))
    (arrow2a (pts (xy 36 52) (xy 37.126504 52.586421)))
    (arrow2b (pts (xy 36 52) (xy 37.126504 51.413579)))
  )
  (dimension 72 (width 0.3) (layer Cmts.User)
    (gr_text "72.000 mm" (at 22.65 101 90) (layer Cmts.User))
    (feature1 (pts (xy 35 65) (xy 21.3 65)))
    (feature2 (pts (xy 35 137) (xy 21.3 137)))
    (crossbar (pts (xy 24 137) (xy 24 65)))
    (arrow1a (pts (xy 24 65) (xy 24.586421 66.126504)))
    (arrow1b (pts (xy 24 65) (xy 23.413579 66.126504)))
    (arrow2a (pts (xy 24 137) (xy 24.586421 135.873496)))
    (arrow2b (pts (xy 24 137) (xy 23.413579 135.873496)))
  )
  (gr_arc (start 37 136) (end 37 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 85 136) (end 86 136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 37 66) (end 36 66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86 66) (end 86 136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 36 66) (end 36 136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86 137) (xy 36 137) (xy 36 65) (xy 86 65) (xy 86 137)
      )
    )
    (polygon
      (pts        (xy 38 66) (xy 38 136) (xy 84 136) (xy 84 66) (xy 38 66)
      )
    )
  )
)
