(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 0)
    (area 41.834999 36.754999 90.245001 85.165001)
    (thickness 1.6)
    (drawings 4)
    (tracks 271)
    (zones 0)
    (modules 5)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5A942262)
    (at 55.88 42.926 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "" (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "" (at 1.27 22.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5A94241C)
    (at 75.946 78.74 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "" (at 1.27 -2.33 270) (layer F.SilkS) hide)
    (fp_text value "" (at 1.27 22.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5A942513)
    (at 48.26 71.12 180)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "" (at 1.27 -2.33 180) (layer F.SilkS) hide)
    (fp_text value "" (at 1.27 22.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 10.16 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets:PLCC68 (layer F.Cu) (tedit 5A91EB47)
    (at 66.04 60.96 270)
    (descr "Support Plcc 68 pins, pads ronds")
    (tags PLCC)
    (fp_text reference REF** (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value PLCC68 (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -12.7 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -10.16 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -12.7 2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -10.16 2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -12.7 5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -10.16 5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -12.7 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -10.16 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -12.7 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -10.16 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -10.16 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -7.62 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at -7.62 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -5.08 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -5.08 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -2.54 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -2.54 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 0 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 0 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 2.54 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 2.54 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 5.08 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 5.08 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 7.62 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 7.62 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 10.16 12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at 12.7 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 10.16 10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at 12.7 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 10.16 7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 12.7 5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 10.16 5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 12.7 2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 10.16 2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 12.7 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 10.16 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 12.7 -2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 10.16 -2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 12.7 -5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 40 thru_hole circle (at 10.16 -5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at 12.7 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 42 thru_hole circle (at 10.16 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at 12.7 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at 10.16 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 45 thru_hole circle (at 10.16 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 46 thru_hole circle (at 7.62 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at 7.62 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at 5.08 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at 5.08 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 50 thru_hole circle (at 2.54 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 51 thru_hole circle (at 2.54 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at 0 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 53 thru_hole circle (at 0 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 54 thru_hole circle (at -2.54 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 55 thru_hole circle (at -2.54 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 56 thru_hole circle (at -5.08 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 57 thru_hole circle (at -5.08 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 58 thru_hole circle (at -7.62 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 59 thru_hole circle (at -7.62 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 60 thru_hole circle (at -10.16 -12.7 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 61 thru_hole circle (at -12.7 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 62 thru_hole circle (at -10.16 -10.16 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 63 thru_hole circle (at -12.7 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 64 thru_hole circle (at -10.16 -7.62 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 65 thru_hole circle (at -12.7 -5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 66 thru_hole circle (at -10.16 -5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 67 thru_hole circle (at -12.7 -2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 68 thru_hole circle (at -10.16 -2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (model Sockets.3dshapes/PLCC68.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5A942279)
    (at 84.074 50.8)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference "" (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value "" (at 1.27 22.65) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 10.16 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 41.91 85.09) (end 41.91 36.83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.17 85.09) (end 41.91 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.17 36.83) (end 90.17 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.91 36.83) (end 90.17 36.83) (angle 90) (layer Edge.Cuts) (width 0.15))
)
