(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 139)
    (no_connects 0)
    (area 107.5 71.5 257.500001 162.000001)
    (thickness 1.6)
    (drawings 47)
    (tracks 477)
    (zones 0)
    (modules 53)
    (nets 67)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 126 135)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /3.3V)
  (net 3 /5V)
  (net 4 "Net-(C11-Pad1)")
  (net 5 /NRST)
  (net 6 /PC2)
  (net 7 "Net-(D1-Pad1)")
  (net 8 /PC0)
  (net 9 "Net-(D2-Pad1)")
  (net 10 "Net-(D3-Pad1)")
  (net 11 /PC1)
  (net 12 "Net-(D4-Pad1)")
  (net 13 /PC5)
  (net 14 "Net-(D5-Pad2)")
  (net 15 "Net-(D6-Pad2)")
  (net 16 "Net-(D7-Pad2)")
  (net 17 /RGB_OUT)
  (net 18 /I2C1_SCL)
  (net 19 /I2C1_SDA)
  (net 20 /FI2C1_SCL)
  (net 21 /FI2C1_SDA)
  (net 22 /ADC1_IN0)
  (net 23 /ADC2_IN1)
  (net 24 /SWDCLK)
  (net 25 /SWDO)
  (net 26 /SWDIO)
  (net 27 "Net-(P9-Pad7)")
  (net 28 "Net-(U1-Pad2)")
  (net 29 "Net-(U1-Pad3)")
  (net 30 "Net-(U1-Pad4)")
  (net 31 "Net-(U1-Pad5)")
  (net 32 "Net-(U1-Pad6)")
  (net 33 "Net-(U1-Pad11)")
  (net 34 "Net-(U1-Pad16)")
  (net 35 "Net-(U1-Pad17)")
  (net 36 "Net-(U1-Pad24)")
  (net 37 "Net-(U1-Pad26)")
  (net 38 "Net-(U1-Pad27)")
  (net 39 "Net-(U1-Pad29)")
  (net 40 "Net-(U1-Pad39)")
  (net 41 "Net-(U1-Pad40)")
  (net 42 "Net-(U1-Pad41)")
  (net 43 "Net-(U1-Pad44)")
  (net 44 "Net-(U1-Pad45)")
  (net 45 "Net-(U1-Pad50)")
  (net 46 /UART4_TX)
  (net 47 /UART4_RX)
  (net 48 "Net-(U1-Pad53)")
  (net 49 "Net-(U1-Pad54)")
  (net 50 "Net-(U1-Pad56)")
  (net 51 "Net-(U1-Pad57)")
  (net 52 "Net-(U1-Pad61)")
  (net 53 "Net-(U1-Pad62)")
  (net 54 "Net-(P9-Pad8)")
  (net 55 /SPI1_NSS)
  (net 56 /SPI1_SCK)
  (net 57 /SPI1_MISO)
  (net 58 /SPI1_MOSI)
  (net 59 /SPI2_NSS)
  (net 60 /SPI2_SCK)
  (net 61 /SPI2_MISO)
  (net 62 /SPI2_MOSI)
  (net 63 /USART1_TX)
  (net 64 /USART1_RX)
  (net 65 /BOOT0)
  (net 66 /BOOT1)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /ADC1_IN0)
    (add_net /ADC2_IN1)
    (add_net /BOOT0)
    (add_net /BOOT1)
    (add_net /FI2C1_SCL)
    (add_net /FI2C1_SDA)
    (add_net /I2C1_SCL)
    (add_net /I2C1_SDA)
    (add_net /NRST)
    (add_net /PC0)
    (add_net /PC1)
    (add_net /PC2)
    (add_net /PC5)
    (add_net /RGB_OUT)
    (add_net /SPI1_MISO)
    (add_net /SPI1_MOSI)
    (add_net /SPI1_NSS)
    (add_net /SPI1_SCK)
    (add_net /SPI2_MISO)
    (add_net /SPI2_MOSI)
    (add_net /SPI2_NSS)
    (add_net /SPI2_SCK)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /SWDO)
    (add_net /UART4_RX)
    (add_net /UART4_TX)
    (add_net /USART1_RX)
    (add_net /USART1_TX)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(P9-Pad8)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad53)")
    (add_net "Net-(U1-Pad54)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad57)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad61)")
    (add_net "Net-(U1-Pad62)")
  )
  (net_class PWR ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /3.3V)
    (add_net /5V)
    (add_net /GND)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 152.162 112.648)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.9) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 142.764 107.06 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.9 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 142.764 102.742 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 145.05 99.44 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.9 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 151.908 101.472 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer B.Cu) (tedit 0)
    (at 150.622 121.412)
    (attr smd)
    (fp_text reference C6 (at 0 0) (layer B.SilkS))
    (fp_text value 4.7u (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 166.5 78.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 166.5 132 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 130.4 124.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 130.5 78.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer B.Cu) (tedit 0)
    (at 149.622 107.822 180)
    (attr smd)
    (fp_text reference C11 (at 0 0 180) (layer B.SilkS))
    (fp_text value 4.7u (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 130 93.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /NRST))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 129.75 117.25 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /PC2))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 145.558 112.648)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 153.416 117.094 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value Power (at 0 1.55 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 144 117)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value PC0 (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /PC0))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 153.416 120.142 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 5V (at 0 1.55 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 144 120)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45) (layer F.SilkS))
    (fp_text value PC1 (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /PC1))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Common-Parts-Library:LED_WS2812B (layer F.Cu) (tedit 0)
    (at 130.5 128)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference D5 (at -1.9744 -3.3064) (layer F.SilkS))
    (fp_text value RGB1 (at -1.55318 3.30908) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V) (solder_mask_margin 0.2))
    (pad 4 smd rect (at 2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /PC5) (solder_mask_margin 0.2))
    (pad 2 smd rect (at -2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad2)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at 2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.2))
  )
  (module Common-Parts-Library:LED_WS2812B (layer F.Cu) (tedit 0)
    (at 130.5 82.5)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference D6 (at -1.9744 -3.3064) (layer F.SilkS))
    (fp_text value RGB2 (at -1.55318 3.30908) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V) (solder_mask_margin 0.2))
    (pad 4 smd rect (at 2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad2)") (solder_mask_margin 0.2))
    (pad 2 smd rect (at -2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D6-Pad2)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at 2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.2))
  )
  (module Common-Parts-Library:LED_WS2812B (layer F.Cu) (tedit 0)
    (at 166.5 82.5)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference D7 (at -1.9744 -3.3064) (layer F.SilkS))
    (fp_text value RGB3 (at -1.55318 3.30908) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V) (solder_mask_margin 0.2))
    (pad 4 smd rect (at 2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D6-Pad2)") (solder_mask_margin 0.2))
    (pad 2 smd rect (at -2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D7-Pad2)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at 2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.2))
  )
  (module Common-Parts-Library:LED_WS2812B (layer F.Cu) (tedit 0)
    (at 166.5 128)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference D8 (at -1.9744 -3.3064) (layer F.SilkS))
    (fp_text value RGB4 (at -1.55318 3.30908) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V) (solder_mask_margin 0.2))
    (pad 4 smd rect (at 2.45 -1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D7-Pad2)") (solder_mask_margin 0.2))
    (pad 2 smd rect (at -2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /RGB_OUT) (solder_mask_margin 0.2))
    (pad 3 smd rect (at 2.45 1.65 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND) (solder_mask_margin 0.2))
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer B.Cu) (tedit 588DE956)
    (at 138.5 85.5 270)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference P1 (at -4.38 2.27 270) (layer B.SilkS))
    (fp_text value I2C1 (at -4.38 -9.89 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5V))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /I2C1_SCL))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /I2C1_SDA))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer B.Cu) (tedit 588DE956)
    (at 160.5 97 180)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference P2 (at -4.38 2.27 180) (layer B.SilkS))
    (fp_text value FI2C1 (at -4.38 -9.89 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5V))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /FI2C1_SCL))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /FI2C1_SDA))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer B.Cu) (tedit 588DE956)
    (at 151 85.5 270)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference P3 (at -4.38 2.27 270) (layer B.SilkS))
    (fp_text value UART4 (at -4.38 -9.89 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3.3V))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /UART4_RX))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /UART4_TX))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x03_Pitch2.54mm (layer B.Cu) (tedit 588DE956)
    (at 136.5 103.5)
    (descr "Through hole angled socket strip, 1x03, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x03 2.54mm single row")
    (fp_text reference P4 (at -4.38 2.27) (layer B.SilkS))
    (fp_text value ADC1 (at -4.38 -7.35) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3.3V))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /ADC1_IN0))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x03_Pitch2.54mm (layer B.Cu) (tedit 588DE956)
    (at 136.5 113)
    (descr "Through hole angled socket strip, 1x03, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x03 2.54mm single row")
    (fp_text reference P5 (at -4.38 2.27) (layer B.SilkS))
    (fp_text value ADC2 (at -4.38 -7.35) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3.3V))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /ADC2_IN1))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x03_Pitch2.54mm (layer B.Cu) (tedit 588DE956)
    (at 160.5 108.5 180)
    (descr "Through hole angled socket strip, 1x03, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x03 2.54mm single row")
    (fp_text reference P6 (at -4.38 2.27 180) (layer B.SilkS))
    (fp_text value RGB_OUT (at -4.38 -7.35 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5V))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /RGB_OUT))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53261-0371_03x1.25mm_Angled (layer B.Cu) (tedit 57C9972C)
    (at 148.5 130.5 180)
    (descr "Molex PicoBlade, single row, side entry type, surface mount, PN:53261-0371")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference P7 (at 0 3.5 180) (layer B.SilkS))
    (fp_text value Power (at 0 -5 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 1.45 180) (size 0.8 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 0 1.45 180) (size 0.8 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (pad 3 smd rect (at 1.25 1.45 180) (size 0.8 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /5V))
    (pad "" smd rect (at -3.75 -1.45 180) (size 2.2 3.1) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 3.75 -1.45 180) (size 2.2 3.1) (layers B.Cu B.Paste B.Mask))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53261-0371_03x1.25mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 144.5 95 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /BOOT0))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 144.5 97)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /BOOT0))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 142.25 88.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 2k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /I2C1_SCL))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 142.25 88.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.9 180) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 /I2C1_SDA))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 /5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 157.75 100.75 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 2k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /FI2C1_SCL))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 157.75 100.75 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 2k (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 /FI2C1_SDA))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 /5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 157.988 117.094)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 139.25 117 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 157.988 120.142)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 139.25 120 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 139.25 102 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 /NRST))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 139.25 106.75 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.9 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /PC2))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3S-1000 (layer F.Cu) (tedit 56EDA1C6)
    (at 130 99.5 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5 270) (layer F.SilkS))
    (fp_text value Reset (at 0 4.5 270) (layer F.Fab))
    (pad 1 smd rect (at -3.975 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /NRST))
    (pad 1 smd rect (at 3.975 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /NRST))
    (pad 2 smd rect (at -3.975 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 3.975 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_B3S-1000 (layer F.Cu) (tedit 56EDA1C6)
    (at 130 111 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -4.5 270) (layer F.SilkS))
    (fp_text value USER (at 0 4.5 270) (layer F.Fab))
    (pad 1 smd rect (at -3.975 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /PC2))
    (pad 1 smd rect (at 3.975 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /PC2))
    (pad 2 smd rect (at -3.975 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 3.975 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (module Housings_QFP:LQFP-64_10x10mm_Pitch0.5mm placed (layer F.Cu) (tedit 54130A77)
    (at 148.5 105)
    (descr "64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -7.2) (layer F.SilkS))
    (fp_text value STM32F446RETx (at 0 7.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -3.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (pad 2 smd rect (at -5.7 -3.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -5.7 -2.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -5.7 -1.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -5.7 -1.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -5.7 -0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /NRST))
    (pad 8 smd rect (at -5.7 -0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /PC0))
    (pad 9 smd rect (at -5.7 0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /PC1))
    (pad 10 smd rect (at -5.7 0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /PC2))
    (pad 11 smd rect (at -5.7 1.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -5.7 1.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 13 smd rect (at -5.7 2.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (pad 14 smd rect (at -5.7 2.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /ADC1_IN0))
    (pad 15 smd rect (at -5.7 3.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /ADC2_IN1))
    (pad 16 smd rect (at -5.7 3.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at -3.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at -3.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 19 smd rect (at -2.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (pad 20 smd rect (at -2.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 /SPI1_NSS))
    (pad 21 smd rect (at -1.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /SPI1_SCK))
    (pad 22 smd rect (at -1.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 /SPI1_MISO))
    (pad 23 smd rect (at -0.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 /SPI1_MOSI))
    (pad 24 smd rect (at -0.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 0.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /PC5))
    (pad 26 smd rect (at 0.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 1.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 1.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 /BOOT1))
    (pad 29 smd rect (at 2.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 2.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (pad 31 smd rect (at 3.25 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 32 smd rect (at 3.75 5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (pad 33 smd rect (at 5.7 3.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 /SPI2_NSS))
    (pad 34 smd rect (at 5.7 3.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 /SPI2_SCK))
    (pad 35 smd rect (at 5.7 2.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 /SPI2_MISO))
    (pad 36 smd rect (at 5.7 2.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 /SPI2_MOSI))
    (pad 37 smd rect (at 5.7 1.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /FI2C1_SCL))
    (pad 38 smd rect (at 5.7 1.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /FI2C1_SDA))
    (pad 39 smd rect (at 5.7 0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at 5.7 0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad40)"))
    (pad 41 smd rect (at 5.7 -0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at 5.7 -0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 /USART1_TX))
    (pad 43 smd rect (at 5.7 -1.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 /USART1_RX))
    (pad 44 smd rect (at 5.7 -1.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad44)"))
    (pad 45 smd rect (at 5.7 -2.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad45)"))
    (pad 46 smd rect (at 5.7 -2.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /SWDIO))
    (pad 47 smd rect (at 5.7 -3.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 48 smd rect (at 5.7 -3.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (pad 49 smd rect (at 3.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /SWDCLK))
    (pad 50 smd rect (at 3.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad50)"))
    (pad 51 smd rect (at 2.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 /UART4_TX))
    (pad 52 smd rect (at 2.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 /UART4_RX))
    (pad 53 smd rect (at 1.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad53)"))
    (pad 54 smd rect (at 1.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad54)"))
    (pad 55 smd rect (at 0.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /SWDO))
    (pad 56 smd rect (at 0.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad56)"))
    (pad 57 smd rect (at -0.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad57)"))
    (pad 58 smd rect (at -0.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /I2C1_SCL))
    (pad 59 smd rect (at -1.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /I2C1_SDA))
    (pad 60 smd rect (at -1.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 /BOOT0))
    (pad 61 smd rect (at -2.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-Pad61)"))
    (pad 62 smd rect (at -2.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad62)"))
    (pad 63 smd rect (at -3.25 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 64 smd rect (at -3.75 -5.7 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (model Housings_QFP.3dshapes/LQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pkl_samtec:FTSH-105-XX-X-DV (layer F.Cu) (tedit 576E3874)
    (at 153.178 92.328)
    (fp_text reference P9 (at 0 4.5) (layer F.Fab))
    (fp_text value JTAG-10 (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at 2.54 -2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /3.3V))
    (pad 2 smd rect (at 2.54 2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 26 /SWDIO))
    (pad 3 smd rect (at 1.27 -2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at 1.27 2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /SWDCLK))
    (pad 5 smd rect (at 0 -2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at 0 2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 25 /SWDO))
    (pad 7 smd rect (at -1.27 -2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P9-Pad7)"))
    (pad 8 smd rect (at -1.27 2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(P9-Pad8)"))
    (pad 9 smd rect (at -2.54 -2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 10 smd rect (at -2.54 2 180) (size 0.74 2.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /NRST))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 156.988 106.044)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P8 (at 0 -2.39) (layer F.SilkS))
    (fp_text value UART1 (at 0 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3.3V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /USART1_RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /USART1_TX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x06_Pitch2.54mm (layer F.Cu) (tedit 588DE956)
    (at 142.24 124.714 90)
    (descr "Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x06 2.54mm single row")
    (fp_text reference P10 (at -4.38 -2.27 90) (layer F.SilkS))
    (fp_text value SPI1 (at -4.38 14.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3.3V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /SPI1_NSS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /SPI1_SCK))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /SPI1_MISO))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /SPI1_MOSI))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 149.9 104.2)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 1.45) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 66 /BOOT1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 149.9 105.7)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 1.45) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 66 /BOOT1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 136 129.1)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at 0 1.75) (layer B.SilkS))
    (fp_text value 1u (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /5V))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 141 131 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 136.5 132.4 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 2.5 180) (layer B.SilkS))
    (fp_text value MCP1700T-3002E/TT (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 /3.3V))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 /5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 161.1 124.4 270)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 4.315 -2.27 270) (layer F.SilkS))
    (fp_text value 5V (at 4.315 4.81 270) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text USER (at 128.7 119) (layer F.SilkS))
  (gr_text RESET (at 137.1 95.4) (layer F.SilkS))
  (gr_text ADC1-0 (at 139.8 98.4) (layer F.SilkS))
  (gr_text 3 (at 138.8 101.1) (layer F.SilkS))
  (gr_text ADC2-1 (at 139.8 107.8) (layer F.SilkS))
  (gr_text 3 (at 138.9 110.5) (layer F.SilkS))
  (gr_text MISO (at 152.4 122.7 90) (layer F.SilkS))
  (gr_text MOSI (at 154.9 122.7 90) (layer F.SilkS))
  (gr_text SCK (at 150 122.2 90) (layer F.SilkS))
  (gr_text NSS (at 147.4 122.2 90) (layer F.SilkS))
  (gr_text 3 (at 144.8 123) (layer F.SilkS))
  (gr_text TX (at 154.2 113.6) (layer F.SilkS))
  (gr_text RX (at 154.2 111.2) (layer F.SilkS))
  (gr_text 3 (at 154.6 109.7) (layer F.SilkS))
  (gr_text 5 (at 163.2 99.7) (layer F.SilkS))
  (gr_text SDA (at 146.1 81.6 90) (layer F.SilkS))
  (gr_text SCL (at 143.7 81.5 90) (layer F.SilkS))
  (gr_text 5 (at 141.1 82.6) (layer F.SilkS))
  (gr_text 3 (at 153.5 82.6) (layer F.SilkS))
  (gr_text 5 (at 163.1 111.2) (layer F.SilkS))
  (gr_text T (at 158.6 82.6) (layer F.SilkS))
  (gr_text R (at 156 82.6) (layer F.SilkS))
  (gr_text SDA (at 164 105) (layer F.SilkS))
  (gr_text SCL (at 164 102) (layer F.SilkS))
  (gr_text "5 3 -" (at 148.844 126.492 180) (layer B.SilkS))
  (gr_text ADC1_IN0 (at 131.75 95.25) (layer B.SilkS))
  (gr_text ADC2_IN1 (at 131.75 116.25) (layer B.SilkS))
  (gr_text RGB (at 164.7 113.6) (layer F.SilkS))
  (gr_text FI2C1 (at 165.7 94.2) (layer F.SilkS))
  (gr_text UART4 (at 156.2 76.8) (layer F.SilkS))
  (gr_text I2C1 (at 144.1 76.9) (layer F.SilkS))
  (dimension 22.5 (width 0.3) (layer Dwgs.User)
    (gr_text "22.500 mm" (at 137.25 137.85) (layer Dwgs.User))
    (feature1 (pts (xy 148.5 135) (xy 148.5 139.2)))
    (feature2 (pts (xy 126 135) (xy 126 139.2)))
    (crossbar (pts (xy 126 136.5) (xy 148.5 136.5)))
    (arrow1a (pts (xy 148.5 136.5) (xy 147.373496 137.086421)))
    (arrow1b (pts (xy 148.5 136.5) (xy 147.373496 135.913579)))
    (arrow2a (pts (xy 126 136.5) (xy 127.126504 137.086421)))
    (arrow2b (pts (xy 126 136.5) (xy 127.126504 135.913579)))
  )
  (dimension 45 (width 0.3) (layer Dwgs.User)
    (gr_text "45.000 mm" (at 148.5 146.35) (layer Dwgs.User))
    (feature1 (pts (xy 171 135) (xy 171 147.7)))
    (feature2 (pts (xy 126 135) (xy 126 147.7)))
    (crossbar (pts (xy 126 145) (xy 171 145)))
    (arrow1a (pts (xy 171 145) (xy 169.873496 145.586421)))
    (arrow1b (pts (xy 171 145) (xy 169.873496 144.413579)))
    (arrow2a (pts (xy 126 145) (xy 127.126504 145.586421)))
    (arrow2b (pts (xy 126 145) (xy 127.126504 144.413579)))
  )
  (dimension 5 (width 0.3) (layer Dwgs.User)
    (gr_text "5.000 mm" (at 123.4 102.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 126.5 100) (xy 122.05 100)))
    (feature2 (pts (xy 126.5 105) (xy 122.05 105)))
    (crossbar (pts (xy 124.75 105) (xy 124.75 100)))
    (arrow1a (pts (xy 124.75 100) (xy 125.336421 101.126504)))
    (arrow1b (pts (xy 124.75 100) (xy 124.163579 101.126504)))
    (arrow2a (pts (xy 124.75 105) (xy 125.336421 103.873496)))
    (arrow2b (pts (xy 124.75 105) (xy 124.163579 103.873496)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 121.65 90 270) (layer Dwgs.User))
    (feature1 (pts (xy 126 105) (xy 120.3 105)))
    (feature2 (pts (xy 126 75) (xy 120.3 75)))
    (crossbar (pts (xy 123 75) (xy 123 105)))
    (arrow1a (pts (xy 123 105) (xy 122.413579 103.873496)))
    (arrow1b (pts (xy 123 105) (xy 123.586421 103.873496)))
    (arrow2a (pts (xy 123 75) (xy 122.413579 76.126504)))
    (arrow2b (pts (xy 123 75) (xy 123.586421 76.126504)))
  )
  (gr_circle (center 163.7511 89.7536) (end 165.3511 89.7536) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 163.7511 120.2536) (end 165.3511 120.2536) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 133.2511 120.2536) (end 134.8511 120.2536) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 133.2511 89.7536) (end 134.8511 89.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.0011 135.0036) (end 131.0011 135.0036) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 166.0011 130.0036) (end 166.0011 135.0036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.0011 130.0036) (end 126.0011 130.0036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.0011 80.0036) (end 171.0011 130.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.0011 130.0036) (end 126.0011 80.0036) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 166.0011 80.0036) (end 171.0011 80.0036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.0011 80.0036) (end 131.0011 75.0036) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.0011 75.0036) (end 166.0011 75.0036) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 257.5 162) (xy 107.5 162) (xy 107.5 71.5) (xy 257.5 71.5)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.249)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 257.5 162) (xy 107.5 162) (xy 107.5 71.5) (xy 257.5 71.5)
      )
    )
  )
)
