(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 55)
    (zones 0)
    (modules 18)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +24V)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D3-Pad2)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J4-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J4-Pad2)")
  )
  (module KiCad/Resistors_SMD.pretty:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 145.828 84.709)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -0.032 -1.778) (layer F.SilkS))
    (fp_text value R220k (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Diodes_ThroughHole.pretty:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5877C982)
    (at 147.701 63.754 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D4 (at 5.08 -0.127 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.08 2.41 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Diodes_ThroughHole.pretty:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5877C982)
    (at 147.701 99.949 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.08 2.41 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +24V))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module apexelectrix/apex-screw-terminals.pretty:Screw_Terminal_1x02 (layer F.Cu) (tedit 54C93B6B)
    (at 132.842 81.661 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0 -3.5 270) (layer F.SilkS) hide)
    (fp_text value "PWR IN" (at 0.5 3.5 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 0 270) (size 4 4) (drill 1.75) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 4 4) (drill 1.75) (layers *.Cu *.Mask F.SilkS)
      (net 1 +24V))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 145.701 95.631 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0.032 -1.905 180) (layer F.SilkS))
    (fp_text value R1K (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +24V))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 145.828 78.486)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -0.032 1.905) (layer F.SilkS))
    (fp_text value R220k (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 145.701 67.691 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value R1K (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +24V))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5C2FD2B4)
    (at 153.797 96.266 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J3 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value "Fan 1" (at -0.635 -3.683 270) (layer F.SilkS))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5C2FD289)
    (at 153.797 65.024 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J5 (at 1.25 -3.5 270) (layer F.SilkS) hide)
    (fp_text value "Fan 2" (at -0.635 -3.683 270) (layer F.SilkS))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 +24V))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Diodes_SMD.pretty:D_1206 (layer F.Cu) (tedit 587F7EF9)
    (at 138.43 95.631)
    (descr "Diode SMD 1206, reflow soldering")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D1 (at 0 1.905) (layer F.SilkS))
    (fp_text value LED (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (module KiCad/Diodes_SMD.pretty:D_1206 (layer F.Cu) (tedit 587F7EF9)
    (at 138.43 67.691)
    (descr "Diode SMD 1206, reflow soldering")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D3 (at -0.024 -1.778) (layer F.SilkS))
    (fp_text value LED (at 0 2.3) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B2B-PH-K_02x2.00mm_Straight (layer F.Cu) (tedit 5C309D60)
    (at 154.432 87.884 270)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J2 (at 1.5 -2.8 270) (layer F.SilkS) hide)
    (fp_text value "Sig 1" (at -0.508 -3.048 270) (layer F.SilkS))
    (fp_text user %R (at 1 1.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (model Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Connectors_JST.pretty:JST_PH_B2B-PH-K_02x2.00mm_Straight (layer F.Cu) (tedit 5C309D71)
    (at 154.432 73.787 270)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J4 (at 1.5 -2.8 270) (layer F.SilkS) hide)
    (fp_text value "Sig 2" (at -0.381 -3.048 270) (layer F.SilkS))
    (fp_text user %R (at 1 1.5 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GND))
    (model Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Mounting_Holes.pretty:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C30A185)
    (at 132.08 65.405)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module KiCad/Mounting_Holes.pretty:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C30A18D)
    (at 132.08 98.425)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module KiCad/Mounting_Holes.pretty:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C30A17E)
    (at 154.686 81.788)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module KiCad/TO_SOT_Packages_SMD.pretty:TO-252-2Lead (layer F.Cu) (tedit 58879E1B)
    (at 141.715 90.414)
    (descr TO-252-2Lead)
    (attr smd)
    (fp_text reference Q1 (at -6.604 0 90) (layer F.SilkS))
    (fp_text value SUD50N04 (at 0.25 4.81) (layer F.Fab))
    (pad 2 smd rect (at 3.7 0.01 270) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at -3.7 2.29 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -3.7 -2.29 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes\TO-252-2Lead.wrl
      (offset (xyz -3.499999947435274 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiCad/TO_SOT_Packages_SMD.pretty:TO-252-2Lead (layer F.Cu) (tedit 58879E1B)
    (at 141.732 72.898)
    (descr TO-252-2Lead)
    (attr smd)
    (fp_text reference Q2 (at -6.477 0 90) (layer F.SilkS))
    (fp_text value SUD50N04 (at 0.25 4.81) (layer F.Fab))
    (pad 1 smd rect (at -3.7 -2.29 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J4-Pad2)"))
    (pad 3 smd rect (at -3.7 2.29 270) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 3.7 0.01 270) (size 7 7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes\TO-252-2Lead.wrl
      (offset (xyz -3.499999947435274 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 158.75 102.108) (end 158.75 61.595) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 102.108) (end 158.75 102.108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 61.595) (end 128.27 102.108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 61.595) (end 128.27 61.595) (layer Edge.Cuts) (width 0.15))
  (gr_text "+\n" (at 157.48 98.679) (layer F.SilkS))
  (gr_text "+\n" (at 157.48 90.424) (layer F.SilkS))
  (gr_text "+\n" (at 157.48 76.2) (layer F.SilkS))
  (gr_text "+\n" (at 157.48 67.437) (layer F.SilkS))
  (gr_text "+\n" (at 129.667 87.503) (layer F.SilkS))
  (gr_text - (at 129.667 75.565 90) (layer F.SilkS))
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 102.108) (xy 158.75 61.595) (xy 128.27 61.595) (xy 128.27 102.108)
      )
    )
  )
  (zone (net 1) (net_name +24V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 61.595) (xy 158.75 61.595) (xy 158.75 102.108) (xy 128.27 102.108)
      )
    )
  )
)
