(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 17)
    (no_connects 0)
    (area 115.899999 89.399999 161.100001 109.600001)
    (thickness 1.6)
    (drawings 14)
    (tracks 77)
    (zones 0)
    (modules 10)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad2)")
  (net 3 "Net-(R1-Pad2)")
  (net 4 /IN)
  (net 5 /ToCoil)
  (net 6 /OUT)
  (net 7 /ENABLE)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ENABLE)
    (add_net /IN)
    (add_net /OUT)
    (add_net /ToCoil)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EF001A)
    (at 141.8 104.3 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.5 1.6 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 -2.7 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /IN))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EF0037)
    (at 150.95 100.35 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.1 0.05 360) (layer F.SilkS))
    (fp_text value 100nF (at -0.3 -2.2 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /ToCoil))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58EF000C)
    (at 132.65 98.65 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 4.15 -0.1 180) (layer F.SilkS))
    (fp_text value 47uF (at 0.15 -1.95 90) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /OUT))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EF0026)
    (at 142.9 90.95)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.05 -3) (layer F.SilkS) hide)
    (fp_text value 55k (at -2.5 0.05) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /OUT))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EF002F)
    (at 147 91)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0.9 -3.05) (layer F.SilkS) hide)
    (fp_text value 10k (at 3 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58EF0020)
    (at 147.45 104.25)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0.15 2.8) (layer F.SilkS))
    (fp_text value TPS563200 (at -11.65 3.8) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /ToCoil))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /IN))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad2)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /ENABLE))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:1X02 (layer F.Cu) (tedit 58EEFF9A)
    (at 128 104.15 270)
    (fp_text reference J1 (at 0.3 0 270) (layer Eco1.User) hide)
    (fp_text value 9V-IN (at 2.05 2.4 270) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /IN))
  )
  (module freetronics_footprints:1X02 (layer F.Cu) (tedit 58EEFFC2)
    (at 157.2 100.75 90)
    (fp_text reference J2 (at 0.3 0 90) (layer Eco1.User) hide)
    (fp_text value EN (at 1.4 1.8 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /ENABLE))
  )
  (module freetronics_footprints:1X02 (layer F.Cu) (tedit 58EEFF83)
    (at 128 93.05 270)
    (fp_text reference J3 (at 0.3 0 270) (layer Eco1.User) hide)
    (fp_text value 5V-OUT (at 0.95 2.8 270) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /OUT))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "My Libraries:KT-MPLCH-0740-Hand" (layer F.Cu) (tedit 58EFD78D)
    (at 142.4 96.6 180)
    (fp_text reference L-KEMET1 (at -1.99 -4.45 180) (layer F.SilkS))
    (fp_text value 33uH (at 4.9 4.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.32 0 180) (size 3 3.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /ToCoil))
    (pad 2 smd rect (at 3.07 0 180) (size 3 3.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /OUT))
  )
  (gr_text "james@baldengineer.com\nRetroPie Switcher Proto 1" (at 117.1 100.2) (layer F.SilkS))
  (gr_text EN (at 159.2 98.1 90) (layer F.SilkS))
  (gr_text <12V (at 125 106.9) (layer F.SilkS))
  (gr_text 5V (at 125.5 93) (layer F.SilkS))
  (gr_text GND (at 158.7 102.7) (layer B.SilkS))
  (gr_text GND (at 128 102.1) (layer B.SilkS))
  (gr_text GND (at 128 97.8) (layer B.SilkS))
  (gr_text GND (at 158.6 102.6) (layer F.SilkS))
  (gr_text GND (at 128 102 180) (layer F.SilkS))
  (gr_text GND (at 128 97.8) (layer F.SilkS))
  (gr_line (start 116 109.5) (end 116 89.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 161 109.5) (end 116 109.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 161 89.5) (end 161 109.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 116 89.5) (end 161 89.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (zone (net 6) (net_name /OUT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.9 91.8) (xy 142.1 91.8) (xy 142 101.4) (xy 136.1 101.4) (xy 136.1 98.2)
        (xy 130.2 98.2) (xy 130.2 94.3) (xy 126.3 94.3) (xy 126.3 90.1) (xy 142.9 90.1)
      )
    )
  )
  (zone (net 6) (net_name /OUT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.9 91.8) (xy 142.1 91.8) (xy 142 101.4) (xy 136.1 101.4) (xy 136.1 98.2)
        (xy 130.2 98.2) (xy 130.2 94.3) (xy 126.3 94.3) (xy 126.3 90.1) (xy 142.9 90.1)
      )
    )
  )
  (zone (net 5) (net_name /ToCoil) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.4 100.1) (xy 149.3 100.1) (xy 149.3 101.4) (xy 143.2 101.4) (xy 143.2 92.6)
        (xy 152.4 92.6)
      )
    )
  )
  (zone (net 5) (net_name /ToCoil) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.4 100.1) (xy 149.3 100.1) (xy 149.3 101.4) (xy 147.4 101.4) (xy 147.4 104.7)
        (xy 143.2 104.7) (xy 143.2 92.6) (xy 152.4 92.6)
      )
    )
  )
  (zone (net 4) (net_name /IN) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.9 105) (xy 147.4 105) (xy 147.4 109) (xy 126.5 109) (xy 126.4 105.5)
        (xy 131.6 105.5) (xy 131.6 104.6) (xy 142.9 104.6)
      )
    )
  )
  (zone (net 4) (net_name /IN) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.9 105) (xy 147.4 105) (xy 147.4 109) (xy 126.5 109) (xy 126.4 105.5)
        (xy 131.6 105.5) (xy 131.6 104.6) (xy 142.9 104.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.6 90) (xy 160.5 90) (xy 160.5 109) (xy 116.5 109.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 108.9) (xy 116.6 109.1) (xy 116.6 90.1) (xy 160.5 90.1)
      )
    )
  )
)
