(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 10)
    (no_connects 0)
    (area 136.4772 104.064999 155.124 119.455001)
    (thickness 1.6)
    (drawings 6)
    (tracks 82)
    (zones 0)
    (modules 2)
    (nets 11)
  )
  (page USLetter)
  (title_block
    (title "IDC 0.1 to 0.05 10 Pin Adapter")
    (date 2017-11-08)
    (rev 1.0)
    (company "Sid Price Design")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFCFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad5)")
  (net 4 "Net-(J1-Pad7)")
  (net 5 "Net-(J1-Pad9)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J1-Pad4)")
  (net 8 "Net-(J1-Pad6)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module Connectors_Samtec:SDL-110-X-XX_2x05 (layer F.Cu) (tedit 590274CA)
    (at 139.6746 106.9848)
    (descr "Double row, low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht dual")
    (fp_text reference J1 (at -2.27 5.08 90) (layer F.SilkS))
    (fp_text value "0.1\" Pitch" (at 4.81 5.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 0 5.08) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 7 thru_hole circle (at 0 7.62) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 9 thru_hole circle (at 0 10.16) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad9)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 6 thru_hole circle (at 2.54 5.08) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 8 thru_hole circle (at 2.54 7.62) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 10 thru_hole circle (at 2.54 10.16) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SDL-110-X-XX_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module IDC_10_Adapter:Conn_02x05_0.05 (layer F.Cu) (tedit 5A0344B8)
    (at 150.5966 114.2492 90)
    (descr "10Pin IDC conn 0.05 pitch")
    (tags "connector idc 0.05")
    (fp_text reference J2 (at 2.5 3.5 90) (layer F.SilkS))
    (fp_text value "0.05\" Pitch" (at 2.5 -4.3 90) (layer F.Fab))
    (fp_text user %R (at 2.5 -0.625 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at 1.25 0 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 2.5 0 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 7 thru_hole circle (at 3.75 0 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 9 thru_hole circle (at 5 0 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad9)"))
    (pad 2 thru_hole circle (at 0 -1.25 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 1.25 -1.25 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 6 thru_hole circle (at 2.5 -1.25 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 8 thru_hole circle (at 3.75 -1.25 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 10 thru_hole circle (at 5 -1.25 90) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Connectors_Harwin.3dshapes/Harwin_Gecko-G125-MVX1005L0X_2x05x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "IDC Adapter v1.0" (at 148.844 106.172) (layer F.SilkS))
  (gr_text "Sid Price Design" (at 148.844 104.902) (layer F.SilkS))
  (gr_line (start 137.16 119.38) (end 137.16 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.178 119.38) (end 137.16 119.38) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.178 104.14) (end 154.178 119.38) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 104.14) (end 154.178 104.14) (layer Edge.Cuts) (width 0.15))
)
