(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 167)
    (no_connects 0)
    (area 29.114287 35.4 171.600001 131.650001)
    (thickness 1.6)
    (drawings 19)
    (tracks 1321)
    (zones 0)
    (modules 63)
    (nets 76)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +3V3)
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 "Net-(C5-Pad2)")
  (net 9 "Net-(C6-Pad2)")
  (net 10 "Net-(C7-Pad2)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(C11-Pad1)")
  (net 13 +24V)
  (net 14 "Net-(D1-Pad1)")
  (net 15 "Net-(D1-Pad3)")
  (net 16 "Net-(D2-Pad1)")
  (net 17 "Net-(D2-Pad2)")
  (net 18 "Net-(J1-Pad1)")
  (net 19 "Net-(J1-Pad2)")
  (net 20 "Net-(J1-Pad3)")
  (net 21 "Net-(J1-Pad4)")
  (net 22 "Net-(J1-Pad5)")
  (net 23 "Net-(J1-Pad6)")
  (net 24 "Net-(J1-Pad7)")
  (net 25 "Net-(J1-Pad8)")
  (net 26 /ETH1_TX+)
  (net 27 /ETH1_TX-)
  (net 28 /ETH1_RX+)
  (net 29 /ETH1_RX-)
  (net 30 "Net-(J2-Pad9)")
  (net 31 /ETH1_LED)
  (net 32 /DCD)
  (net 33 /RXD)
  (net 34 /TXD)
  (net 35 /DTR)
  (net 36 /CTS)
  (net 37 /RTS)
  (net 38 /DSR)
  (net 39 "Net-(J5-Pad2)")
  (net 40 "Net-(J5-Pad10)")
  (net 41 /SBB_DATA2+)
  (net 42 /SBB_DATA2-)
  (net 43 /ETH0_TX+)
  (net 44 /ETH0_TX-)
  (net 45 /ETH0_RX+)
  (net 46 /ETH0_RX-)
  (net 47 /ETH_PWR+)
  (net 48 /ETH_PWR-)
  (net 49 "Net-(J8-Pad9)")
  (net 50 /ETH0_LED)
  (net 51 "Net-(J8-Pad11)")
  (net 52 /WLAN_LED)
  (net 53 /Omega_RX)
  (net 54 /Omega_TX)
  (net 55 /I2C_SCL)
  (net 56 /G19)
  (net 57 /I2C_SDA)
  (net 58 /G18)
  (net 59 "Net-(R1-Pad1)")
  (net 60 "Net-(R2-Pad1)")
  (net 61 "Net-(R7-Pad2)")
  (net 62 /USB+)
  (net 63 /USB-)
  (net 64 /RS485_TXEN2)
  (net 65 /UART_TX2)
  (net 66 /UART_RX2)
  (net 67 /UART_RX1)
  (net 68 /UART_TX1)
  (net 69 /HS_IN)
  (net 70 /HS_OUT)
  (net 71 "Net-(C8-Pad1)")
  (net 72 "Net-(C16-Pad1)")
  (net 73 /VBUS)
  (net 74 /PPoE+)
  (net 75 /USBPWR)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CTS)
    (add_net /DCD)
    (add_net /DSR)
    (add_net /DTR)
    (add_net /ETH0_LED)
    (add_net /ETH0_RX+)
    (add_net /ETH0_RX-)
    (add_net /ETH0_TX+)
    (add_net /ETH0_TX-)
    (add_net /ETH1_LED)
    (add_net /ETH1_RX+)
    (add_net /ETH1_RX-)
    (add_net /ETH1_TX+)
    (add_net /ETH1_TX-)
    (add_net /G18)
    (add_net /G19)
    (add_net /HS_IN)
    (add_net /HS_OUT)
    (add_net /I2C_SCL)
    (add_net /I2C_SDA)
    (add_net /Omega_RX)
    (add_net /Omega_TX)
    (add_net /RS485_TXEN2)
    (add_net /RTS)
    (add_net /RXD)
    (add_net /SBB_DATA2+)
    (add_net /SBB_DATA2-)
    (add_net /TXD)
    (add_net /UART_RX1)
    (add_net /UART_RX2)
    (add_net /UART_TX1)
    (add_net /UART_TX2)
    (add_net /USB+)
    (add_net /USB-)
    (add_net /WLAN_LED)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J8-Pad11)")
    (add_net "Net-(J8-Pad9)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R7-Pad2)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +3V3)
    (add_net /ETH_PWR+)
    (add_net /ETH_PWR-)
    (add_net /PPoE+)
    (add_net /VBUS)
    (add_net GND)
  )
  (net_class PowerSmall ""
    (clearance 0.15)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /USBPWR)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2C92)
    (at 121.7 79.8 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -4.274 -0.034 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2C54)
    (at 103.1 86 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -4.17 0.024 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 75.3 81.6 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2BF6)
    (at 90.4 92.1 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -2.184 2.008 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2C08)
    (at 95.1 89.2 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 2.136 -1.986 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2BF1)
    (at 97.6 91.8 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -4.254 0.106 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2BFF)
    (at 90.4 100.9 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at -4.256 0.024 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 130 75.8)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2BD5)
    (at 109.9 104.1)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at -4.236 -0.214 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2C5C)
    (at 99.9 86 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 4.72 1.192 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2C27)
    (at 83.4 86 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at -4.17 0.166 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 77.2 115.8)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 591A2C14)
    (at 76.4 102.8)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C13 (at -2.486 3.88 90) (layer F.SilkS))
    (fp_text value "10uF 50VDC" (at 1.25 4.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +24V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 154.5 96.3)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at 0 1.75) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 591A2C1C)
    (at 76.4 93.6)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C15 (at -2.74 3.682 90) (layer F.SilkS))
    (fp_text value "22uF 25V" (at 1.25 4.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2C9B)
    (at 124.6 76 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 1.832 -2.172 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2CF7)
    (at 144.5 75 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at -0.07 -0.026 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 154.4 86.6)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 0 1.75) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 132 89.3 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C19 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-3 (layer B.Cu) (tedit 591A2DFE)
    (at 108.2 94.4 90)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-59EGC(Ver.17A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins")
    (fp_text reference D1 (at 2.706 -4.06 90) (layer B.SilkS))
    (fp_text value "Everlight 339-1SURSYGW/S530-A3" (at 2.54 -3.96 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad3)"))
    (model LEDs.3dshapes/LED_D5.0mm-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 591A2BBC)
    (at 121.3 106.9)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D2 (at 5.446 0.034 90) (layer F.SilkS))
    (fp_text value DO-214AA (at 0 3) (layer F.Fab))
    (fp_text user %R (at 0 -3) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 591A2BB4)
    (at 121.4 102.2 180)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D3 (at 5.576 0.092 270) (layer F.SilkS))
    (fp_text value DO-214AA (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 591A2BAC)
    (at 121.3 111.5)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D4 (at 5.446 0.006 90) (layer F.SilkS))
    (fp_text value DO-214AA (at 0 3) (layer F.Fab))
    (fp_text user %R (at 0 -3) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer B.Cu) (tedit 591A2B53)
    (at 160.5 68.7 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D5 (at 3.168 -2.512 90) (layer B.SilkS))
    (fp_text value STPS1L30A (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at -5.722 0.282 180) (layer B.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 13 +24V))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 75 /USBPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 591A2CB3)
    (at 138.1 75.9 180)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D6 (at 2.718 2.494 180) (layer F.SilkS))
    (fp_text value STPS1L30A (at 0 2.6 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 180) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 +24V))
    (pad 2 smd rect (at 2.5 0 180) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 74 /PPoE+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 591A2B8F)
    (at 150 114 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at -2.908 -0.046 180) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 1.27 9.95 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:USB_A (layer F.Cu) (tedit 5543E289)
    (at 132.6 110.7)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J4 (at 0 -2.35) (layer F.SilkS))
    (fp_text value USB_A (at 3.84 7.44) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 73 /VBUS))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 591A2E22)
    (at 86.9 103.3 180)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J5 (at 0.032 -2.364 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 1.27 12.49 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /DCD))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /DTR))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad10)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /DSR))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /CTS))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad2)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RTS))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad10)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 591A2AD3)
    (at 78.5 73.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 591A2AB0)
    (at 156 73.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 591A2AC4)
    (at 78.75 110.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH3 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 591A2ABA)
    (at 156 110.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH4 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 591A2B96)
    (at 147.4 117.2 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P1 (at -0.148 -2.62 90) (layer F.SilkS))
    (fp_text value FDI_Cable (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /Omega_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /Omega_TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 591A2BA4)
    (at 118.5 117.7 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P2 (at -0.41 -2.422 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /I2C_SCL))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /G19))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /I2C_SDA))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /G18))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 591A2A87)
    (at 77 66 270)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference P3 (at 0.04 -2.756 270) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 1.27 4.87 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /PPoE+))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /ETH_PWR+))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /ETH_PWR-))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591A2BCD)
    (at 110 100.7 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 4.082 0.116 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591A2BC6)
    (at 110 97.7 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 4.082 -0.09 270) (layer F.SilkS))
    (fp_text value 1k2 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 591A2C87)
    (at 116.8 85 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.392 0.04 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /ETH1_TX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 113.2 85 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /ETH1_TX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 591A2C72)
    (at 109.7 85 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.392 0.028 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /ETH1_RX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 591A2C77)
    (at 106.3 85 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.392 -0.128 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /ETH1_RX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 118.4 97.8)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 112.3 72.1 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 1.85 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J2-Pad9)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 141 106.3 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 62 /USB+))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591A2B85)
    (at 160.7 108 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at -2.336 2.204 270) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 63 /USB-))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 96.8 85 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /ETH0_TX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 93.2 85 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /ETH0_TX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 89.9 85.2 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /ETH0_RX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 591A2C2F)
    (at 86.3 85.1 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at -3.292 0.06 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 /ETH0_RX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591A2CDC)
    (at 144.4 67.7 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at -0.372 1.904 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 64 /RS485_TXEN2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 591A2E59)
    (at 93.4 71.6 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at -4.036 -0.58 360) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J8-Pad9)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 591A2E54)
    (at 89.9 71.6 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R17 (at -4.036 -0.524 360) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(J8-Pad11)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h4.3mm (layer B.Cu) (tedit 591A2E06)
    (at 120.4 89.6 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at -2.536 -2.348 270) (layer B.SilkS))
    (fp_text value "Omron PB" (at 3.75 -6.7 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 0 -4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 6.5 -4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h4.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 591A2B18)
    (at 149 74 180)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at -3.654 -3.216 180) (layer F.SilkS))
    (fp_text value ADM3485E (at 0 1.27 180) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 42 /SBB_DATA2-))
    (pad 6 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 41 /SBB_DATA2+))
    (pad 5 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 65 /UART_TX2))
    (pad 3 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 64 /RS485_TXEN2))
    (pad 2 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 66 /UART_RX2))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 591A2B57)
    (at 160.5 68.8 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D7 (at -0.034 -2.512 90) (layer F.SilkS))
    (fp_text value STPS1L30A (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 73 /VBUS))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 75 /USBPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 96.52 99.06)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6) (layer F.SilkS))
    (fp_text value MAX3232 (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C7-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J5-Pad10)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J5-Pad2)"))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 /HS_IN))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 /HS_OUT))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 /UART_TX1))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 /UART_RX1))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /RXD))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /TXD))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:HLJ-6115ANL (layer F.Cu) (tedit 593D6FCE)
    (at 112.2 71.6)
    (descr "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (tags "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (attr virtual)
    (fp_text reference J2 (at -10.6 -2.512 90) (layer F.SilkS))
    (fp_text value HLJ-6115ANL (at -1.4 -8.75) (layer F.Fab))
    (pad "" np_thru_hole circle (at 4.45 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 3.15468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 26 /ETH1_TX+))
    (pad 2 thru_hole circle (at 1.88468 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 27 /ETH1_TX-))
    (pad 3 thru_hole circle (at 0.61468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 28 /ETH1_RX+))
    (pad 4 thru_hole circle (at -0.65278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 71 "Net-(C8-Pad1)"))
    (pad 5 thru_hole circle (at -1.92278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 71 "Net-(C8-Pad1)"))
    (pad 6 thru_hole circle (at -3.19278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 29 /ETH1_RX-))
    (pad 7 thru_hole circle (at -4.46278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad 8 thru_hole circle (at -5.73278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad 9 thru_hole circle (at 5.36956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 30 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at 2.82956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 31 /ETH1_LED))
    (pad 11 thru_hole circle (at -5.32892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad 12 thru_hole circle (at -7.86892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad S1 thru_hole circle (at 6.477 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad S2 thru_hole circle (at -9.017 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -6.95 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module plan44:DB9-MALE-20x30mm (layer F.Cu) (tedit 591A03FB)
    (at 93.5 107.7 180)
    (descr "Connecteur DB9 male couche")
    (tags "CONN DB9")
    (fp_text reference J3 (at -5.3 -9.3 180) (layer F.SilkS))
    (fp_text value DB9_MALE (at -5.3 -4.5 180) (layer F.Fab))
    (pad "" thru_hole circle (at 7.25 -1.525 180) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -18.175 -1.5 180) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 /DCD))
    (pad 2 thru_hole circle (at -2.79 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 /RXD))
    (pad 3 thru_hole circle (at -5.59 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 /TXD))
    (pad 4 thru_hole circle (at -8.25 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 /DTR))
    (pad 5 thru_hole circle (at -11.05 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at -9.65 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -6.86 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 /CTS))
    (pad 7 thru_hole circle (at -4.19 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 /RTS))
    (pad 6 thru_hole circle (at -1.4 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 /DSR))
    (model Connectors.3dshapes/DB9MC.wrl
      (at (xyz -0.22 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:USB_Micro-B-SMD (layer F.Cu) (tedit 591A0D4E)
    (at 151.7 66.7 180)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (clearance 0.18)
    (attr smd)
    (fp_text reference J6 (at 0 -3.24 180) (layer F.SilkS))
    (fp_text value USB_Micro_AB (at 0 5.3 180) (layer F.Fab))
    (pad 6 thru_hole circle (at -2.25 -1.65 180) (size 1.1 1.1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.3 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 75 /USBPWR))
    (pad 2 smd rect (at -0.65 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -4.15 1.4 270) (size 1.55 1.55) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 4.25 1.4 270) (size 1.55 1.55) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.25 -1.65 180) (size 1.1 1.1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module plan44:STELVIO-4P-508 (layer F.Cu) (tedit 58131576)
    (at 123.9 70.3)
    (attr virtual)
    (fp_text reference J7 (at -4.064 0 90) (layer F.SilkS))
    (fp_text value SBB (at 7.62 -11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 13 +24V))
    (pad 2 thru_hole circle (at 10.16 0) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 41 /SBB_DATA2+))
    (pad 4 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 42 /SBB_DATA2-))
  )
  (module plan44:HLJ-6115ANL (layer F.Cu) (tedit 593D6FCE)
    (at 93 71.6)
    (descr "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (tags "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (attr virtual)
    (fp_text reference J8 (at -10.6 -2.512 90) (layer F.SilkS))
    (fp_text value HLJ-6115ANL (at -1.4 -8.75) (layer F.Fab))
    (pad "" np_thru_hole circle (at 4.45 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 3.15468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 43 /ETH0_TX+))
    (pad 2 thru_hole circle (at 1.88468 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 44 /ETH0_TX-))
    (pad 3 thru_hole circle (at 0.61468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 45 /ETH0_RX+))
    (pad 4 thru_hole circle (at -0.65278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 72 "Net-(C16-Pad1)"))
    (pad 5 thru_hole circle (at -1.92278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 72 "Net-(C16-Pad1)"))
    (pad 6 thru_hole circle (at -3.19278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 46 /ETH0_RX-))
    (pad 7 thru_hole circle (at -4.46278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 47 /ETH_PWR+))
    (pad 8 thru_hole circle (at -5.73278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 48 /ETH_PWR-))
    (pad 9 thru_hole circle (at 5.36956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 49 "Net-(J8-Pad9)"))
    (pad 10 thru_hole circle (at 2.82956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 50 /ETH0_LED))
    (pad 11 thru_hole circle (at -5.32892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 51 "Net-(J8-Pad11)"))
    (pad 12 thru_hole circle (at -7.86892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 52 /WLAN_LED))
    (pad S1 thru_hole circle (at 6.477 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad S2 thru_hole circle (at -9.017 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -6.95 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module plan44:Recom-R78Cxx (layer F.Cu) (tedit 593D7237)
    (at 79.4 80.5 270)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U3 (at -0.4 5.6 270) (layer F.SilkS))
    (fp_text value Recom_R78Cxx (at 2.4 -3.2 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 5.08 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 +24V))
    (pad 3 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
  )
  (module plan44:ONION-OMEGA2S (layer F.Cu) (tedit 5971C332)
    (at 146.304 88.646 90)
    (clearance 0.25)
    (fp_text reference U1 (at 8.55 -20.5 90) (layer F.SilkS))
    (fp_text value ONION-OMEGA2S (at 4.4 -3.9 180) (layer F.Fab))
    (pad A13 smd rect (at -9.8155 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A12 smd rect (at -8.5455 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A11 smd rect (at -7.2755 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A10 smd rect (at -6.0055 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A9 smd rect (at -4.7355 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at -3.4655 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at -2.1955 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad A6 smd rect (at -0.9255 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 57 /I2C_SDA))
    (pad A5 smd rect (at 0.3445 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 55 /I2C_SCL))
    (pad A4 smd rect (at 1.6145 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A3 smd rect (at 2.8845 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A2 smd rect (at 4.1545 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B1 smd rect (at -13.0125 -17.78 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 54 /Omega_TX))
    (pad B2 smd rect (at -13.0125 -16.51 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 53 /Omega_RX))
    (pad B3 smd rect (at -13.0125 -15.24 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 45 /ETH0_RX+))
    (pad B4 smd rect (at -13.0125 -13.97 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 46 /ETH0_RX-))
    (pad B5 smd rect (at -13.0125 -12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 43 /ETH0_TX+))
    (pad B6 smd rect (at -13.0125 -11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 44 /ETH0_TX-))
    (pad B7 smd rect (at -13.0125 -10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /ETH1_TX+))
    (pad B8 smd rect (at -13.0125 -8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /ETH1_TX-))
    (pad B9 smd rect (at -13.0125 -7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /ETH1_RX+))
    (pad B10 smd rect (at -13.0125 -6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /ETH1_RX-))
    (pad B11 smd rect (at -13.0125 -5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 58 /G18))
    (pad B12 smd rect (at -13.0125 -3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 56 /G19))
    (pad B13 smd rect (at -13.0125 -2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 65 /UART_TX2))
    (pad B14 smd rect (at -13.0125 -1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 66 /UART_RX2))
    (pad B15 smd rect (at -13.0125 0 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad2)"))
    (pad B16 smd rect (at -13.0125 1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad4)"))
    (pad B17 smd rect (at -13.0125 2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad6)"))
    (pad B18 smd rect (at -13.0125 3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J1-Pad8)"))
    (pad B19 smd rect (at -13.0125 5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J1-Pad7)"))
    (pad B20 smd rect (at -13.0125 6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-Pad5)"))
    (pad B21 smd rect (at -13.0125 7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad3)"))
    (pad B22 smd rect (at -13.0125 8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad1)"))
    (pad B23 smd rect (at -13.0125 10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 62 /USB+))
    (pad B24 smd rect (at -13.0125 11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 63 /USB-))
    (pad B25 smd rect (at -13.0125 12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C1 smd rect (at 8.5675 -17.78 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C2 smd rect (at 8.5675 -16.51 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd rect (at 8.5675 -15.24 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C4 smd rect (at 8.5675 -13.97 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C5 smd rect (at 8.5675 -12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 67 /UART_RX1))
    (pad C6 smd rect (at 8.5675 -11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 68 /UART_TX1))
    (pad C7 smd rect (at 8.5675 -10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 52 /WLAN_LED))
    (pad C8 smd rect (at 8.5675 -8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 50 /ETH0_LED))
    (pad C9 smd rect (at 8.5675 -7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 31 /ETH1_LED))
    (pad C10 smd rect (at 8.5675 -6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 64 /RS485_TXEN2))
    (pad C11 smd rect (at 8.5675 -5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C12 smd rect (at 8.5675 -3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C13 smd rect (at 8.5675 -2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C14 smd rect (at 8.5675 -1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C15 smd rect (at 8.5675 0 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C16 smd rect (at 8.5675 1.27 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C17 smd rect (at 8.5675 2.54 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad C18 smd rect (at 8.5675 3.81 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad C19 smd rect (at 8.5675 5.08 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 69 /HS_IN))
    (pad C20 smd rect (at 8.5675 6.35 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 70 /HS_OUT))
    (pad C21 smd rect (at 8.5675 7.62 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C22 smd rect (at 8.5675 8.89 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R7-Pad2)"))
    (pad C23 smd rect (at 8.5675 10.16 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R2-Pad1)"))
    (pad C24 smd rect (at 8.5675 11.43 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R1-Pad1)"))
    (pad C25 smd rect (at 8.5675 12.7 90) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad A1 smd rect (at 5.4245 -20.5055 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad "" thru_hole rect (at -5.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at -3.15 -3.55 90) (size 10 15) (layers B.Cu B.Paste B.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -6.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -5.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -4.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -3.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -2.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -1.9 90) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
  )
  (dimension 2.9 (width 0.3) (layer Dwgs.User)
    (gr_text "2.900 mm" (at 39 130.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 123.6) (xy 36.4 123.6)))
    (feature2 (pts (xy 67.8 120.7) (xy 36.4 120.7)))
    (crossbar (pts (xy 39.1 120.7) (xy 39.1 123.6)))
    (arrow1a (pts (xy 39.1 123.6) (xy 38.513579 122.473496)))
    (arrow1b (pts (xy 39.1 123.6) (xy 39.686421 122.473496)))
    (arrow2a (pts (xy 39.1 120.7) (xy 38.513579 121.826504)))
    (arrow2b (pts (xy 39.1 120.7) (xy 39.686421 121.826504)))
  )
  (dimension 2.9 (width 0.3) (layer Dwgs.User)
    (gr_text "2.900 mm" (at 34.9 53.7 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 60.3) (xy 32 60.3)))
    (feature2 (pts (xy 67.8 63.2) (xy 32 63.2)))
    (crossbar (pts (xy 34.7 63.2) (xy 34.7 60.3)))
    (arrow1a (pts (xy 34.7 60.3) (xy 35.286421 61.426504)))
    (arrow1b (pts (xy 34.7 60.3) (xy 34.113579 61.426504)))
    (arrow2a (pts (xy 34.7 63.2) (xy 35.286421 62.073496)))
    (arrow2b (pts (xy 34.7 63.2) (xy 34.113579 62.073496)))
  )
  (gr_line (start 72 120) (end 72 64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.5 120) (end 72 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.5 64) (end 162.5 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72 64) (end 162.5 64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 108 (width 0.3) (layer Dwgs.User)
    (gr_text "108.000 mm" (at 117.25 36.75) (layer Dwgs.User))
    (feature1 (pts (xy 171.25 73.8) (xy 171.25 35.4)))
    (feature2 (pts (xy 63.25 73.8) (xy 63.25 35.4)))
    (crossbar (pts (xy 63.25 38.1) (xy 171.25 38.1)))
    (arrow1a (pts (xy 171.25 38.1) (xy 170.123496 38.686421)))
    (arrow1b (pts (xy 171.25 38.1) (xy 170.123496 37.513579)))
    (arrow2a (pts (xy 63.25 38.1) (xy 64.376504 38.686421)))
    (arrow2b (pts (xy 63.25 38.1) (xy 64.376504 37.513579)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 57 47.5) (layer Dwgs.User))
    (feature1 (pts (xy 63.25 73.8) (xy 63.25 45.05)))
    (feature2 (pts (xy 71.25 73.8) (xy 71.25 45.05)))
    (crossbar (pts (xy 71.25 47.75) (xy 63.25 47.75)))
    (arrow1a (pts (xy 63.25 47.75) (xy 64.376504 47.163579)))
    (arrow1b (pts (xy 63.25 47.75) (xy 64.376504 48.336421)))
    (arrow2a (pts (xy 71.25 47.75) (xy 70.123496 47.163579)))
    (arrow2b (pts (xy 71.25 47.75) (xy 70.123496 48.336421)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 34.9 69.8 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 63.3) (xy 36.3 63.3)))
    (feature2 (pts (xy 67.8 71.3) (xy 36.3 71.3)))
    (crossbar (pts (xy 39 71.3) (xy 39 63.3)))
    (arrow1a (pts (xy 39 63.3) (xy 39.586421 64.426504)))
    (arrow1b (pts (xy 39 63.3) (xy 38.413579 64.426504)))
    (arrow2a (pts (xy 39 71.3) (xy 39.586421 70.173496)))
    (arrow2b (pts (xy 39 71.3) (xy 38.413579 70.173496)))
  )
  (dimension 49.5 (width 0.3) (layer Dwgs.User)
    (gr_text "49.500 mm" (at 37.7 96.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 120.8) (xy 36.35 120.8)))
    (feature2 (pts (xy 67.8 71.3) (xy 36.35 71.3)))
    (crossbar (pts (xy 39.05 71.3) (xy 39.05 120.8)))
    (arrow1a (pts (xy 39.05 120.8) (xy 38.463579 119.673496)))
    (arrow1b (pts (xy 39.05 120.8) (xy 39.636421 119.673496)))
    (arrow2a (pts (xy 39.05 71.3) (xy 38.463579 72.426504)))
    (arrow2b (pts (xy 39.05 71.3) (xy 39.636421 72.426504)))
  )
  (dimension 41.5 (width 0.3) (layer Dwgs.User)
    (gr_text "41.500 mm" (at 43.35 92.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 112.8) (xy 42 112.8)))
    (feature2 (pts (xy 67.8 71.3) (xy 42 71.3)))
    (crossbar (pts (xy 44.7 71.3) (xy 44.7 112.8)))
    (arrow1a (pts (xy 44.7 112.8) (xy 44.113579 111.673496)))
    (arrow1b (pts (xy 44.7 112.8) (xy 45.286421 111.673496)))
    (arrow2a (pts (xy 44.7 71.3) (xy 44.113579 72.426504)))
    (arrow2b (pts (xy 44.7 71.3) (xy 45.286421 72.426504)))
  )
  (dimension 2.5 (width 0.3) (layer Dwgs.User)
    (gr_text "2.500 mm" (at 58.4 80 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 71.3) (xy 55.8 71.3)))
    (feature2 (pts (xy 67.8 73.8) (xy 55.8 73.8)))
    (crossbar (pts (xy 58.5 73.8) (xy 58.5 71.3)))
    (arrow1a (pts (xy 58.5 71.3) (xy 59.086421 72.426504)))
    (arrow1b (pts (xy 58.5 71.3) (xy 57.913579 72.426504)))
    (arrow2a (pts (xy 58.5 73.8) (xy 59.086421 72.673496)))
    (arrow2b (pts (xy 58.5 73.8) (xy 57.913579 72.673496)))
  )
  (dimension 92 (width 0.3) (layer Dwgs.User)
    (gr_text "92.000 mm" (at 117.25 46.4) (layer Dwgs.User))
    (feature1 (pts (xy 163.25 70.5) (xy 163.25 45.05)))
    (feature2 (pts (xy 71.25 70.5) (xy 71.25 45.05)))
    (crossbar (pts (xy 71.25 47.75) (xy 163.25 47.75)))
    (arrow1a (pts (xy 163.25 47.75) (xy 162.123496 48.336421)))
    (arrow1b (pts (xy 163.25 47.75) (xy 162.123496 47.163579)))
    (arrow2a (pts (xy 71.25 47.75) (xy 72.376504 48.336421)))
    (arrow2b (pts (xy 71.25 47.75) (xy 72.376504 47.163579)))
  )
  (dimension 7.25 (width 0.3) (layer Dwgs.User)
    (gr_text "7.250 mm" (at 84.8 43.5) (layer Dwgs.User))
    (feature1 (pts (xy 71.25 73.8) (xy 71.25 40.9)))
    (feature2 (pts (xy 78.5 73.8) (xy 78.5 40.9)))
    (crossbar (pts (xy 78.5 43.6) (xy 71.25 43.6)))
    (arrow1a (pts (xy 71.25 43.6) (xy 72.376504 43.013579)))
    (arrow1b (pts (xy 71.25 43.6) (xy 72.376504 44.186421)))
    (arrow2a (pts (xy 78.5 43.6) (xy 77.373496 43.013579)))
    (arrow2b (pts (xy 78.5 43.6) (xy 77.373496 44.186421)))
  )
  (dimension 77.5 (width 0.3) (layer Dwgs.User)
    (gr_text "77.500 mm" (at 117.25 51.75) (layer Dwgs.User))
    (feature1 (pts (xy 156 77) (xy 156 50.4)))
    (feature2 (pts (xy 78.5 77) (xy 78.5 50.4)))
    (crossbar (pts (xy 78.5 53.1) (xy 156 53.1)))
    (arrow1a (pts (xy 156 53.1) (xy 154.873496 53.686421)))
    (arrow1b (pts (xy 156 53.1) (xy 154.873496 52.513579)))
    (arrow2a (pts (xy 78.5 53.1) (xy 79.626504 53.686421)))
    (arrow2b (pts (xy 78.5 53.1) (xy 79.626504 52.513579)))
  )
  (dimension 36.5 (width 0.3) (layer Dwgs.User)
    (gr_text "36.500 mm" (at 61.45 92.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 85.6 110.3) (xy 60.1 110.3)))
    (feature2 (pts (xy 85.6 73.8) (xy 60.1 73.8)))
    (crossbar (pts (xy 62.8 73.8) (xy 62.8 110.3)))
    (arrow1a (pts (xy 62.8 110.3) (xy 62.213579 109.173496)))
    (arrow1b (pts (xy 62.8 110.3) (xy 63.386421 109.173496)))
    (arrow2a (pts (xy 62.8 73.8) (xy 62.213579 74.926504)))
    (arrow2b (pts (xy 62.8 73.8) (xy 63.386421 74.926504)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.644 64.516) (xy 162.052 64.516) (xy 162.052 119.38) (xy 72.644 118.872)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.644 64.516) (xy 162.052 64.516) (xy 162.052 119.38) (xy 72.644 118.872)
      )
    )
  )
)
