<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>KPS 20150403</text>
<text>FRY!</text>
<text>-</text>
<text>+</text>
<text>BATT</text>
<text>GND</text>
<text>Vcc</text>
<text>D.6</text>
<text>B.0</text>
<text>B.1</text>
<text>B.2</text>
<text>B.3</text>
<text>B.4</text>
<text>D.0</text>
<text>D.1</text>
<wire x1="0" y1="0" x2="0" y2="13.97" width="0.0254" layer="20"/>
<wire x1="0" y1="13.97" x2="35.56" y2="13.97" width="0.0254" layer="20"/>
<wire x1="35.56" y1="13.97" x2="35.56" y2="0" width="0.0254" layer="20"/>
<wire x1="35.56" y1="0" x2="0" y2="0" width="0.0254" layer="20"/>
</plain>
<libraries>
<library name="misc">
<packages>
<package name="SMD-1206-N">
</package>
</packages>
</library>
<library name="ic">
<packages>
<package name="IC-20-SOIC-300">
<description>SOIC (Small Outline Integrated Circuit), 20 pin, 300 mil width</description>
</package>
<package name="IC-5-SOT23">
<description>SOT-23 (Small Outline Transitor), 5 pin</description>
</package>
</packages>
</library>
<library name="conn">
<packages>
<package name="J-6-AVR-ISP">
</package>
<package name="J-2-100">
</package>
<package name="J-5-100">
</package>
</packages>
</library>
<library name="glyphs">
<packages>
<package name="GLYPH-DT&amp;E-40">
</package>
<package name="GLYPH-DT&amp;E-100-TEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="misc" package="SMD-1206-N" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="U1" library="ic" package="IC-20-SOIC-300" value="ATTINY2313">
<attribute name="VALUE"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="J2" library="conn" package="J-6-AVR-ISP" value="">
<attribute name="DESC" value=""/>
<attribute name="SOURCE" value=""/>
</element>
<element name="U2" library="ic" package="IC-5-SOT23" value="3V">
<attribute name="VALUE"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="C2" library="misc" package="SMD-1206-N" value="1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="J0" library="conn" package="J-2-100" value="">
<attribute name="VALUE"/>
<attribute name="DESC" value="SW0"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="J1" library="conn" package="J-2-100" value="">
<attribute name="VALUE"/>
<attribute name="DESC" value="SW1"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="J5" library="conn" package="J-2-100" value="">
<attribute name="VALUE"/>
<attribute name="DESC" value="BATTERY"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="J3" library="conn" package="J-5-100" value="">
<attribute name="DESC" value="LEDS0"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="J4" library="conn" package="J-5-100" value="">
<attribute name="DESC" value="LEDS1"/>
<attribute name="SOURCE" value=""/>
</element>
<element name="U$2" library="glyphs" package="GLYPH-DT&amp;E-40" value=""/>
<element name="U$4" library="glyphs" package="GLYPH-DT&amp;E-100-TEXT" value=""/>
</elements>
<signals>
<signal name="SCK">
<contactref element="U1" pad="19"/>
<contactref element="J2" pad="SCK"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="18"/>
<contactref element="J2" pad="MISO"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="17"/>
<contactref element="J2" pad="MOSI"/>
</signal>
<signal name="/RESET">
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="!RESET"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="J2" pad="GND"/>
<contactref element="U1" pad="10"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J0" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SW1">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SW0">
<contactref element="U1" pad="6"/>
<contactref element="J0" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="20"/>
<contactref element="J2" pad="VCC"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="C2" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="/SHDN">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="D0">
<contactref element="J4" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D1">
<contactref element="J4" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="D6">
<contactref element="J3" pad="5"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="B0">
<contactref element="U1" pad="12"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="B1">
<contactref element="U1" pad="13"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="B2">
<contactref element="U1" pad="14"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="B3">
<contactref element="U1" pad="15"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="B4">
<contactref element="U1" pad="16"/>
<contactref element="J4" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
