(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(D1-K)")
  (net 3 "Net-(U1-PROG)")
  (net 4 "+5V")
  (net 5 "Net-(J1-Pin_1)")
  (net 6 "Net-(U1-~{CHRG})")
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 139.35 79.9)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -3.125 0.65) (layer "F.SilkS"))
    (fp_text value "1k" (at -3.125 -0.45) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "Net-(U1-~{CHRG})") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:JT-flat-conn-large-holes" (layer "F.Cu")
    (at 139.3 82.795 180)
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -0.025 -4.58 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 1 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.5 -2.5 180) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 -2.5 180) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:TSOT-23-5" (layer "F.Cu")
    (at 144.675 83.025)
    (descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSOT TO_SOT_SMD")
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Constant-current/constant-voltage linear charger for single cell lithium-ion batteries with 2.9V Trickle Charge, 4.5V to 6.5V VDD, -40 to +85 degree Celsius, TSOT-23-5")
    (property "ki_keywords" "Constant-current constant-voltage linear charger single cell lithium-ion battery")
    (attr smd)
    (fp_text reference "U1 4054" (at 1.375 -0.075) (layer "F.SilkS"))
    (fp_text value "LTC4054ES5-4.2" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(U1-~{CHRG})") (pinfunction "~{CHRG}") (pintype "open_collector"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pin_1)") (pinfunction "BAT") (pintype "power_out"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+5V") (pinfunction "V_{CC}") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U1-PROG)") (pinfunction "PROG") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 144.975 88.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0.125 -1.6) (layer "F.SilkS"))
    (fp_text value "100k" (at 0.075 1.575) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 139.3 82.6 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at 3.075 0.525) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392982)
      (net 2 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392982)
      (net 4 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:JT-flat-conn-large-holes" (layer "F.Cu")
    (at 139.3 85.895 180)
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 1.87 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 1 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.5 -2.5 180) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 -2.5 180) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 149.475 81.35 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "    (property \"Reference\" \"#PWR\" (at 0 -3.81 0)")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -1.675 -1.575) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 145.075 79.9 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 4.675 0.775) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 3.3 0.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "Net-(U1-PROG)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:JT-flat-conn-large-holes" (layer "F.Cu")
    (at 152 86.8 90)
    (property "Sheetfile" "LTC4054.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at -0.125 -0.875 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 1 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.5 -2.5 90) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 4 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 -2.5 90) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (gr_rect (start 135.35 78.55) (end 151.625 90.45)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Batt" (at 140.6 87.35) (layer "B.SilkS"))
  (gr_text "Lipo Batt 4054\n1.6 v \nSherm 6/2/23" (at 146.45 82.25) (layer "B.SilkS"))
  (gr_text "Power" (at 148.2 85.05 90) (layer "B.SilkS"))
  (gr_text "Batt-out" (at 142.775 84.35) (layer "B.SilkS"))
  (gr_text "GND" (at 151.525 86.25 90) (layer "F.SilkS"))
  (gr_text "+" (at 150.5 88.8) (layer "F.SilkS"))
  (gr_text "GND" (at 135.375 90.4) (layer "F.SilkS"))
  (gr_text "+" (at 140.85 90.3) (layer "F.SilkS"))
  (gr_text "." (at 142.2 82.175) (layer "F.SilkS"))
  (gr_text "-" (at 141.9 83.2) (layer "F.SilkS"))
  (gr_text "+" (at 135.775 83.525) (layer "F.SilkS"))
  (gr_text "GND" (at 135.35 87.325) (layer "F.SilkS"))
  (gr_text "+" (at 146.825 84.2) (layer "F.SilkS"))
)
