<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>Shelly FTDI v1.0</text>
<wire x1="17.145" y1="11.684" x2="17.145" y2="27.305" width="0" layer="20"/>
<wire x1="17.145" y1="27.305" x2="39.624" y2="27.305" width="0" layer="20"/>
<wire x1="17.145" y1="11.684" x2="39.624" y2="11.684" width="0" layer="20"/>
<wire x1="39.624" y1="11.684" x2="39.624" y2="27.305" width="0" layer="20"/>
<text>GND</text>
<text>NC</text>
<text>3V3</text>
<text>NC</text>
<text>3V3</text>
<text>RXD</text>
<text>TXD</text>
<text>GND</text>
<text>GND</text>
<text>IO0</text>
<text>IO0</text>
<text>RST</text>
<text>3V3</text>
<text>RXD</text>
<text>TXD</text>
<text>IO0</text>
<text>Shelly</text>
<text>v1.0</text>
<text>TX</text>
<text>Debug</text>
<text>GND</text>
<text>NC</text>
<text>3V3</text>
<text>NC</text>
<text>GND</text>
<text>IO0</text>
<text>3V3</text>
<text>RXD</text>
<text>TXD</text>
<text>3V3</text>
<text>RXD</text>
<text>TXD</text>
<text>GND</text>
<text>IO0</text>
<text>RST</text>
<text>TX</text>
<text>Debug</text>
<text>FTDI</text>
<text>programmer</text>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="M1X6">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_1.27MM">
</package>
</packages>
</library>
<library name="_c2h">
<packages>
<package name="SW2-2.6-3.0X2.5X1.2+0.4MM">
</package>
<package name="LOGO_C2I_015">
</package>
<package name="PAD-SMALL">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NO_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="dp_devices" package="M1X6" value="CON_HEADER_1X06-PTH"/>
<element name="J4" library="SparkFun-Connectors" package="1X05_1.27MM" value="">
<attribute name="VALUE"/>
</element>
<element name="BOOT" library="_c2h" package="SW2-2.6-3.0X2.5X1.2+0.4MM" value="B3U">
<attribute name="MPN" value="B3U-1000P-2P-SMD"/>
<attribute name="NAME"/>
</element>
<element name="RESET" library="_c2h" package="SW2-2.6-3.0X2.5X1.2+0.4MM" value="B3U">
<attribute name="MPN" value="B3U-1000P-2P-SMD"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="_c2h" package="LOGO_C2I_015" value=""/>
<element name="U$2" library="_c2h" package="LOGO_C2I_015" value=""/>
<element name="P1" library="_c2h" package="PAD-SMALL" value="PADSMALL"/>
<element name="J5" library="SparkFun-Connectors" package="1X07_1.27MM" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_NO_SILK" value="DBG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="RESET" pad="1"/>
<contactref element="BOOT" pad="1"/>
<contactref element="J4" pad="5"/>
<contactref element="J5" pad="6"/>
</signal>
<signal name="RXD-SH">
<contactref element="J2" pad="4"/>
<contactref element="J4" pad="2"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="TXD-SH">
<contactref element="J2" pad="5"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="J4" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="GPIO0">
<contactref element="BOOT" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="RST">
<contactref element="RESET" pad="2"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="TX_DBG">
<contactref element="J5" pad="7"/>
<contactref element="P1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
