<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="6.985" x2="49.2" y2="6.985" width="0" layer="20"/>
<wire x1="49.2" y1="6.985" x2="49.2" y2="49.86" width="0" layer="20"/>
<wire x1="49.2" y1="49.86" x2="44.46" y2="53.965" width="0" layer="20"/>
<wire x1="44.46" y1="53.965" x2="5.07" y2="53.965" width="0" layer="20"/>
<wire x1="5.07" y1="53.965" x2="0" y2="49.53" width="0" layer="20"/>
<wire x1="0" y1="49.53" x2="0" y2="6.985" width="0" layer="20"/>
<text>22/7 1.1.0</text>
</plain>
<libraries>
<library name="capacitors-elec">
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitors-film">
<packages>
<package name="BOX_SMALL">
</package>
</packages>
</library>
<library name="diodes">
<packages>
<package name="DO41-1">
<description>&lt;b&gt;DO-41 0.1" pad spacing, vertical&lt;/b&gt;</description>
</package>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="3MM_D">
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="ROUND">
<description>&lt;b&gt;Round Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="gm-ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="DPDT2_PCB">
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="R0207/1V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
vertical position&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 1 hole

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="16MM">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;
&lt;p&gt;potentiometer for showing off-board connections</description>
</package>
</packages>
</library>
<library name="enclosures">
<packages>
<package name="1590B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitors-elec" package="050_020_1" value="100µ">
<attribute name="NAME"/>
</element>
<element name="C10" library="capacitors-film" package="BOX_SMALL" value="6n8">
<attribute name="NAME"/>
</element>
<element name="C11" library="capacitors-film" package="BOX_SMALL" value="10n">
<attribute name="NAME"/>
</element>
<element name="C12" library="capacitors-film" package="BOX_SMALL" value="10n">
<attribute name="NAME"/>
</element>
<element name="C13" library="capacitors-film" package="BOX_SMALL" value="100n">
<attribute name="NAME"/>
</element>
<element name="C14" library="capacitors-film" package="BOX_SMALL" value="150p">
<attribute name="NAME"/>
</element>
<element name="C15" library="capacitors-film" package="BOX_SMALL" value="100n">
<attribute name="NAME"/>
</element>
<element name="C2" library="capacitors-film" package="BOX_SMALL" value="33n">
<attribute name="NAME"/>
</element>
<element name="C3" library="capacitors-film" package="BOX_SMALL" value="100n">
<attribute name="NAME"/>
</element>
<element name="C4" library="capacitors-film" package="BOX_SMALL" value="220p">
<attribute name="NAME"/>
</element>
<element name="C5" library="capacitors-film" package="BOX_SMALL" value="150p">
<attribute name="NAME"/>
</element>
<element name="C6" library="capacitors-film" package="BOX_SMALL" value="150p">
<attribute name="NAME"/>
</element>
<element name="C7" library="capacitors-film" package="BOX_SMALL" value="100n">
<attribute name="NAME"/>
</element>
<element name="C8" library="capacitors-film" package="BOX_SMALL" value="100n">
<attribute name="NAME"/>
</element>
<element name="C9" library="capacitors-film" package="BOX_SMALL" value="3n3">
<attribute name="NAME"/>
</element>
<element name="D1" library="diodes" package="DO41-1" value="1N914">
<attribute name="NAME"/>
</element>
<element name="D2" library="diodes" package="DO41-1" value="1N914">
<attribute name="NAME"/>
</element>
<element name="D3" library="diodes" package="DO41-1" value="1N914">
<attribute name="NAME"/>
</element>
<element name="D4" library="diodes" package="DO41-1" value="1N914">
<attribute name="NAME"/>
</element>
<element name="D5" library="diodes" package="DO41-3" value="1N5817">
<attribute name="NAME"/>
</element>
<element name="D6" library="diodes" package="3MM_D" value="LED">
<attribute name="NAME"/>
</element>
<element name="FXIN" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="FXOUT" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="IC1" library="gm-ics" package="DIL16" value="CD4049UBE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SUSTAIN" library="potentiometers" package="16MM" value="A100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TONE" library="potentiometers" package="16MM" value="B100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VOLUME" library="potentiometers" package="16MM" value="A100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistors" package="R0207/3" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="resistors" package="R0207/3" value="27K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="resistors" package="R0207/3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="resistors" package="R0207/3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="resistors" package="R0207/3" value="330K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="resistors" package="R0207/3" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="resistors" package="R0207/3" value="RLED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistors" package="R0207/3" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistors" package="R0207/3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistors" package="R0207/3" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="resistors" package="R0207/3" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="resistors" package="R0207/1V" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="resistors" package="R0207/3" value="33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="resistors" package="R0207/1V" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="resistors" package="R0207/3" value="39K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWG" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="SWL" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="V+" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="V-" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="RANGE" library="switches" package="DPDT2_PCB" value="ONOFFON">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="OUTG" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="ING" library="supply pins" package="ROUND" value="PADRND">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="enclosures" package="1590B" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="TONE" pad="3"/>
<contactref element="C9" pad="1"/>
<contactref element="RANGE" pad="A1"/>
</signal>
<signal name="N$8">
<contactref element="R14" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="TONE" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R11" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="RANGE" pad="A2"/>
</signal>
<signal name="N$11">
<contactref element="TONE" pad="2"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R14" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R12" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="RANGE" pad="B2"/>
</signal>
<signal name="N$16">
<contactref element="C15" pad="2"/>
<contactref element="IC1" pad="15"/>
<contactref element="R13" pad="2"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="VOLUME" pad="3"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="SUSTAIN" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="SUSTAIN" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="SUSTAIN" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R5" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="V-" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="VOLUME" pad="1"/>
<contactref element="SWG" pad="1"/>
<contactref element="RANGE" pad="B3"/>
<contactref element="OUTG" pad="1"/>
<contactref element="ING" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="1"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$15">
<contactref element="D5" pad="A"/>
<contactref element="R15" pad="2"/>
<contactref element="V+" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R15" pad="1"/>
<contactref element="D6" pad="ANODE"/>
</signal>
<signal name="N$20">
<contactref element="D6" pad="P$1"/>
<contactref element="SWL" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="VOLUME" pad="2"/>
<contactref element="FXOUT" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="C2" pad="2"/>
<contactref element="FXIN" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="11"/>
<contactref element="R8" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="C"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R9" pad="1"/>
<contactref element="IC1" pad="12"/>
<contactref element="R8" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="A"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="C7" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="R6" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
