(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 344)
    (no_connects 0)
    (area 113.487299 38.487299 173.512701 88.512701)
    (thickness 1.6)
    (drawings 44)
    (tracks 819)
    (zones 0)
    (modules 175)
    (nets 76)
  )
  (page A4)
  (title_block
    (title OpenLST)
    (date 2018-07-08)
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.127)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.4572 0.4572)
    (pad_drill 0.254)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 113.5 88.5)
    (visible_elements FFFEF77F)
    (pcbplotparams
      (layerselection 0x010fc_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /3V3_FILT)
  (net 2 GND)
  (net 3 +5V)
  (net 4 +3V3)
  (net 5 "Net-(C19-Pad1)")
  (net 6 VCC_3V6)
  (net 7 "Net-(C21-Pad2)")
  (net 8 "Net-(C22-Pad1)")
  (net 9 "Net-(C23-Pad2)")
  (net 10 "Net-(C24-Pad1)")
  (net 11 "Net-(C24-Pad2)")
  (net 12 "Net-(C25-Pad2)")
  (net 13 "Net-(C26-Pad1)")
  (net 14 "Net-(C38-Pad1)")
  (net 15 "Net-(C38-Pad2)")
  (net 16 "Net-(C39-Pad1)")
  (net 17 "Net-(C39-Pad2)")
  (net 18 /PA_VAPC)
  (net 19 "Net-(C45-Pad1)")
  (net 20 "Net-(C45-Pad2)")
  (net 21 "Net-(D1-Pad2)")
  (net 22 "Net-(D2-Pad2)")
  (net 23 "Net-(D3-Pad1)")
  (net 24 /PROG_DC)
  (net 25 /PROG_DD)
  (net 26 /~LST_RESET)
  (net 27 /UART0_RTS)
  (net 28 "Net-(J3-Pad3)")
  (net 29 /UART0_RX)
  (net 30 /UART0_TX)
  (net 31 /UART0_CTS)
  (net 32 /UART1_RTS)
  (net 33 "Net-(J4-Pad3)")
  (net 34 /UART1_RX)
  (net 35 /UART1_TX)
  (net 36 /UART1_CTS)
  (net 37 /~LST_RX_MODE)
  (net 38 "Net-(R3-Pad2)")
  (net 39 "Net-(R4-Pad2)")
  (net 40 "Net-(R5-Pad1)")
  (net 41 "Net-(R6-Pad1)")
  (net 42 "Net-(R7-Pad1)")
  (net 43 "Net-(R8-Pad1)")
  (net 44 "Net-(R9-Pad1)")
  (net 45 "Net-(R10-Pad1)")
  (net 46 "Net-(R11-Pad1)")
  (net 47 "Net-(R12-Pad1)")
  (net 48 /RF_EN)
  (net 49 "Net-(R15-Pad2)")
  (net 50 "Net-(R16-Pad2)")
  (net 51 "Net-(R17-Pad1)")
  (net 52 "Net-(R17-Pad2)")
  (net 53 /AN0)
  (net 54 /AN1)
  (net 55 /RF_BYP)
  (net 56 "Net-(U8-Pad2)")
  (net 57 "Net-(J5-Pad2)")
  (net 58 "Net-(J5-Pad3)")
  (net 59 "Net-(R25-Pad2)")
  (net 60 "Net-(U8-Pad6)")
  (net 61 "Net-(MK1-Pad1)")
  (net 62 "Net-(MK2-Pad1)")
  (net 63 "Net-(MK3-Pad1)")
  (net 64 "Net-(MK4-Pad1)")
  (net 65 "Net-(J2-Pad5)")
  (net 66 "Net-(J2-Pad6)")
  (net 67 "Net-(J2-Pad8)")
  (net 68 "Net-(J2-Pad9)")
  (net 69 "Net-(J2-Pad10)")
  (net 70 "Net-(U2-Pad18)")
  (net 71 "Net-(U2-Pad20)")
  (net 72 "Net-(U9-Pad16)")
  (net 73 "Net-(U9-Pad14)")
  (net 74 "Net-(U9-Pad25)")
  (net 75 /LST_TX_MODE)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.2032)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /3V3_FILT)
    (add_net /AN0)
    (add_net /AN1)
    (add_net /LST_TX_MODE)
    (add_net /PA_VAPC)
    (add_net /PROG_DC)
    (add_net /PROG_DD)
    (add_net /RF_BYP)
    (add_net /RF_EN)
    (add_net /UART0_CTS)
    (add_net /UART0_RTS)
    (add_net /UART0_RX)
    (add_net /UART0_TX)
    (add_net /UART1_CTS)
    (add_net /UART1_RTS)
    (add_net /UART1_RX)
    (add_net /UART1_TX)
    (add_net /~LST_RESET)
    (add_net /~LST_RX_MODE)
    (add_net GND)
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(MK1-Pad1)")
    (add_net "Net-(MK2-Pad1)")
    (add_net "Net-(MK3-Pad1)")
    (add_net "Net-(MK4-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U9-Pad14)")
    (add_net "Net-(U9-Pad16)")
    (add_net "Net-(U9-Pad25)")
    (add_net VCC_3V6)
  )
  (net_class 50ohm ""
    (clearance 0.127)
    (trace_width 0.35052)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C38-Pad2)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(C39-Pad2)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(C45-Pad2)")
    (add_net "Net-(U8-Pad2)")
    (add_net "Net-(U8-Pad6)")
  )
  (net_class 8mil ""
    (clearance 0.127)
    (trace_width 0.2032)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class PWR ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(D3-Pad1)")
  )
  (module archive:PinHeader_1x06_P2.54mm_Vertical locked (layer F.Cu) (tedit 5B5A2C6E)
    (at 117 60.5)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 2.8 -0.5 180) (layer F.SilkS))
    (fp_text value UART0 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /UART0_RTS))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /UART0_RX))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /UART0_TX))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /UART0_CTS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 137.1 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:TI_CC_QFN36 locked (layer F.Cu) (tedit 5B5A2C8F)
    (at 131.5 69)
    (fp_text reference U2 (at -2.4 -4.2) (layer F.SilkS))
    (fp_text value CC1110 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 37 thru_hole circle (at 0 1.5) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at 1.5 1.5) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at 1.5 -1.5) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at 0 -1.5) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at -1.5 -1.5) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 32 smd rect (at 0 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 /~LST_RX_MODE))
    (pad 31 smd rect (at 0.5 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C22-Pad1)"))
    (pad 30 smd rect (at 1 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C19-Pad1)"))
    (pad 29 smd rect (at 1.5 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 28 smd rect (at 2 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 33 smd rect (at -0.5 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 /LST_TX_MODE))
    (pad 34 smd rect (at -1 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R12-Pad1)"))
    (pad 35 smd rect (at -1.5 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R11-Pad1)"))
    (pad 36 smd rect (at -2 -2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R10-Pad1)"))
    (pad 23 smd rect (at 2.78 0 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C24-Pad1)"))
    (pad 22 smd rect (at 2.78 0.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 21 smd rect (at 2.78 1 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R17-Pad2)"))
    (pad 20 smd rect (at 2.78 1.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U2-Pad20)"))
    (pad 19 smd rect (at 2.78 2 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 27 smd rect (at 2.78 -2 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R16-Pad2)"))
    (pad 26 smd rect (at 2.78 -1.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 25 smd rect (at 2.78 -1 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 24 smd rect (at 2.78 -0.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C23-Pad2)"))
    (pad 14 smd rect (at 0 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R15-Pad2)"))
    (pad 13 smd rect (at -0.5 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R4-Pad2)"))
    (pad 12 smd rect (at -1 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R3-Pad2)"))
    (pad 11 smd rect (at -1.5 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R8-Pad1)"))
    (pad 10 smd rect (at -2 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 18 smd rect (at 2 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U2-Pad18)"))
    (pad 17 smd rect (at 1.5 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R25-Pad2)"))
    (pad 16 smd rect (at 1 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 /PROG_DC))
    (pad 15 smd rect (at 0.5 2.78) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 /PROG_DD))
    (pad 5 smd rect (at -2.78 0 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 /AN0))
    (pad 4 smd rect (at -2.78 -0.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 /RF_EN))
    (pad 3 smd rect (at -2.78 -1 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 /RF_BYP))
    (pad 2 smd rect (at -2.78 -1.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 1 smd rect (at -2.78 -2 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R9-Pad1)"))
    (pad 9 smd rect (at -2.78 2 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R7-Pad1)"))
    (pad 8 smd rect (at -2.78 1.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R6-Pad1)"))
    (pad 7 smd rect (at -2.78 1 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R5-Pad1)"))
    (pad 6 smd rect (at -2.78 0.5 90) (size 0.28 0.75) (layers F.Cu F.Paste F.Mask)
      (net 54 /AN1))
    (pad 37 smd rect (at 0 0) (size 4.4 4.4) (layers F.Cu)
      (net 2 GND))
    (pad 37 thru_hole circle (at -1.5 1.5) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at 1.5 0) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at 0 0) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at -1.5 0) (size 0.6096 0.6096) (drill 0.3556) (layers *.Cu B.Mask)
      (net 2 GND))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B42540C)
    (at 133.5 57.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 4 +3V3) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 124.05 56.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 125.05 56.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 126.05 56.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B42540C)
    (at 134.9 46.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 4 +3V3) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B42540C)
    (at 135.9 46.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 4 +3V3) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B42540C)
    (at 134.9 40.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 4 +3V3) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B42540C)
    (at 135.9 40.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 4 +3V3) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 141.3 47.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 142.1 47.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 143.3 46.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 143.3 45.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 159.9 40.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 159.9 43.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 159.9 43.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 159.9 42.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 159.9 41.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 155.3 39.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 156.1 39.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 156.9 39.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 153.5 66.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 157.7 72.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 156.1 72.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 155.1 73.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 159.7 73.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 149.9 55.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 162.3 55.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 149.9 54.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 162.3 54.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 149.9 53.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 162.3 53.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 149.9 52.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 162.3 52.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 149.9 51.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B424EF4)
    (at 162.3 51.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 6 VCC_3V6) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 164.1 67.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 165.9 61.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 163.1 63.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 162.3 59.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 154.7 57.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 151.9 58.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 151.1 62.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 138.3 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 139.7 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 140.9 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 142.1 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 148.9 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 150.3 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 151.7 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 153.1 70.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 136.7 65.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 137.5 65.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 139.1 65.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 140.5 65.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 141.5 66.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 143 66.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 144.1 66.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 145.5 66.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 146.9 66.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 148.3 66.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 149.5 66.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 157.25 63)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 151.1 59.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 160.7 57.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 162.3 64.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 166.9 66.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 164.9 67.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 162.9 67.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 161.7 67.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 164.1 61.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 159.75 57.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 163.1 59.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 163.1 60.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 163.1 62.1)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 161.5 64.9)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 153.7 57.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 152.7 57.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 166.7 60.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 161.5 58.3)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 151.1 60.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 151.1 61.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 151.9 63.7)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 152.9 64.5)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:SAW-8_3.8mm locked (layer F.Cu) (tedit 5B4156F8)
    (at 157.25 59.75 90)
    (fp_text reference U8 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value STA1120A (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.27 1.5 90) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 1.5 90) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U8-Pad2)"))
    (pad 3 smd rect (at 1.27 1.5 90) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.5 0 180) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.27 -1.5 90) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0 -1.5 90) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U8-Pad6)"))
    (pad 7 smd rect (at -1.27 -1.5 90) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -1.25 0 180) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module openlst:VIA-10mil locked (layer F.Cu) (tedit 5B423CA9)
    (at 157.25 64)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-10mil (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module openlst:Qorvo_LGA_28_ThermalVias locked (layer F.Cu) (tedit 5B5A2BC5)
    (at 157.25 68.25 180)
    (fp_text reference U9 (at -4.45 -2.65 180) (layer F.SilkS))
    (fp_text value RFFM6403 (at 0 3.8 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 29 smd rect (at 0 0.75 270) (size 0.6 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 smd rect (at 0 -0.75 270) (size 0.6 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 smd rect (at 0.75 0 180) (size 0.6 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at -1.5 -1.5 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at -1.5 0 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at 0 0 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at 1.5 0 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at -1.5 1.5 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at 0 1.5 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at 1.5 1.5 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at 1.5 -1.5 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at 0 -1.5 180) (size 0.5588 0.5588) (drill 0.254) (layers *.Cu B.Mask)
      (net 2 GND))
    (pad 29 smd rect (at -0.75 0 180) (size 0.6 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at 1.813 -2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 22 smd rect (at 2.625 -2.65 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 2.625 1.875 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U9-Pad16)"))
    (pad 15 smd rect (at 2.625 2.65 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -2.625 2.65 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 smd rect (at 0 0 180) (size 3.875 3.875) (layers F.Cu)
      (net 2 GND))
    (pad 1 smd rect (at -2.625 -2.65 180) (size 0.55 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.625 -1.875 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 75 /LST_TX_MODE))
    (pad 3 smd rect (at -2.625 -1.125 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 /RF_EN))
    (pad 4 smd rect (at -2.625 -0.375 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 55 /RF_BYP))
    (pad 5 smd rect (at -2.625 0.375 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA_VAPC))
    (pad 6 smd rect (at -2.625 1.125 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2.625 1.875 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C45-Pad2)"))
    (pad 9 smd rect (at -1.813 2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1.088 2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U8-Pad2)"))
    (pad 11 smd rect (at -0.363 2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 0.363 2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 1.088 2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U8-Pad6)"))
    (pad 14 smd rect (at 1.813 2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U9-Pad14)"))
    (pad 17 smd rect (at 2.625 1.125 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 18 smd rect (at 2.625 0.375 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C38-Pad2)"))
    (pad 19 smd rect (at 2.625 -0.375 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 2.625 -1.125 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C39-Pad2)"))
    (pad 21 smd rect (at 2.625 -1.875 180) (size 0.55 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 1.088 -2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 25 smd rect (at 0.363 -2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U9-Pad25)"))
    (pad 26 smd rect (at -0.363 -2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 27 smd rect (at -1.088 -2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 28 smd rect (at -1.813 -2.625 180) (size 0.4 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D5C)
    (at 128 73.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.2 1.3 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B4281CC)
    (at 136.1 67.1 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 1.4 0 180) (layer F.SilkS))
    (fp_text value 220p (at 0 1.18 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0 90) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 2 smd rect (at 0.3875 0 90) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2F54)
    (at 135.8 63.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 4 1.8 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A3005)
    (at 144.9 43.7 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.15 0.05 360) (layer F.SilkS))
    (fp_text value 10u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2F56)
    (at 134.1 63.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 4.1 1 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BE0)
    (at 165.25 73 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.3 0.15 540) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA_VAPC))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2B64)
    (at 136.1 71.9)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -0.1 1.35 180) (layer F.SilkS))
    (fp_text value 220p (at 0 1.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 2 smd rect (at 0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2E33)
    (at 151.75 66.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.15 1.45 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2F8D)
    (at 129.5 59.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.05 2.05 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B4152FA)
    (at 126.75 65.75 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -3 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B631ED5)
    (at 133 45 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 1.25 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:CP_EIA-3528-15_AVX-H locked (layer F.Cu) (tedit 5B4151DA)
    (at 148 46 270)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C14 (at 3.25 0 540) (layer F.SilkS))
    (fp_text value 100u (at 0 2.35 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.48 0 270) (size 1.46 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.48 0 270) (size 1.46 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-15_AVX-H.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B631ED0)
    (at 133 41 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DBA)
    (at 148 40.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2F72)
    (at 132.375 63.425 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0.525 -3.275 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DAF)
    (at 163 47 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at -0.3 1.6 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2B70)
    (at 139.2 70 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at -0.1 -2.3 360) (layer F.SilkS))
    (fp_text value 220p (at 0 1.18 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0 180) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.3875 0 180) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D69)
    (at 129 75.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 3 0 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2B4A)
    (at 137.6 67.2 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -1.7 -1.15 360) (layer F.SilkS))
    (fp_text value 3.9p (at 0 1.18 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0 270) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.3875 0 270) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C23-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2B79)
    (at 139.2 68.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 3.1 1.1 180) (layer F.SilkS))
    (fp_text value 3.9p (at 0 1.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2B3E)
    (at 141.4 68.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 2.35 0 180) (layer F.SilkS))
    (fp_text value 220p (at 0 1.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C24-Pad2)"))
    (pad 2 smd rect (at 0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C25-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2E56)
    (at 145.1 70.9 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0 -1.6 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C26-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2FAF)
    (at 148.5 54.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at -2.9 2.25 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BBB)
    (at 153.9 73.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 2.4 1.1 360) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2E3D)
    (at 152.25 67.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at -3.75 -3.05 180) (layer F.SilkS))
    (fp_text value 220p (at 0 1.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C38-Pad1)"))
    (pad 2 smd rect (at 0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C38-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2E26)
    (at 152.25 69.25)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at -0.45 2.85) (layer F.SilkS))
    (fp_text value 220p (at 0 1.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C39-Pad1)"))
    (pad 2 smd rect (at 0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C39-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BBE)
    (at 156.3 73.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C44 (at 2.5 0 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2F4A)
    (at 162 66.25 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C45 (at 0 1.25 360) (layer F.SilkS))
    (fp_text value 220p (at 0 1.18 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0 180) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 0.3875 0 180) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C45-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BBF)
    (at 158.5 73.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C46 (at 2.5 -1.2 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:C_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2F96)
    (at 131.25 59.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C47 (at -3.95 0 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:LED_0603_1608Metric locked (layer F.Cu) (tedit 5B631F72)
    (at 170.75 50.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:LED_0603_1608Metric locked (layer F.Cu) (tedit 5B631F7B)
    (at 170.75 53.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0.5 -1.5 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:D_SMB locked (layer F.Cu) (tedit 5B428008)
    (at 125.1 52.3 270)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D3 (at -0.2 3.2 270) (layer F.SilkS))
    (fp_text value STPS340U (at 0 3.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -3 270) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 5B42816C)
    (at 117 51.5)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at -0.1 5.2) (layer F.SilkS))
    (fp_text value 5VDC (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:PinHeader_2x05_P1.27mm_Vertical_SMD locked (layer F.Cu) (tedit 59FED6E3)
    (at 127 43.5 180)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -4.235 180) (layer F.SilkS))
    (fp_text value "CC Prog/Debug" (at 0 4.235 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.95 -2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at -1.95 -1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 24 /PROG_DC))
    (pad 4 smd rect (at 1.95 -1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 25 /PROG_DD))
    (pad 5 smd rect (at -1.95 0 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at 1.95 0 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at -1.95 1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 26 /~LST_RESET))
    (pad 8 smd rect (at 1.95 1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at -1.95 2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J2-Pad9)"))
    (pad 10 smd rect (at 1.95 2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:PinHeader_1x06_P2.54mm_Vertical locked (layer F.Cu) (tedit 5B631F3E)
    (at 124.5 85 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at -1.75 -2.75 360) (layer F.SilkS))
    (fp_text value UART1 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /UART1_RTS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /UART1_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /UART1_TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /UART1_CTS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:PinHeader_1x03_P2.54mm_Vertical locked (layer F.Cu) (tedit 5B415478)
    (at 141.5 85 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at -2.5 0 180) (layer F.SilkS))
    (fp_text value "Control Outputs" (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:SMA_Molex_73251-1153_EdgeMount_Horizontal locked (layer F.Cu) (tedit 5A1B666F)
    (at 169 63.5 180)
    (descr "Molex SMA RF Connectors, Edge Mount, (http://www.molex.com/pdm_docs/sd/732511150_sd.pdf)")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J6 (at -1.5 7 180) (layer F.SilkS))
    (fp_text value ANT (at -1.72 -7.11 180) (layer F.Fab))
    (fp_text user %R (at -1.5 7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.72 -4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.72 4.38 180) (size 0.97 0.97) (drill 0.46) (layers *.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers F.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 -4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 GND))
    (pad 2 smd rect (at 1.27 4.38 180) (size 0.95 0.46) (layers B.Cu)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:L_1206_3216Metric locked (layer F.Cu) (tedit 5AC5DB75)
    (at 130.5 49.5 180)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value "Z=500 @ 100M" (at 0 1.85 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.43 0 180) (size 1.22 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.43 0 180) (size 1.22 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:L_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2F92)
    (at 133 59.75 270)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at -2.75 -0.25 360) (layer F.SilkS))
    (fp_text value "Z=1k @ 100M" (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /3V3_FILT))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:L_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2B57)
    (at 137.6 69.2 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L5 (at -0.05 -1.6 180) (layer F.SilkS))
    (fp_text value 27n (at 0 1.18 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0 90) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at 0.3875 0 90) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C24-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:L_0402_1005Metric locked (layer F.Cu) (tedit 5B5A2E5B)
    (at 139.2 67.6)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L6 (at 2.9 -2.7) (layer F.SilkS))
    (fp_text value 27n (at 0 1.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C23-Pad2)"))
    (pad 2 smd rect (at 0.3875 0) (size 0.575 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:L_0603_1608Metric locked (layer F.Cu) (tedit 5B631FD7)
    (at 147.5 71.7 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L8 (at -0.05 1.5 180) (layer F.SilkS))
    (fp_text value "Z=1k @ 100M" (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:MountingHole_3.2mm_M3_Pad_Via locked (layer F.Cu) (tedit 5B428038)
    (at 118.5 83.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MK1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 61 "Net-(MK1-Pad1)"))
  )
  (module archive:MountingHole_3.2mm_M3_Pad_Via locked (layer F.Cu) (tedit 5B428038)
    (at 118.5 43.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MK2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 62 "Net-(MK2-Pad1)"))
  )
  (module archive:MountingHole_3.2mm_M3_Pad_Via locked (layer F.Cu) (tedit 5B428038)
    (at 168.5 43.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MK3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 63 "Net-(MK3-Pad1)"))
  )
  (module archive:MountingHole_3.2mm_M3_Pad_Via locked (layer F.Cu) (tedit 5B428038)
    (at 168.5 83.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MK4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value M3_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 64 "Net-(MK4-Pad1)"))
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D90)
    (at 143 78 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /~LST_RX_MODE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D9E)
    (at 147.25 78 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.55 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 75 /LST_TX_MODE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B631F76)
    (at 167.5 50.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B631F7D)
    (at 167.5 53.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -0.5 -1.5 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D87)
    (at 138 82)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.2) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 36 /UART1_CTS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D7A)
    (at 124.5 81.25 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -0.05 1.8 360) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 32 /UART1_RTS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D85)
    (at 134.5 82)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.2) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /UART1_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D80)
    (at 131 82)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.2) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 34 /UART1_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2C5A)
    (at 120.75 73.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -2.55 0 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 31 /UART0_CTS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2C4E)
    (at 120.75 63 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -3.05 0 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /UART0_RTS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2C54)
    (at 120.75 68.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -3.05 -0.15 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /UART0_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2C57)
    (at 120.75 70.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -3.05 0.05 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /UART0_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DA1)
    (at 147.25 80)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 2.95 0) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 75 /LST_TX_MODE))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DA3)
    (at 143 80)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -2.9 0) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /~LST_RX_MODE))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5AC5DB74)
    (at 154.25 81.25 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 48 /RF_EN))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2B37)
    (at 139.3 63.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0.05 1.35 180) (layer F.SilkS))
    (fp_text value 56K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5AC5DB74)
    (at 138.7 55.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D73)
    (at 129 79.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 3 0.2 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /~LST_RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2C51)
    (at 120.75 65.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -3.05 0 180) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D7E)
    (at 127.5 82)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -1.2) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DD1)
    (at 147.1 58.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 1.5) (layer F.SilkS))
    (fp_text value 33K (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 53 /AN0))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DCF)
    (at 143.9 58.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 1.5) (layer F.SilkS))
    (fp_text value 10K (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 53 /AN0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5AC5DB74)
    (at 134.5 50.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 33K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 54 /AN1))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5AC5DB74)
    (at 138 50.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 54 /AN1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BE9)
    (at 171.25 73 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 2.7 -0.05 360) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA_VAPC))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R25-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BF2)
    (at 157.25 81.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at -0.05 1.45 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 48 /RF_EN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2D61)
    (at 129 77.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 3 -0.1 180) (layer F.SilkS))
    (fp_text value 33K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /~LST_RESET))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5AC5DB74)
    (at 160.25 81.25 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 55 /RF_BYP))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2E00)
    (at 119.5 78.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(MK1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DF8)
    (at 117 48)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 2.9 0) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(MK2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2DB4)
    (at 163 43.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 3 0 90) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(MK3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5AC5DB74)
    (at 163.5 80)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at 0 -1.45) (layer F.SilkS))
    (fp_text value DNI (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.8 0) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(MK4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BE6)
    (at 169.25 73 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at -2.3 0.05 360) (layer F.SilkS))
    (fp_text value 5K6 (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA_VAPC))
    (pad 2 smd rect (at 0.8 0 270) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:R_0603_1608Metric locked (layer F.Cu) (tedit 5B5A2BE4)
    (at 167.25 73 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at -2.8 -0.05 180) (layer F.SilkS))
    (fp_text value 3K3 (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 2 smd rect (at 0.8 0 90) (size 0.82 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA_VAPC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:SOT-223-3_TabPin2 locked (layer F.Cu) (tedit 5A02FF57)
    (at 138.5 43.5 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 180) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:TO-263-3_TabPin2 locked (layer F.Cu) (tedit 5B40F2F7)
    (at 156 48 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U3 (at 3.5 -6.5 450) (layer F.SilkS))
    (fp_text value LT1086-3.6 (at 0 6.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -5.775 0 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC_3V6))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 6 VCC_3V6))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:Oscillator_SMD_Fordahl_DFAS15-4Pin_5.0x3.2mm locked (layer F.Cu) (tedit 5B5A2DDA)
    (at 144 53.75 180)
    (descr "Ultraminiature Crystal Clock Oscillator TXCO Fordahl DFA S15-OV/UOV, http://www.iqdfrequencyproducts.com/products/details/iqxo-70-11-30.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference U4 (at -1.9 2.95 180) (layer F.SilkS))
    (fp_text value "FOX924 27MHz" (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.05 1.4 180) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.05 1.4 180) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.05 -1.4 180) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R17-Pad1)"))
    (pad 4 smd rect (at -2.05 -1.4 180) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_Fordahl_DFAS15-4Pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:SOT-23 locked (layer F.Cu) (tedit 5B4280BD)
    (at 133 77.5 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U5 (at 0.2 -2.9 360) (layer F.SilkS))
    (fp_text value TLV803S (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C22-Pad1)"))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module archive:SOT-363_SC-70-6 locked (layer F.Cu) (tedit 5B424AAB)
    (at 147.25 68.5 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U6 (at -0.05 2 180) (layer F.SilkS))
    (fp_text value PE4259 (at 0 2 360) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C39-Pad1)"))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C38-Pad1)"))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C25-Pad2)"))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 /~LST_RX_MODE))
    (pad 6 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "This work is licensed under a\nCreative Commons Attribution-ShareAlike 4.0\nInternational License (CC-BY-SA 4.0)." (at 162 43.5) (layer B.SilkS))
  (gr_text rwk (at 171.75 79 90) (layer B.SilkS))
  (gr_line (start 113.5 83.5) (end 113.5 43.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 168.5 88.5) (end 118.5 88.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 173.5 43.5) (end 173.5 83.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 118.5 38.5) (end 168.5 38.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 118.5 83.5) (end 118.5 88.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 168.5 83.5) (end 173.5 83.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 168.5 43.5) (end 168.5 38.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 118.5 43.5) (end 113.5 43.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text "rev 2.1, 2018-08-02" (at 156.7 87.5) (layer F.SilkS))
  (gr_text OpenLST (at 156.7 84.5) (layer B.SilkS))
  (gr_text Aux (at 145.3 87.5) (layer F.SilkS))
  (gr_text Power (at 114.5 52.9 270) (layer F.SilkS))
  (gr_text UART0 (at 114.5 68.5 270) (layer F.SilkS))
  (gr_text UART1 (at 131 87.5) (layer F.SilkS))
  (gr_text GND (at 119.3 54.5 270) (layer F.SilkS))
  (gr_text +5V (at 119.3 50.9 270) (layer F.SilkS))
  (dimension 60 (width 0.3) (layer Eco1.User)
    (gr_text "60.000 mm" (at 143.5 28.15) (layer Eco1.User))
    (feature1 (pts (xy 173.5 38.5) (xy 173.5 26.8)))
    (feature2 (pts (xy 113.5 38.5) (xy 113.5 26.8)))
    (crossbar (pts (xy 113.5 29.5) (xy 173.5 29.5)))
    (arrow1a (pts (xy 173.5 29.5) (xy 172.373496 30.086421)))
    (arrow1b (pts (xy 173.5 29.5) (xy 172.373496 28.913579)))
    (arrow2a (pts (xy 113.5 29.5) (xy 114.626504 30.086421)))
    (arrow2b (pts (xy 113.5 29.5) (xy 114.626504 28.913579)))
  )
  (dimension 50 (width 0.3) (layer Eco1.User)
    (gr_text "50.000 mm" (at 143.5 33.15) (layer Eco1.User))
    (feature1 (pts (xy 168.5 39.5) (xy 168.5 31.8)))
    (feature2 (pts (xy 118.5 39.5) (xy 118.5 31.8)))
    (crossbar (pts (xy 118.5 34.5) (xy 168.5 34.5)))
    (arrow1a (pts (xy 168.5 34.5) (xy 167.373496 35.086421)))
    (arrow1b (pts (xy 168.5 34.5) (xy 167.373496 33.913579)))
    (arrow2a (pts (xy 118.5 34.5) (xy 119.626504 35.086421)))
    (arrow2b (pts (xy 118.5 34.5) (xy 119.626504 33.913579)))
  )
  (dimension 40 (width 0.3) (layer Eco1.User)
    (gr_text "40.000 mm" (at 108.15 63.5 270) (layer Eco1.User))
    (feature1 (pts (xy 114.5 83.5) (xy 106.8 83.5)))
    (feature2 (pts (xy 114.5 43.5) (xy 106.8 43.5)))
    (crossbar (pts (xy 109.5 43.5) (xy 109.5 83.5)))
    (arrow1a (pts (xy 109.5 83.5) (xy 108.913579 82.373496)))
    (arrow1b (pts (xy 109.5 83.5) (xy 110.086421 82.373496)))
    (arrow2a (pts (xy 109.5 43.5) (xy 108.913579 44.626504)))
    (arrow2b (pts (xy 109.5 43.5) (xy 110.086421 44.626504)))
  )
  (gr_text TX (at 146.5 82.9) (layer F.SilkS))
  (gr_text ~RX (at 143.9 82.9) (layer F.SilkS))
  (dimension 50 (width 0.3) (layer Eco1.User)
    (gr_text "50.000 mm" (at 104.15 63.5 270) (layer Eco1.User))
    (feature1 (pts (xy 113.5 88.5) (xy 102.8 88.5)))
    (feature2 (pts (xy 113.5 38.5) (xy 102.8 38.5)))
    (crossbar (pts (xy 105.5 38.5) (xy 105.5 88.5)))
    (arrow1a (pts (xy 105.5 88.5) (xy 104.913579 87.373496)))
    (arrow1b (pts (xy 105.5 88.5) (xy 106.086421 87.373496)))
    (arrow2a (pts (xy 105.5 38.5) (xy 104.913579 39.626504)))
    (arrow2b (pts (xy 105.5 38.5) (xy 106.086421 39.626504)))
  )
  (gr_text OpenLST (at 156.5 84.5) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 173.5 88.5) (xy 113.5 88.5) (xy 113.5 38.5) (xy 173.5 38.5)
      )
    )
  )
  (zone (net 6) (net_name VCC_3V6) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 148.5 38.5) (xy 148.5 76.9) (xy 173.5 76.9) (xy 173.5 38.5)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 113.5 38.5) (xy 113.5 88.5) (xy 173.5 88.5) (xy 173.5 38.5)
      )
    )
  )
  (zone (net 6) (net_name VCC_3V6) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 2.54))
    (polygon
      (pts
        (xy 164.7 38.5) (xy 164.7 57.3) (xy 149.1 57.3) (xy 149.1 38.5)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 1.27))
    (polygon
      (pts
        (xy 131.7 39.1) (xy 131.7 51.5) (xy 144.3 51.5) (xy 144.3 39.1)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 1.27))
    (polygon
      (pts
        (xy 173.5 88.5) (xy 113.5 88.5) (xy 113.5 38.5) (xy 173.5 38.5)
      )
    )
  )
  (zone (net 1) (net_name /3V3_FILT) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 125.5 75) (xy 137.5 75) (xy 137.5 59.5) (xy 125.5 59.5)
      )
    )
  )
)
