(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 51)
    (tracks 37)
    (zones 0)
    (modules 6)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 5E4788E2)
    (at 128.76 72.72)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at -0.715 5.295) (layer F.SilkS) hide)
    (fp_text value hole (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 5E4788E2)
    (at 159.665 93.415)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at -0.715 5.295) (layer F.SilkS) hide)
    (fp_text value hole (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 5E4788E2)
    (at 157.435 65.37)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at -0.715 5.295) (layer F.SilkS) hide)
    (fp_text value hole (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module customFootprints_PPNFC:PP_6_pogo_pin_contacts (layer B.Cu) (tedit 5E47609C)
    (at 148.465 83.36 180)
    (fp_text reference J1 (at 4.245 3.39) (layer B.SilkS) hide)
    (fp_text value Conn_01x06 (at 4.075 5.31) (layer B.Fab))
    (pad 3 smd circle (at 7.5 0 180) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 smd circle (at 3.75 0 180) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd circle (at 0 0 180) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 4 smd circle (at 0 -4 180) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd circle (at 3.75 -4 180) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd circle (at 7.5 -4 180) (size 2.6 2.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad6)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 136.085 58.08 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 2.85 -1.64 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 154.86 58.06 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at -1.755 2.855 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text github.com/SMR404/PinephonePogoBreakout (at 145.855 72.645) (layer F.SilkS))
  (gr_text "Pinephone\nPogo Pin Breakout Board\nV1.0\n" (at 131.995 68.9) (layer F.SilkS))
  (gr_text 5V (at 149.795 61.4 90) (layer F.SilkS))
  (gr_text BAT (at 152.4 61.32 90) (layer F.SilkS))
  (gr_text GND (at 154.83 61.33 90) (layer F.SilkS))
  (gr_text I2C (at 136.16 61.205 90) (layer F.SilkS))
  (gr_text I2C (at 133.565 61.215 90) (layer F.SilkS))
  (gr_text INT (at 130.98 61.255 90) (layer F.SilkS))
  (gr_text GND (at 148.375 87.355) (layer F.SilkS))
  (gr_text BAT (at 144.65 87.395) (layer F.SilkS))
  (gr_text 5V (at 140.94 87.43) (layer F.SilkS))
  (gr_text INT (at 140.93 83.35) (layer F.SilkS))
  (gr_text I2C (at 144.78 83.35) (layer F.SilkS))
  (gr_text I2C (at 148.49 83.365) (layer F.SilkS))
  (gr_arc (start 128.762857 72.719777) (end 125.762857 72.719777) (angle -52.25880262) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 127.042672 60.878092) (end 127.152765 62.374046) (angle -85.79099191) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 135.713832 82.784412) (end 137.213833 82.784412) (angle -56.18093969) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 128.542672 60.878092) (end 128.542672 57.62) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 127.262857 63.87) (end 127.152765 62.374046) (angle -85.79099191) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 125.762857 72.719777) (end 125.762857 63.87) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 136.548691 81.538213) (end 126.92657 75.092128) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 155.185 57.62) (end 157.435 57.62) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 149.525 57.62) (end 149.525 55.37) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 147.275 60.62) (end 147.275 57.62) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 136.452672 57.62) (end 138.702672 57.62) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 130.792672 55.37) (end 136.452672 55.37) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 130.792672 57.62) (end 130.792672 55.37) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 140.452672 62.37) (end 145.525 62.37) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.213833 88.862608) (end 137.213833 82.784412) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 138.713833 88.862608) (end 137.213833 88.862608) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 149.264928 90.362608) (end 138.713833 90.362608) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 149.264928 91.862608) (end 150.099786 90.616409) (angle -33.81906031) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 157.994115 95.905006) (end 150.099786 90.616409) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 159.663831 93.412608) (end 157.994115 95.905006) (angle -128.3633848) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160.425569 65.13231) (end 162.6544 93.174917) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 140.452672 60.62) (end 138.702672 60.62) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 138.702672 57.62) (end 138.702672 60.62) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 157.435 65.37) (end 160.425569 65.13231) (angle -63.83740313) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 159.185 60.95412) (end 157.435 60.95412) (angle -68.38172758) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 157.435 57.62) (end 157.435 60.95412) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 149.525 55.37) (end 155.185 55.37) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 145.525 60.62) (end 145.525 62.37) (angle -90) (layer Edge.Cuts) (width 0.2))
)
