<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.94" y2="0" width="0" layer="20"/>
<wire x1="27.94" y1="0" x2="27.94" y2="45.72" width="0" layer="20"/>
<wire x1="27.94" y1="45.72" x2="0" y2="45.72" width="0" layer="20"/>
<wire x1="0" y1="45.72" x2="0" y2="0" width="0" layer="20"/>
<text>+5V Decoder</text>
<text>+V Ontvanger</text>
<text>+12V LNB</text>
<text>+12--19V</text>
<text>(c) Rob Alblas
(r) Harryu H. Arends</text>
<text>2019-V0.1</text>
</plain>
<libraries>
<library name="2019 Kunstmanen">
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="6POL254">
<description>&lt;b&gt;PHOENIX CONNECTOR&lt;/b&gt;</description>
</package>
<package name="TCK141">
</package>
<package name="TSR-1">
<description>&lt;p&gt;&lt;b&gt;Traco TSR-1&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;i&gt;Source: www.tracopower.com&lt;/i&gt;&lt;/p&gt;</description>
</package>
<package name="E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Diodes">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Diodes&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="DO-41">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="2019 Kunstmanen" package="POWER_JACK_PTH" value="15-19V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="2019 Kunstmanen" package="6POL254" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="2019 Kunstmanen" package="TCK141" value="TCK-141">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="2019 Kunstmanen" package="TSR-1" value="TSR_1-2450">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="2019 Kunstmanen" package="TSR-1" value="TSR_1-2412">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Diodes" package="DO-41" value="1N4007">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1N4007MSCT-ND"/>
<attribute name="MANUFACTURER" value="Micro Commercial Co"/>
<attribute name="MPN" value="1N4007"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DO-41"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="2019 Kunstmanen" package="E5-5" value="47uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="2019 Kunstmanen" package="E5-6" value="100uF/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="2019 Kunstmanen" package="TO92" value="7812L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="K1" pad="6"/>
<contactref element="K1" pad="4"/>
<contactref element="K1" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="DECODER">
<contactref element="U1" pad="3"/>
<contactref element="K1" pad="5"/>
</signal>
<signal name="ONTVANGER">
<contactref element="U2" pad="3"/>
<contactref element="K1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="PWR"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="D1" pad="C"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="LNB">
<contactref element="C2" pad="+"/>
<contactref element="IC2" pad="1"/>
<contactref element="K1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
