<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="42.2148" y1="32.1056" x2="42.2148" y2="17.5768" width="0" layer="20"/>
<wire x1="42.2148" y1="17.5768" x2="43.4848" y2="16.3068" width="0" layer="20" curve="90"/>
<wire x1="43.4848" y1="16.3068" x2="71.5772" y2="16.3068" width="0" layer="20"/>
<wire x1="71.5772" y1="16.3068" x2="72.8472" y2="17.5768" width="0" layer="20" curve="90"/>
<wire x1="72.8472" y1="17.5768" x2="72.8472" y2="32.1056" width="0" layer="20"/>
<wire x1="72.8472" y1="32.1056" x2="71.5772" y2="33.3756" width="0" layer="20" curve="90"/>
<wire x1="71.5772" y1="33.3756" x2="43.4848" y2="33.3756" width="0" layer="20"/>
<wire x1="43.4848" y1="33.3756" x2="42.2148" y2="32.1056" width="0" layer="20" curve="90"/>
<text>13</text>
<text>CEC</text>
<text>17</text>
<text>GND</text>
<text>15</text>
<text>16</text>
<text>SCL</text>
<text>SDA</text>
<text>al1</text>
<text>HDMI breakout</text>
<text>18</text>
<text>19</text>
<text>5V</text>
<text>HPS</text>
</plain>
<libraries>
<library name="USBSteckverbinderWR-COM">
<description>&lt;BR&gt;Würth Elektronik -- Electronic Interconnect &amp; Electromechanical Solutions&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Version 6,  January 13th 2015
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="685119134923">
<description>WR-COM SMT Horizontal HDMI, 19 pins</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02_ROUND_NOSM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K1" library="USBSteckverbinderWR-COM" package="685119134923" value="685119134923"/>
<element name="K2" library="USBSteckverbinderWR-COM" package="685119134923" value="685119134923"/>
<element name="JP1" library="pinhead" package="1X02_ROUND_NOSM" value=""/>
<element name="JP2" library="pinhead" package="1X02_ROUND_NOSM" value=""/>
<element name="JP3" library="pinhead" package="1X02_ROUND_NOSM" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="K1" pad="5"/>
<contactref element="K2" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="K1" pad="4"/>
<contactref element="K2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="K1" pad="3"/>
<contactref element="K2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="K1" pad="2"/>
<contactref element="K2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="K1" pad="1"/>
<contactref element="K2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="K1" pad="6"/>
<contactref element="K2" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="K1" pad="7"/>
<contactref element="K2" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="K1" pad="8"/>
<contactref element="K2" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="K1" pad="9"/>
<contactref element="K2" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="K1" pad="10"/>
<contactref element="K2" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="K1" pad="11"/>
<contactref element="K2" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="K1" pad="12"/>
<contactref element="K2" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="K1" pad="13"/>
<contactref element="K2" pad="13"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="K1" pad="14"/>
<contactref element="K2" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="K1" pad="15"/>
<contactref element="K2" pad="15"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="K1" pad="16"/>
<contactref element="K2" pad="16"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="K1" pad="17"/>
<contactref element="K2" pad="17"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="K1" pad="18"/>
<contactref element="K2" pad="18"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="K1" pad="19"/>
<contactref element="K2" pad="19"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="K2" pad="Z1"/>
<contactref element="K2" pad="Z4"/>
<contactref element="K2" pad="Z3"/>
<contactref element="K2" pad="Z2"/>
<contactref element="K1" pad="Z1"/>
<contactref element="K1" pad="Z4"/>
<contactref element="K1" pad="Z3"/>
<contactref element="K1" pad="Z2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
