(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "disposable_pcb_prototype")
    (rev "v01")
    (company "Johns Hopkins University - Design Team 8")
    (comment 1 "Author: Aidan Aug")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (grid_origin 233.5 139.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 187.78 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 200.48 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 215.72 87.18)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 215.72 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 208.1 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 175.08 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 190.32 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 180.16 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 213.18 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 182.7 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 172.54 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 205.56 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 218.26 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 197.94 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 210.64 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 175.08 87.18)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 177.62 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 192.86 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 185.24 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 203.02 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 195.4 24.95)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "" thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (pinfunction "D8") (pintype "bidirectional"))
  )
  (gr_line (start 220.8 22.41) (end 170 22.41) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 220.8 92.26) (end 220.8 22.41) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 170 92.26) (end 220.8 92.26) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 170 22.41) (end 170 92.26) (layer "Edge.Cuts") (width 0.1))
)
