(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "./gerbers")
		)
	)
	(net 0 "")
	(net 1 "Net-(R1-Pad1)")
	(net 2 "Net-(R3-Pad2)")
	(net 3 "GND")
	(net 4 "/HV")
	(net 5 "+REG")
	(net 6 "+RAW")
	(net 7 "Net-(U1-adj)")
	(net 8 "unconnected-(reg1-Pad4)")
	(net 9 "Net-(reg1-SENSE{slash}adj)")
	(footprint "kicad-mza:TestPoint_16AWG"
		(layer "F.Cu")
		(at 210.185 142.875 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP2"
			(at 0 -2.286 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at -2.3114 -0.127 -90)
			(layer "F.SilkS")
		)
		(property "Footprint" "kicad-mza:TestPoint_16AWG"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2.286 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3.048 3.048)
			(drill 1.9812)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3224G_Horizontal"
		(layer "F.Cu")
		(at 227.965 140.335 -90)
		(descr "Potentiometer, horizontal, Bourns 3224G, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer horizontal Bourns 3224G")
		(property "Reference" "Radj2"
			(at 0.61 5.455 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 3.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3224G_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 2.6 -1.15 270)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(R1-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.6 0 270)
			(size 1.3 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(U1-adj)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.6 1.15 270)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(R3-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224G_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:TestPoint_16AWG"
		(layer "F.Cu")
		(at 206.883 139.065 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP4"
			(at 0 -2.286 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HV"
			(at 2.0066 1.8034 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "kicad-mza:TestPoint_16AWG"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2.286 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3.048 3.048)
			(drill 1.9812)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/HV")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "kicad-mza:0603"
		(layer "F.Cu")
		(at 229.108 145.669 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 3.429 0.381 90)
			(layer "F.SilkS")
		)
		(property "Value" "14k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "kicad-mza:0603"
			(at 0.175 1.5 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.075 1.525 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(R1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:MMCX_Molex_73415-1471_Vertical"
		(layer "F.Cu")
		(at 210.566 139.065 180)
		(descr "http://www.molex.com/pdm_docs/sd/734151471_sd.pdf")
		(tags "Molex MMCX Coaxial Connector 50 ohms Female Jack Vertical THT")
		(property "Reference" "J1"
			(at 0 -3.0368 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 2.794 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "kicad-mza:MMCX_Molex_73415-1471_Vertical"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/HV")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.27 -1.27 180)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.27 1.27 180)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 -1.27 180)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 1.27 180)
			(size 1.24 1.24)
			(drill 0.84)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/MMCX_Molex_73415-1471_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:PinHeader_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 204.125 146.75 180)
		(descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x04 2.54mm single row")
		(property "Reference" "inout1"
			(at 4.385 -2.27 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Male"
			(at 4.385 9.89 0)
			(layer "F.Fab")
		)
		(property "Footprint" "kicad-mza:PinHeader_1x04_P2.54mm_Horizontal"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+RAW")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/HV")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:TestPoint_16AWG"
		(layer "F.Cu")
		(at 206.883 146.685 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP1"
			(at 0 -2.286 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RAW"
			(at 1.6002 -2.2606 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "kicad-mza:TestPoint_16AWG"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2.286 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3.048 3.048)
			(drill 1.9812)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+RAW")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "kicad-mza:ultravolt-xs"
		(layer "F.Cu")
		(at 222.631 144.1831 180)
		(property "Reference" "U1"
			(at 10.16 1.524 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ultravolt-xs"
			(at -2.54 -10.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "kicad-mza:ultravolt-xs"
			(at 4.064 8.636 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.advancedenergy.com/globalassets/resources-root/data-sheets/en-hv-xs-series-data-sheet.pdf"
			(at -0.127 -6.35 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.429 1.651 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.778 1.778)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+REG")
			(pinfunction "power_in")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.778 1.778)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "gnd")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 1.778 1.778)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(U1-adj)")
			(pinfunction "adj")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 7.239 5.08 180)
			(size 1.778 1.778)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/HV")
			(pinfunction "HV_out")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 3.6322 -3.8608 180)
			(size 3.175 1.778)
			(drill oval 2.0066 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "shield")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 3.6322 6.731 180)
			(size 3.175 1.778)
			(drill oval 2.0066 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "shield")
			(pintype "input")
		)
	)
	(footprint "kicad-mza:TestPoint_16AWG"
		(layer "F.Cu")
		(at 206.883 142.875 180)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP3"
			(at 0 -2.286 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "kicad-mza:TestPoint_16AWG"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2.286 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3.048 3.048)
			(drill 1.9812)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "kicad-mza:0603"
		(layer "F.Cu")
		(at 226.9236 145.669 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at -3.556 0.0254 -90)
			(layer "F.SilkS")
		)
		(property "Value" "25k"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "kicad-mza:0603"
			(at 0.175 1.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.075 1.525 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+REG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(R3-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:0805"
		(layer "B.Cu")
		(at 220.726 141.351 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C4"
			(at 0 1.65 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "15uF"
			(at 0 -1.65 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "kicad-mza:0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "+REG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "B.Cu")
		(at 216.027 144.272 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "reg1"
			(at -1.905 3.556 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LT1963AES8"
			(at 0 -3.4 0)
			(layer "B.Fab")
		)
		(property "Footprint" "kicad-mza:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO*263*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+REG")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(reg1-SENSE{slash}adj)")
			(pinfunction "SENSE/adj")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "unconnected-(reg1-Pad4)")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+RAW")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+RAW")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:0603"
		(layer "B.Cu")
		(at 223.3168 147.7264 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0.9398 -1.2446 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "kicad-mza:0603"
			(at 0.175 -1.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.075 -1.525 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(reg1-SENSE{slash}adj)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:0603"
		(layer "B.Cu")
		(at 224.3836 140.4112 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C1"
			(at 0.9398 -1.2954 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "kicad-mza:0603"
			(at 0.175 -1.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.075 -1.525 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U1-adj)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:0603"
		(layer "B.Cu")
		(at 213.487 138.049 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C2"
			(at -3.429 0 -90)
			(layer "B.SilkS")
		)
		(property "Value" "220pF"
			(at 0 -1.43 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "kicad-mza:0603"
			(at 0.175 -1.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100V"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.075 -1.525 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/HV")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:0805"
		(layer "B.Cu")
		(at 215.0872 148.4884)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C3"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "15uF"
			(at 0 -1.65 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "kicad-mza:0805"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 6 "+RAW")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kicad-mza:0603"
		(layer "B.Cu")
		(at 224.2312 145.0829 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at -0.3029 -1.1938 90)
			(layer "B.SilkS")
		)
		(property "Value" "3.1k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "kicad-mza:0603"
			(at 0.175 -1.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "little-HV-board.revC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.075 -1.525 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+REG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(reg1-SENSE{slash}adj)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 230.632 136.8044) (xy 230.632 148.9964) (xy 229.87 149.7584) (xy 203.8096 149.7584) (xy 202.7936 148.7424)
			(xy 202.7936 136.9568) (xy 203.6064 136.144) (xy 229.9716 136.144)
		)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 211.328 145.8976 90)
		(layer "B.SilkS")
	)
	(gr_text "2024-10-07"
		(at 229.235 143.129 90)
		(layer "B.SilkS")
	)
	(gr_text "RAW"
		(at 205.1304 148.9456 0)
		(layer "B.SilkS")
	)
	(gr_text "HV"
		(at 204.9272 137.1092 0)
		(layer "B.SilkS")
	)
	(gr_text "IDL_024_039"
		(at 227.584 143.129 90)
		(layer "B.SilkS")
	)
	(gr_text "revC"
		(at 224.409 148.844 0)
		(layer "F.SilkS")
	)
	(gr_text "mza"
		(at 210.947 146.177 0)
		(layer "F.SilkS")
	)
	(gr_text "little HV board"
		(at 212.598 148.844 0)
		(layer "F.SilkS")
	)
	(zone
		(net 3)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 231.14 150.4188) (xy 201.9808 150.4188) (xy 201.9808 135.636) (xy 231.14 135.636)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 215.3412 140.335) (xy 203.0476 140.462) (xy 203.0984 137.8204) (xy 215.3412 137.795)
			)
		)
	)
	(zone
		(net 6)
		(net_name "+RAW")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 215.9 141.4272) (xy 216.662 142.1384) (xy 216.662 146.4056) (xy 215.290404 147.676162) (xy 215.303678 150.076022)
				(xy 202.384479 150.056868) (xy 202.3872 145.3388) (xy 204.9272 145.3388) (xy 205.5368 144.7292)
				(xy 208.534 144.7292) (xy 210.6676 145.8468) (xy 214.0204 145.8468) (xy 214.0204 143.1544) (xy 213.106 143.1544)
				(xy 213.106 141.4272)
			)
		)
	)
)
