<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<hole x="22" y="18" drill="4.2"/>
<wire x1="0" y1="1" x2="0" y2="35" width="0.3048" layer="20"/>
<hole x="26" y="34" drill="2.8"/>
<hole x="3" y="9" drill="2.8"/>
<wire x1="29" y1="8" x2="29" y2="41" width="0.3048" layer="20"/>
<wire x1="29" y1="41" x2="28" y2="42" width="0.3048" layer="20" curve="90"/>
<wire x1="28" y1="42" x2="8" y2="42" width="0.3048" layer="20"/>
<wire x1="7" y1="37" x2="7" y2="41" width="0.3048" layer="20"/>
<wire x1="7" y1="41" x2="8" y2="42" width="0.3048" layer="20" curve="-90"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0.3048" layer="20" curve="90"/>
<wire x1="21" y1="0" x2="1" y2="0" width="0.3048" layer="20"/>
<wire x1="22" y1="1" x2="22" y2="6" width="0.3048" layer="20"/>
<wire x1="22" y1="6" x2="23" y2="7" width="0.3048" layer="20" curve="-90"/>
<wire x1="23" y1="7" x2="28" y2="7" width="0.3048" layer="20"/>
<wire x1="0" y1="35" x2="1" y2="36" width="0.3048" layer="20" curve="-90"/>
<wire x1="1" y1="36" x2="6" y2="36" width="0.3048" layer="20"/>
<wire x1="6" y1="36" x2="7" y2="37" width="0.3048" layer="20" curve="90"/>
<wire x1="21" y1="0" x2="22" y2="1" width="0.3048" layer="20" curve="90"/>
<wire x1="28" y1="7" x2="29" y2="8" width="0.3048" layer="20" curve="90"/>
</plain>
<libraries>
<library name="injector">
<description>Generated from &lt;b&gt;injector.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs-filter.ulp</description>
<packages>
<package name="UD-6,3X5,8_NICHICON">
</package>
<package name="C0805">
</package>
<package name="A/3216-18R">
</package>
<package name="SOD123FL">
</package>
<package name="1206">
</package>
<package name="1X03">
</package>
<package name="2X03">
</package>
<package name="R0805">
</package>
<package name="SO-08">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="injector" package="UD-6,3X5,8_NICHICON" value="22uF 40V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="injector" package="C0805" value="0.1uF 50V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="injector" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="injector" package="C0805" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="injector" package="A/3216-18R" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="injector" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="injector" package="C0805" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="injector" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="injector" package="SOD123FL" value="MBR0540">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="injector" package="SOD123FL" value="MBR0540">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="injector" package="1206" value="500ma Slow">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="injector" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="injector" package="1X03" value="normalize-text.ULP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="injector" package="2X03" value="ICSP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="injector" package="R0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="injector" package="SO-08" value="ATA6631">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="injector" package="TQFP32-08" value="ATMEGA328">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="injector" package="SO-08" value="ATA6631">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="injector" package="RESONATOR-SMD" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="C7" pad="2"/>
<contactref element="J4" pad="6"/>
<contactref element="C6" pad="-"/>
<contactref element="U1" pad="3"/>
<contactref element="U3" pad="3"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="21"/>
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="LIN1">
<contactref element="U1" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="+12V">
<contactref element="U1" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="C"/>
<contactref element="C2" pad="+"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="J4" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="+"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="4"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="J1" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="ERROR_LED">
<contactref element="U2" pad="13"/>
</signal>
<signal name="FRAME_LED">
<contactref element="U2" pad="12"/>
</signal>
<signal name="LIN2">
<contactref element="R4" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="LIN1_TX">
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="25"/>
</signal>
<signal name="LIN1_RX">
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="32"/>
</signal>
<signal name="LIN2_TX">
<contactref element="U3" pad="6"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="LIN2_RX">
<contactref element="U3" pad="5"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="RESET">
<contactref element="J4" pad="5"/>
<contactref element="U2" pad="29"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="J4" pad="3"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="N$9">
<contactref element="D4" pad="C"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="XTAL1">
<contactref element="X1" pad="3"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="XTAL2">
<contactref element="X1" pad="1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="LIN_TICK">
<contactref element="U2" pad="1"/>
</signal>
<signal name="GP_DEBUG">
<contactref element="U2" pad="10"/>
</signal>
<signal name="MOSI/LIN_ERR">
<contactref element="U2" pad="15"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="MISO/LIN_DATA">
<contactref element="U2" pad="16"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="LIN_BREAK">
<contactref element="U2" pad="23"/>
</signal>
<signal name="LIN_ISR">
<contactref element="U2" pad="26"/>
</signal>
<signal name="SECONDARY_5V">
<contactref element="U3" pad="8"/>
<contactref element="C9" pad="1"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="STATUS_LED">
<contactref element="U2" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
