(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 2733)
    (zones 0)
    (modules 50)
    (nets 38)
  )
  (page A4)
  (title_block
    (title "RPT Extension Module")
    (date 2019-11-11)
    (rev A)
    (company "Primoz Beltram s.p.")
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.8)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.254)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 123 70)
    (grid_origin 123 70)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /board/SHIELD)
  (net 4 /VCC5V0)
  (net 5 "Net-(C402-Pad2)")
  (net 6 "Net-(C402-Pad1)")
  (net 7 /board/VSWT5V0)
  (net 8 /board/DIO_N1)
  (net 9 /board/DIO_P1)
  (net 10 /board/DIO_N4)
  (net 11 /board/DIO_P4)
  (net 12 /board/DIO_N3)
  (net 13 /board/DIO_P3)
  (net 14 /board/DIO_N2)
  (net 15 /board/DIO_P2)
  (net 16 +5V)
  (net 17 /power/VCC5VBOOST)
  (net 18 "Net-(R403-Pad2)")
  (net 19 /board/CDIO_P1)
  (net 20 /board/CDIO_N1)
  (net 21 /board/CDIO_P2)
  (net 22 /board/CDIO_N2)
  (net 23 /board/CDIO_P3)
  (net 24 /board/CDIO_N3)
  (net 25 /board/CDIO_P4)
  (net 26 /board/CDIO_N4)
  (net 27 /board/CI2C_SCL)
  (net 28 /board/CI2C_SDA)
  (net 29 /board/CCEC)
  (net 30 /board/I2CEN)
  (net 31 /board/~OE)
  (net 32 /board/PRE)
  (net 33 /board/OVS)
  (net 34 /board/VSADJ)
  (net 35 /rpt_connector/I2C1_SDA)
  (net 36 /rpt_connector/I2C1_SCL)
  (net 37 -3V3)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.3)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net +3V3)
    (add_net +5V)
    (add_net -3V3)
    (add_net /VCC5V0)
    (add_net /board/CCEC)
    (add_net /board/CDIO_N1)
    (add_net /board/CDIO_N2)
    (add_net /board/CDIO_N3)
    (add_net /board/CDIO_N4)
    (add_net /board/CDIO_P1)
    (add_net /board/CDIO_P2)
    (add_net /board/CDIO_P3)
    (add_net /board/CDIO_P4)
    (add_net /board/CI2C_SCL)
    (add_net /board/CI2C_SDA)
    (add_net /board/DIO_N1)
    (add_net /board/DIO_N2)
    (add_net /board/DIO_N3)
    (add_net /board/DIO_N4)
    (add_net /board/DIO_P1)
    (add_net /board/DIO_P2)
    (add_net /board/DIO_P3)
    (add_net /board/DIO_P4)
    (add_net /board/I2CEN)
    (add_net /board/OVS)
    (add_net /board/PRE)
    (add_net /board/SHIELD)
    (add_net /board/VSADJ)
    (add_net /board/VSWT5V0)
    (add_net /board/~OE)
    (add_net /power/VCC5VBOOST)
    (add_net /rpt_connector/I2C1_SCL)
    (add_net /rpt_connector/I2C1_SDA)
    (add_net GND)
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C402-Pad2)")
    (add_net "Net-(R403-Pad2)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.9)
    (via_drill 0.45)
    (uvia_dia 0.8)
    (uvia_drill 0.3)
    (diff_pair_width 0.25)
    (diff_pair_gap 0.25)
  )
  (module custom_device:QFN50P600X600X100-41N-D locked (layer Top) (tedit 5DE78CF7)
    (at 133.5 79.75 90)
    (descr TMDS141RHAR)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC401 (at 3.95 -7.2 180) (layer F.SilkS))
    (fp_text value TMDS141RHAR (at 0 -4.9 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2.65 4.7 90) (layer F.Fab))
    (pad 41 thru_hole circle (at 1 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at 0 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at -1 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at 1 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at -1 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at 1 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at 0 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 41 thru_hole circle (at -1 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.95 -2.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /board/DIO_N1))
    (pad 2 smd rect (at -2.95 -1.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 9 /board/DIO_P1))
    (pad 3 smd rect (at -2.95 -1.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.95 -0.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 5 smd rect (at -2.95 -0.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 30 /board/I2CEN))
    (pad 6 smd rect (at -2.95 0.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 31 /board/~OE))
    (pad 7 smd rect (at -2.95 0.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 32 /board/PRE))
    (pad 8 smd rect (at -2.95 1.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -2.95 1.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 19 /board/CDIO_P1))
    (pad 10 smd roundrect (at -2.95 2.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /board/CDIO_N1))
    (pad 11 smd roundrect (at -2.25 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 12 smd rect (at -1.75 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 21 /board/CDIO_P2))
    (pad 13 smd rect (at -1.25 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 22 /board/CDIO_N2))
    (pad 14 smd rect (at -0.75 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at -0.25 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 23 /board/CDIO_P3))
    (pad 16 smd rect (at 0.25 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 24 /board/CDIO_N3))
    (pad 17 smd rect (at 0.75 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 18 smd rect (at 1.25 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 25 /board/CDIO_P4))
    (pad 19 smd rect (at 1.75 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 26 /board/CDIO_N4))
    (pad 20 smd roundrect (at 2.25 2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 21 smd roundrect (at 2.95 2.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 22 smd rect (at 2.95 1.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 27 /board/CI2C_SCL))
    (pad 23 smd rect (at 2.95 1.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 28 /board/CI2C_SDA))
    (pad 24 smd rect (at 2.95 0.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 25 smd rect (at 2.95 0.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 33 /board/OVS))
    (pad 26 smd rect (at 2.95 -0.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at 2.95 -0.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 28 smd rect (at 2.95 -1.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 35 /rpt_connector/I2C1_SDA))
    (pad 29 smd rect (at 2.95 -1.75 180) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 36 /rpt_connector/I2C1_SCL))
    (pad 30 smd roundrect (at 2.95 -2.25 180) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /board/VSADJ))
    (pad 31 smd roundrect (at 2.25 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 32 smd rect (at 1.75 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 10 /board/DIO_N4))
    (pad 33 smd rect (at 1.25 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 11 /board/DIO_P4))
    (pad 34 smd rect (at 0.75 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 35 smd rect (at 0.25 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 12 /board/DIO_N3))
    (pad 36 smd rect (at -0.25 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 13 /board/DIO_P3))
    (pad 37 smd rect (at -0.75 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 38 smd rect (at -1.25 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 14 /board/DIO_N2))
    (pad 39 smd rect (at -1.75 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask)
      (net 15 /board/DIO_P2))
    (pad 40 smd roundrect (at -2.25 -2.95 90) (size 0.3 0.9) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 41 smd rect (at 0 0 90) (size 3 3) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model /home/primozb/src/svnrepos/myZynq/hw/libraries/packages3d/device/TMDS141RHAR.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Top) (tedit 5A0F774F)
    (at 125.05 98.75)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP401 (at -0.15 -1.525 180) (layer F.SilkS))
    (fp_text value TP_3V3 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 2 +3V3))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Top) (tedit 5A0F774F)
    (at 152.025 58.6)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP404 (at -1.3 -3.125 90) (layer F.SilkS))
    (fp_text value TP_5V0 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 4 /VCC5V0))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Top) (tedit 5A0F774F)
    (at 123.425 49.575)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP403 (at -3.425 -0.625) (layer F.SilkS))
    (fp_text value TP_-3V (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 37 -3V3))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Top) (tedit 5A0F774F)
    (at 130.25 49.6)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP402 (at 0.075 1.825) (layer F.SilkS))
    (fp_text value TP_5V (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 16 +5V))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Top) (tedit 5A0F774F)
    (at 152.65 65.975)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP301 (at 1.3 2) (layer F.SilkS))
    (fp_text value TP_WT5V0 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 7 /board/VSWT5V0))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Top) (tedit 5A0F774F)
    (at 132.375 60.625)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP202 (at 1.75 0.05 90) (layer F.SilkS))
    (fp_text value TP_SDA (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 35 /rpt_connector/I2C1_SDA))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Top) (tedit 5A0F774F)
    (at 128.175 60.575)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP201 (at -2.2 2.25 90) (layer F.SilkS))
    (fp_text value TP_SCL (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 36 /rpt_connector/I2C1_SCL))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical locked (layer Top) (tedit 59FED5CC)
    (at 86.68 45.89)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J402 (at 0 -2.33) (layer F.SilkS))
    (fp_text value TP_GND (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6_Handsoldering (layer Top) (tedit 5A02FF57)
    (at 142.7 53.7 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U401 (at 0.2 2.6 90) (layer F.SilkS))
    (fp_text value REG710-DBV (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.35 0 270) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 2 +3V3))
    (pad 6 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C402-Pad1)"))
    (pad 4 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 5 "Net-(C402-Pad2)"))
    (pad 3 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 18 "Net-(R403-Pad2)"))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 17 /power/VCC5VBOOST))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 137.4 53.7 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R403 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(R403-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 154.7 55.85 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R402 (at 0 1.7 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 /VCC5V0))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 /power/VCC5VBOOST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 158.6 55.9 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R401 (at 0 1.7 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 /VCC5V0))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 164.75 64 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R313 (at 0 1.8 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 /board/SHIELD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 150.1 69 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R312 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 29 /board/CCEC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 146.05 68.975 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R311 (at 0.125 1.85 90) (layer F.SilkS))
    (fp_text value 1.74k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 27 /board/CI2C_SCL))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 /board/VSWT5V0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 141.9 68.975 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R310 (at 0.125 1.8 90) (layer F.SilkS))
    (fp_text value 1.74k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 28 /board/CI2C_SDA))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 /board/VSWT5V0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 127.6 72.3 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R309 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.64k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 /board/VSADJ))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 131.3 65.85 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R308 (at 0.225 -3.4 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 33 /board/OVS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 134.6 65.85 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R307 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 33 /board/OVS))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 140 95.2 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R306 (at 0.1 1.9 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 32 /board/PRE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 136.1 95.2 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R305 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 32 /board/PRE))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 132.3 95.2 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R304 (at 0.1 2 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 31 /board/~OE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 128.3 95.1875 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R303 (at 1.0375 -1.8 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 30 /board/I2CEN))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 132.375 55.8 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R302 (at -1.45 1.975 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 35 /rpt_connector/I2C1_SDA))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBD)
    (at 128.175 55.825 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R301 (at 0.35 2.375 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 36 /rpt_connector/I2C1_SCL))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_conn:HDMI_10029449-112 locked (layer Bottom) (tedit 5DCA913A)
    (at 165 78.5 270)
    (descr "HSMI 10029449-112")
    (tags Connector)
    (fp_text reference J401 (at 11.88 7.13) (layer F.SilkS))
    (fp_text value 10029449-112 (at 0.05 -7.5 270) (layer B.SilkS) hide)
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 4 5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 3.25 3.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 21 /board/CDIO_P2))
    (pad 3 thru_hole circle (at 3.25 6.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 20 /board/CDIO_N1))
    (pad 5 thru_hole circle (at 2.5 5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 1.75 3.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 /board/CDIO_N2))
    (pad 7 thru_hole circle (at 1.75 6.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 23 /board/CDIO_P3))
    (pad 8 thru_hole circle (at 1 5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 0.25 3.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 /board/CDIO_P4))
    (pad 9 thru_hole circle (at 0.25 6.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 /board/CDIO_N3))
    (pad 11 thru_hole circle (at -0.5 5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at -1.25 3.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 /board/CDIO_N4))
    (pad 13 thru_hole circle (at -1.25 6.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 /board/CCEC))
    (pad 14 thru_hole circle (at -2 5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -2.75 3.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 28 /board/CI2C_SDA))
    (pad 15 thru_hole circle (at -2.75 6.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 27 /board/CI2C_SCL))
    (pad 17 thru_hole circle (at -3.5 5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole circle (at -4.25 3.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 /board/VSWT5V0))
    (pad 19 thru_hole circle (at -4.25 6.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 4.75 6.5 270) (size 0.95 0.95) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 /board/CDIO_P1))
    (pad MH1 thru_hole oval (at 7.25 4.16 270) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 /board/SHIELD))
    (pad MH2 thru_hole oval (at 7.85 -1.8 270) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 /board/SHIELD))
    (pad MH3 thru_hole oval (at -7.25 4.16 270) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 /board/SHIELD))
    (pad MH4 thru_hole oval (at -7.9 -1.8 270) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 /board/SHIELD))
    (pad "" np_thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model /home/primozb/src/svnrepos/myZynq/hw/libraries/packages3d/conn/1746679-1.stp
      (offset (xyz 0 -5.5 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module custom_conn:Samtec_ESQT-103-02-F-D_P2.00mm locked (layer Bottom) (tedit 5DCDB45A)
    (at 82.575 62.175 175)
    (descr "Through hole straight socket strip, 2x03, 2.00mm pitch, double cols, Clock Wise pins")
    (tags "Through hole socket strip THT 2x03 2.00mm double row")
    (fp_text reference J302 (at -1 -6.429 175) (layer F.SilkS))
    (fp_text value CN17 (at -1 -6.5 175) (layer F.Fab))
    (fp_text user %R (at -1 -2 265) (layer B.Fab))
    (pad 4 thru_hole oval (at -2 -4 175) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -4 175) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at -2 -2 175) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2 175) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2 0 175) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 175) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model /home/primozb/src/svnrepos/myZynq/hw/libraries/packages3d/conn/Samtec_ESQT-103-02-F-D-320.stp
      (offset (xyz -1 -2 13.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module custom_conn:Samtec_ESQT-103-02-F-D_P2.00mm locked (layer Bottom) (tedit 5DCDB45A)
    (at 84.925 50.775 165)
    (descr "Through hole straight socket strip, 2x03, 2.00mm pitch, double cols, Clock Wise pins")
    (tags "Through hole socket strip THT 2x03 2.00mm double row")
    (fp_text reference J301 (at -1 -6.559 165) (layer F.SilkS))
    (fp_text value CN16 (at -1 -6.5 165) (layer F.Fab))
    (fp_text user %R (at -1 -2 255) (layer B.Fab))
    (pad 4 thru_hole oval (at -2 -4 165) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -4 165) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at -2 -2 165) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2 165) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2 0 165) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 165) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model /home/primozb/src/svnrepos/myZynq/hw/libraries/packages3d/conn/Samtec_ESQT-103-02-F-D-320.stp
      (offset (xyz -1 -2 13.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer Top) (tedit 5A0AB76C)
    (at 157 62.125 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D401 (at -0.125 2.5 90) (layer F.SilkS))
    (fp_text value BAT54 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers Top F.Paste F.Mask)
      (net 7 /board/VSWT5V0))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers Top F.Paste F.Mask))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers Top F.Paste F.Mask)
      (net 4 /VCC5V0))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 137.4 59.2 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C403 (at 0.1 1.7 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 141.75 59.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C402 (at -4.725 -0.475 90) (layer F.SilkS))
    (fp_text value 220n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C402-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(C402-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBE)
    (at 148.575 60.075 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C401 (at 0.1 1.8 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 /VCC5V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Top) (tedit 5B301BBE)
    (at 164.75 57.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C309 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1nF/250V (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers Top F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 /board/SHIELD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 132.025 71.8 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C308 (at 0.3 2.7 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 140.95 79 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C307 (at 0.15 2.3) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 140.975 82.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C306 (at -0.1 -3.2 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 128.3 86.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C305 (at 0.075 1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 134.6 71.8 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C304 (at -0.025 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 132.75 87.75 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C303 (at 0.275 3.1 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0.05 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 126 79)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C302 (at -4.925 -0.125) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer Top) (tedit 5B36C52B)
    (at 125.775 88 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C301 (at 0.1 1.7 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers Top F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducial:Fiducial_1mm_Mask2mm (layer Top) (tedit 5C18CB26)
    (at 167.25 50)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID102 (at -4 0.25) (layer F.SilkS))
    (fp_text value Fiducial (at 5.25 0.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial:Fiducial_1mm_Mask2mm (layer Top) (tedit 5C18CB26)
    (at 86.75 98.25)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID101 (at 0 -4 90) (layer F.SilkS))
    (fp_text value Fiducial (at 0.5 2.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module custom_conn:Samtec_ESQ-113-44-T-D locked (layer Bottom) (tedit 5DC8777B)
    (at 120.81 43.33 90)
    (descr "Through hole straight Elevated socket strip, 2x13, 2.54mm pitch, double cols")
    (tags "Through hole elevated socket strip THT 2x13 2.54mm double row")
    (fp_text reference J303 (at -5.32 -30.76 180) (layer F.SilkS))
    (fp_text value E2 (at -1.17 2.69 90) (layer F.Fab))
    (fp_text user %R (at -1.27 -15.24 180) (layer B.Fab))
    (pad 26 thru_hole oval (at -2.54 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at -2.54 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at -2.54 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at -2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at -2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at -2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /rpt_connector/I2C1_SDA))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /rpt_connector/I2C1_SCL))
    (pad 4 thru_hole oval (at -2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 -3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x13_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/primozb/src/svnrepos/myZynq/hw/libraries/packages3d/conn/Samtec_ESQ-113-44-T-D.stp
      (offset (xyz -1.5 -15 11.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module custom_conn:Samtec_ESQ-113-44-T-D locked (layer Bottom) (tedit 5DC8777B)
    (at 120.81 94.13 90)
    (descr "Through hole straight Elevated socket strip, 2x13, 2.54mm pitch, double cols")
    (tags "Through hole elevated socket strip THT 2x13 2.54mm double row")
    (fp_text reference J304 (at 2.855 -30.56 180) (layer F.SilkS))
    (fp_text value E1 (at -1.27 2.69 90) (layer F.Fab))
    (fp_text user %R (at -1.27 -15.24 180) (layer B.Fab))
    (pad 26 thru_hole oval (at -2.54 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at -2.54 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at -2.54 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at -2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at -2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at -2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /board/DIO_N4))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /board/DIO_P4))
    (pad 8 thru_hole oval (at -2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /board/DIO_N3))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /board/DIO_P3))
    (pad 6 thru_hole oval (at -2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /board/DIO_N2))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /board/DIO_P2))
    (pad 4 thru_hole oval (at -2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /board/DIO_N1))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /board/DIO_P1))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x13_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/primozb/src/svnrepos/myZynq/hw/libraries/packages3d/conn/Samtec_ESQ-113-44-T-D.stp
      (offset (xyz -1.5 -15 11.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer Top) (tedit 56D1B4CB)
    (at 82 43)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H101 (at 0 4) (layer F.SilkS))
    (fp_text value 3.2mm (at -6 -1.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer Top) (tedit 56D1B4CB)
    (at 82 97)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.8) (layer F.SilkS))
    (fp_text value 3.2mm (at -5.75 1.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer Top) (tedit 56D1B4CB)
    (at 166 43)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H103 (at 0 4) (layer F.SilkS))
    (fp_text value 3.2mm (at 5.75 -1.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer Top) (tedit 56D1B4CB)
    (at 166 97)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.8) (layer F.SilkS))
    (fp_text value 3.2mm (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (dimension 54 (width 0.15) (layer Dwgs.User)
    (gr_text "54,000 mm" (at 66.95 70 270) (layer Dwgs.User))
    (feature1 (pts (xy 82 97) (xy 67.663579 97)))
    (feature2 (pts (xy 82 43) (xy 67.663579 43)))
    (crossbar (pts (xy 68.25 43) (xy 68.25 97)))
    (arrow1a (pts (xy 68.25 97) (xy 67.663579 95.873496)))
    (arrow1b (pts (xy 68.25 97) (xy 68.836421 95.873496)))
    (arrow2a (pts (xy 68.25 43) (xy 67.663579 44.126504)))
    (arrow2b (pts (xy 68.25 43) (xy 68.836421 44.126504)))
  )
  (dimension 84 (width 0.15) (layer Dwgs.User)
    (gr_text "84,000 mm" (at 124 112.049999) (layer Dwgs.User))
    (feature1 (pts (xy 166 97) (xy 166 111.33642)))
    (feature2 (pts (xy 82 97) (xy 82 111.33642)))
    (crossbar (pts (xy 82 110.749999) (xy 166 110.749999)))
    (arrow1a (pts (xy 166 110.749999) (xy 164.873496 111.33642)))
    (arrow1b (pts (xy 166 110.749999) (xy 164.873496 110.163578)))
    (arrow2a (pts (xy 82 110.749999) (xy 83.126504 111.33642)))
    (arrow2b (pts (xy 82 110.749999) (xy 83.126504 110.163578)))
  )
  (gr_line (start 166 40) (end 162 40) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 126 48) (end 126 40) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 162 48) (end 126 48) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 162 40) (end 162 48) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 166 100) (end 162 100) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 143 92) (end 143 100) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 162 92) (end 143 92) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 162 100) (end 162 92) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 166 97) (end 166 100) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 166 43) (end 169 43) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 82 97) (end 79.000001 97.999999) (angle -53.1) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 82 43) (end 81.000001 40.000001) (angle -53.1) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 75 57) (end 79 42) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 74 70) (end 75 57) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 75.5 83) (end 79 98) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 74 70) (end 75.5 83) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 126 40) (end 81 40) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 169 97) (end 169 43) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 80.998424 99.999473) (end 143 100) (layer Edge.Cuts) (width 0.4))
  (dimension 60 (width 0.15) (layer Dwgs.User)
    (gr_text "60,000 mm" (at 60.7 70 270) (layer Dwgs.User))
    (feature1 (pts (xy 74 100) (xy 61.413579 100)))
    (feature2 (pts (xy 74 40) (xy 61.413579 40)))
    (crossbar (pts (xy 62 40) (xy 62 100)))
    (arrow1a (pts (xy 62 100) (xy 61.413579 98.873496)))
    (arrow1b (pts (xy 62 100) (xy 62.586421 98.873496)))
    (arrow2a (pts (xy 62 40) (xy 61.413579 41.126504)))
    (arrow2b (pts (xy 62 40) (xy 62.586421 41.126504)))
  )
  (dimension 95 (width 0.15) (layer Dwgs.User)
    (gr_text "95,000 mm" (at 121.5 26.7) (layer Dwgs.User))
    (feature1 (pts (xy 169 40) (xy 169 27.413579)))
    (feature2 (pts (xy 74 40) (xy 74 27.413579)))
    (crossbar (pts (xy 74 28) (xy 169 28)))
    (arrow1a (pts (xy 169 28) (xy 167.873496 28.586421)))
    (arrow1b (pts (xy 169 28) (xy 167.873496 27.413579)))
    (arrow2a (pts (xy 74 28) (xy 75.126504 28.586421)))
    (arrow2b (pts (xy 74 28) (xy 75.126504 27.413579)))
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173 102.5) (xy 73 102.5) (xy 73 37.5) (xy 173 37.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174 103) (xy 72 103) (xy 72 37) (xy 174 37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.95 77.2) (xy 129.6 77.2) (xy 129.6 75.95) (xy 130.95 75.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.25 77.2) (xy 136.05 77.2) (xy 136.05 75.95) (xy 137.25 75.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.25 83.55) (xy 136.05 83.55) (xy 136.05 82.3) (xy 137.25 82.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.95 83.55) (xy 129.6 83.55) (xy 129.6 82.3) (xy 130.95 82.3)
      )
    )
  )
)
