<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>ERR</text>
<text>STS</text>
<wire x1="45.72" y1="41.91" x2="0" y2="41.91" width="0" layer="20"/>
<wire x1="0" y1="41.91" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="45.72" y2="0" width="0" layer="20"/>
<wire x1="51.054" y1="39.37" x2="51.054" y2="24.13" width="0" layer="20"/>
<wire x1="51.054" y1="24.13" x2="46.99" y2="24.13" width="0" layer="20"/>
<hole x="45.72" y="25.273" drill="0.508"/>
<hole x="45.72" y="24.384" drill="0.508"/>
<hole x="45.72" y="30.988" drill="0.508"/>
<hole x="45.72" y="31.75" drill="0.381"/>
<hole x="45.72" y="32.512" drill="0.508"/>
<hole x="45.72" y="38.227" drill="0.508"/>
<hole x="45.72" y="39.116" drill="0.508"/>
<wire x1="45.72" y1="40.386" x2="46.736" y2="39.37" width="0" layer="20" curve="90"/>
<wire x1="45.72" y1="40.386" x2="45.72" y2="41.91" width="0" layer="20"/>
<wire x1="46.736" y1="39.37" x2="51.054" y2="39.37" width="0" layer="20"/>
<text>3V3</text>
<text>LIPO BATTERY
INTERNAL
RESISTANCE
CHECKER</text>
<text>LIPO IR CALC REV1
TIM KOSTKA | 2016-DEC-08</text>
<text>LIPO IR CALC REV2
TIM KOSTKA | 2016-DEC-08</text>
<wire x1="45.72" y1="0" x2="45.72" y2="22.86" width="0" layer="20"/>
<wire x1="45.72" y1="22.86" x2="46.99" y2="24.13" width="0" layer="20" curve="-90"/>
</plain>
<libraries>
<library name="kcl_connectors">
<packages>
<package name="XT60-MALE-EDGE-3">
</package>
<package name="SAM-FTSH-105-XX-X-DV-K">
</package>
<package name="MODULE-OLED-1P3-HOLES">
</package>
</packages>
</library>
<library name="kcl_ics">
<packages>
<package name="SOT23-3">
<description>TI's DBV package (R-PDSO-G3)</description>
</package>
<package name="SO8-POWERPAK">
<description>Vishay</description>
</package>
<package name="UFQFPN48EP-7X7MM-HANDSOLDER">
</package>
<package name="SOT23-5">
<description>TI's SOT23-5 PACKAGE
DVB (R-PDSO-G5)</description>
</package>
</packages>
</library>
<library name="kcl_passives">
<packages>
<package name="CHIPLED0805">
</package>
<package name="C0805R">
<description>Chip capacitor land pattern, reflow soldering, size 0805.</description>
</package>
<package name="RES0805R">
<description>Vishay MCU 0805 resistor footprint for reflow soldering.</description>
</package>
<package name="SOD-123">
<description>SOD-123 case from On Semi.
Case 425-04, issue G.</description>
</package>
<package name="RIEDON-PFC">
</package>
</packages>
</library>
<library name="kcl_connectors_auto">
<packages>
<package name="SAM-TSW-107-XX-X-S-RA">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="kcl_connectors" package="XT60-MALE-EDGE-3" value="BATTERY-CONNXT60-MALE-EDGE3">
<attribute name="NAME"/>
</element>
<element name="M1" library="kcl_ics" package="SO8-POWERPAK" value="MOSFET-NSI7460DP">
<attribute name="PN" value="PSMN9R1-30YL,115"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="kcl_ics" package="UFQFPN48EP-7X7MM-HANDSOLDER" value="STM32F411-48UFQFPN48EP-HANDSOLDER">
<attribute name="PN" value="STM32F411CEU6"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="kcl_passives" package="C0805R" value="0.1uF">
<attribute name="PN" value="C0805C104K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="kcl_passives" package="C0805R" value="0.1uF">
<attribute name="PN" value="C0805C104K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="kcl_passives" package="C0805R" value="0.1uF">
<attribute name="PN" value="C0805C104K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="kcl_passives" package="C0805R" value="0.1uF">
<attribute name="PN" value="C0805C104K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="kcl_passives" package="C0805R" value="2.2uF">
<attribute name="PN" value="C0805C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="kcl_passives" package="C0805R" value="0.1uF">
<attribute name="PN" value="C0805C104K5RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="kcl_passives" package="RES0805R" value="10K">
<attribute name="PN" value="CRCW080510K0FKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="kcl_passives" package="CHIPLED0805" value="BLU">
<attribute name="PN" value="150080BS75000"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="kcl_passives" package="CHIPLED0805" value="RED">
<attribute name="PN" value="150080RS75000"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="kcl_passives" package="RES0805R" value="10K">
<attribute name="PN" value="CRCW080510K0FKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="kcl_passives" package="RES0805R" value="10K">
<attribute name="PN" value="CRCW080510K0FKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="kcl_passives" package="RES0805R" value="10K">
<attribute name="PN" value="CRCW080510K0FKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="kcl_passives" package="CHIPLED0805" value="GRN">
<attribute name="PN" value="150080GS75000"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="kcl_connectors" package="SAM-FTSH-105-XX-X-DV-K" value="CONN2X05FTSH">
<attribute name="PN" value="FTSH-105-01-L-DV-K"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="kcl_passives" package="C0805R" value="2.2uF">
<attribute name="PN" value="C0805C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="kcl_passives" package="C0805R" value="2.2uF">
<attribute name="PN" value="C0805C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="kcl_ics" package="SOT23-5" value="MIC5219">
<attribute name="PN" value="MIC5225-3.3YM5-TR"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="kcl_passives" package="RES0805R" value="10K">
<attribute name="PN" value="CRCW080510K0FKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="kcl_passives" package="SOD-123" value="SCHOTTKYSOD-123">
<attribute name="PN" value="B0520LW-7-F"/>
<attribute name="NAME"/>
</element>
<element name="J3" library="kcl_connectors" package="MODULE-OLED-1P3-HOLES" value="OLED-MODULE1P3-HOLES"/>
<element name="D1" library="kcl_passives" package="SOD-123" value="4V">
<attribute name="NAME"/>
</element>
<element name="J1" library="kcl_connectors_auto" package="SAM-TSW-107-XX-X-S-RA" value="CONN7TSW-S-RA">
<attribute name="PN" value="TSW-102-08-F-S-RA"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="kcl_passives" package="RES0805R" value="10K">
<attribute name="PN" value="CRCW080510K0FKEA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="kcl_passives" package="RES0805R" value="56K">
<attribute name="PN" value="RT0805BRD0756KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="kcl_passives" package="RES0805R" value="16K">
<attribute name="PN" value="RT0805BRD0716KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="kcl_passives" package="RES0805R" value="2.4K">
<attribute name="PN" value="RT0805BRD072K4L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M2" library="kcl_ics" package="SOT23-3" value="MOSFET-NSOT23-3">
<attribute name="PN" value="DMN62D0U-7"/>
<attribute name="NAME"/>
</element>
<element name="R29" library="kcl_passives" package="RIEDON-PFC" value="1">
<attribute name="NAME"/>
<attribute name="PN" value="PFC10-1RF1"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="NEG1"/>
<contactref element="J2" pad="NEG2"/>
<contactref element="J2" pad="NEG10"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="PAD"/>
<contactref element="C5" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="J4" pad="9"/>
<contactref element="J4" pad="5"/>
<contactref element="J4" pad="3"/>
<contactref element="R17" pad="2"/>
<contactref element="M1" pad="3"/>
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="2"/>
<contactref element="J3" pad="GND"/>
<contactref element="D1" pad="A"/>
<contactref element="R24" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="U1" pad="44"/>
</signal>
<signal name="N$1">
<contactref element="M1" pad="5"/>
<contactref element="M1" pad="6"/>
<contactref element="M1" pad="7"/>
<contactref element="M1" pad="8"/>
<contactref element="M1" pad="PAD"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="POS1"/>
<contactref element="J2" pad="POS2"/>
<contactref element="J2" pad="POS3"/>
<contactref element="R9" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="M2" pad="3"/>
<contactref element="R29" pad="2"/>
<contactref element="R29" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="J4" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="48"/>
<contactref element="U1" pad="36"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="J3" pad="VIN"/>
<contactref element="R1" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="NRST">
<contactref element="U1" pad="7"/>
<contactref element="R32" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="J4" pad="10"/>
</signal>
<signal name="SWDIO">
<contactref element="U1" pad="34"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="U1" pad="37"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="USART1_TX">
<contactref element="J4" pad="8"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="SPI1_SCK1">
</signal>
<signal name="SPI1_MISO1">
</signal>
<signal name="SPI1_MOSI1">
</signal>
<signal name="SPI1_SCK2">
</signal>
<signal name="SPI1_MISO2">
</signal>
<signal name="SPI1_MOSI2">
</signal>
<signal name="SPI1_SCK3">
</signal>
<signal name="SPI1_MISO3">
</signal>
<signal name="SPI1_MOSI3">
</signal>
<signal name="N$23">
<contactref element="R34" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="R35" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="LED_ERR">
<contactref element="R35" pad="1"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="LED_STS">
<contactref element="R34" pad="1"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="N$35">
<contactref element="R33" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="22"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="SPI1_SCK4">
</signal>
<signal name="SPI1_MISO4">
</signal>
<signal name="SPI1_MOSI4">
</signal>
<signal name="SPI1_SCK5">
</signal>
<signal name="SPI1_MISO5">
</signal>
<signal name="SPI1_MOSI5">
</signal>
<signal name="SPI1_SCK6">
</signal>
<signal name="SPI1_MISO6">
</signal>
<signal name="SPI1_MOSI6">
</signal>
<signal name="SPI1_SCK7">
</signal>
<signal name="SPI1_MISO7">
</signal>
<signal name="SPI1_MOSI7">
</signal>
<signal name="SPI1_SCK8">
</signal>
<signal name="SPI1_MISO8">
</signal>
<signal name="SPI1_MOSI8">
</signal>
<signal name="SPI1_SCK9">
</signal>
<signal name="SPI1_MISO9">
</signal>
<signal name="SPI1_MOSI9">
</signal>
<signal name="SPI1_SCK10">
</signal>
<signal name="SPI1_MISO10">
</signal>
<signal name="SPI1_MOSI10">
</signal>
<signal name="SPI1_SCK11">
</signal>
<signal name="SPI1_MISO11">
</signal>
<signal name="SPI1_MOSI11">
</signal>
<signal name="SPI1_SCK12">
</signal>
<signal name="SPI1_MISO12">
</signal>
<signal name="SPI1_MOSI12">
</signal>
<signal name="SPI1_SCK13">
</signal>
<signal name="SPI1_MISO13">
</signal>
<signal name="SPI1_MOSI13">
</signal>
<signal name="SPI1_SCK14">
</signal>
<signal name="SPI1_MISO14">
</signal>
<signal name="SPI1_MOSI14">
</signal>
<signal name="SPI1_SCK15">
</signal>
<signal name="SPI1_MISO15">
</signal>
<signal name="SPI1_MOSI15">
</signal>
<signal name="SPI1_SCK16">
</signal>
<signal name="SPI1_MISO16">
</signal>
<signal name="SPI1_MOSI16">
</signal>
<signal name="SPI1_SCK17">
</signal>
<signal name="SPI1_MISO17">
</signal>
<signal name="SPI1_MOSI17">
</signal>
<signal name="SPI1_SCK18">
</signal>
<signal name="SPI1_MISO18">
</signal>
<signal name="SPI1_MOSI18">
</signal>
<signal name="SPI1_SCK19">
</signal>
<signal name="SPI1_MISO19">
</signal>
<signal name="SPI1_MOSI19">
</signal>
<signal name="SPI1_SCK20">
</signal>
<signal name="SPI1_MISO20">
</signal>
<signal name="SPI1_MOSI20">
</signal>
<signal name="SPI1_SCK21">
</signal>
<signal name="SPI1_MISO21">
</signal>
<signal name="SPI1_MOSI21">
</signal>
<signal name="SPI1_SCK22">
</signal>
<signal name="SPI1_MISO22">
</signal>
<signal name="SPI1_MOSI22">
</signal>
<signal name="SPI1_SCK23">
</signal>
<signal name="SPI1_MISO23">
</signal>
<signal name="SPI1_MOSI23">
</signal>
<signal name="SPI1_SCK24">
</signal>
<signal name="SPI1_MISO24">
</signal>
<signal name="SPI1_MOSI24">
</signal>
<signal name="SPI1_SCK25">
</signal>
<signal name="SPI1_MISO25">
</signal>
<signal name="SPI1_MOSI25">
</signal>
<signal name="SPI1_SCK26">
</signal>
<signal name="SPI1_MISO26">
</signal>
<signal name="SPI1_MOSI26">
</signal>
<signal name="SPI1_SCK27">
</signal>
<signal name="SPI1_MISO27">
</signal>
<signal name="SPI1_MOSI27">
</signal>
<signal name="SPI1_SCK28">
</signal>
<signal name="SPI1_MISO28">
</signal>
<signal name="SPI1_MOSI28">
</signal>
<signal name="SPI1_SCK29">
</signal>
<signal name="SPI1_MISO29">
</signal>
<signal name="SPI1_MOSI29">
</signal>
<signal name="SPI1_SCK30">
</signal>
<signal name="SPI1_MISO30">
</signal>
<signal name="SPI1_MOSI30">
</signal>
<signal name="SPI1_SCK31">
</signal>
<signal name="SPI1_MISO31">
</signal>
<signal name="SPI1_MOSI31">
</signal>
<signal name="SPI1_SCK32">
</signal>
<signal name="SPI1_MISO32">
</signal>
<signal name="SPI1_MOSI32">
</signal>
<signal name="SPI1_SCK33">
</signal>
<signal name="SPI1_MISO33">
</signal>
<signal name="SPI1_MOSI33">
</signal>
<signal name="SPI1_SCK34">
</signal>
<signal name="SPI1_MISO34">
</signal>
<signal name="SPI1_MOSI34">
</signal>
<signal name="SPI1_SCK35">
</signal>
<signal name="SPI1_MISO35">
</signal>
<signal name="SPI1_MOSI35">
</signal>
<signal name="SPI1_SCK36">
</signal>
<signal name="SPI1_MISO36">
</signal>
<signal name="SPI1_MOSI36">
</signal>
<signal name="SPI1_SCK37">
</signal>
<signal name="SPI1_MISO37">
</signal>
<signal name="SPI1_MOSI37">
</signal>
<signal name="SPI1_SCK38">
</signal>
<signal name="SPI1_MISO38">
</signal>
<signal name="SPI1_MOSI38">
</signal>
<signal name="SPI1_SCK39">
</signal>
<signal name="SPI1_MISO39">
</signal>
<signal name="SPI1_MOSI39">
</signal>
<signal name="SPI1_SCK40">
</signal>
<signal name="SPI1_MISO40">
</signal>
<signal name="SPI1_MOSI40">
</signal>
<signal name="SPI1_SCK41">
</signal>
<signal name="SPI1_MISO41">
</signal>
<signal name="SPI1_MOSI41">
</signal>
<signal name="SPI1_SCK42">
</signal>
<signal name="SPI1_MISO42">
</signal>
<signal name="SPI1_MOSI42">
</signal>
<signal name="SPI1_SCK43">
</signal>
<signal name="SPI1_MISO43">
</signal>
<signal name="SPI1_MOSI43">
</signal>
<signal name="SPI1_SCK44">
</signal>
<signal name="SPI1_MISO44">
</signal>
<signal name="SPI1_MOSI44">
</signal>
<signal name="SPI1_SCK45">
</signal>
<signal name="SPI1_MISO45">
</signal>
<signal name="SPI1_MOSI45">
</signal>
<signal name="SPI1_SCK46">
</signal>
<signal name="SPI1_MISO46">
</signal>
<signal name="SPI1_MOSI46">
</signal>
<signal name="SPI1_SCK47">
</signal>
<signal name="SPI1_MISO47">
</signal>
<signal name="SPI1_MOSI47">
</signal>
<signal name="SPI1_SCK48">
</signal>
<signal name="SPI1_MISO48">
</signal>
<signal name="SPI1_MOSI48">
</signal>
<signal name="SPI1_SCK49">
</signal>
<signal name="SPI1_MISO49">
</signal>
<signal name="SPI1_MOSI49">
</signal>
<signal name="SPI1_SCK50">
</signal>
<signal name="SPI1_MISO50">
</signal>
<signal name="SPI1_MOSI50">
</signal>
<signal name="SPI1_SCK51">
</signal>
<signal name="SPI1_MISO51">
</signal>
<signal name="SPI1_MOSI51">
</signal>
<signal name="SPI1_SCK52">
</signal>
<signal name="SPI1_MISO52">
</signal>
<signal name="SPI1_MOSI52">
</signal>
<signal name="SPI1_SCK53">
</signal>
<signal name="SPI1_MISO53">
</signal>
<signal name="SPI1_MOSI53">
</signal>
<signal name="SPI1_SCK54">
</signal>
<signal name="SPI1_MISO54">
</signal>
<signal name="SPI1_MOSI54">
</signal>
<signal name="SPI1_SCK55">
</signal>
<signal name="SPI1_MISO55">
</signal>
<signal name="SPI1_MOSI55">
</signal>
<signal name="SPI1_SCK56">
</signal>
<signal name="SPI1_MISO56">
</signal>
<signal name="SPI1_MOSI56">
</signal>
<signal name="SPI1_SCK57">
</signal>
<signal name="SPI1_MISO57">
</signal>
<signal name="SPI1_MOSI57">
</signal>
<signal name="SPI1_SCK58">
</signal>
<signal name="SPI1_MISO58">
</signal>
<signal name="SPI1_MOSI58">
</signal>
<signal name="SPI1_SCK59">
</signal>
<signal name="SPI1_MISO59">
</signal>
<signal name="SPI1_MOSI59">
</signal>
<signal name="SPI1_SCK60">
</signal>
<signal name="SPI1_MISO60">
</signal>
<signal name="SPI1_MOSI60">
</signal>
<signal name="SPI1_SCK61">
</signal>
<signal name="SPI1_MISO61">
</signal>
<signal name="SPI1_MOSI61">
</signal>
<signal name="SPI1_SCK62">
</signal>
<signal name="SPI1_MISO62">
</signal>
<signal name="SPI1_MOSI62">
</signal>
<signal name="SPI1_SCK63">
</signal>
<signal name="SPI1_MISO63">
</signal>
<signal name="SPI1_MOSI63">
</signal>
<signal name="SPI1_SCK64">
</signal>
<signal name="SPI1_MISO64">
</signal>
<signal name="SPI1_MOSI64">
</signal>
<signal name="SPI1_SCK65">
</signal>
<signal name="SPI1_MISO65">
</signal>
<signal name="SPI1_MOSI65">
</signal>
<signal name="SPI1_SCK66">
</signal>
<signal name="SPI1_MISO66">
</signal>
<signal name="SPI1_MOSI66">
</signal>
<signal name="SPI1_SCK67">
</signal>
<signal name="SPI1_MISO67">
</signal>
<signal name="SPI1_MOSI67">
</signal>
<signal name="SPI1_SCK68">
</signal>
<signal name="SPI1_MISO68">
</signal>
<signal name="SPI1_MOSI68">
</signal>
<signal name="SPI1_SCK69">
</signal>
<signal name="SPI1_MISO69">
</signal>
<signal name="SPI1_MOSI69">
</signal>
<signal name="SPI1_SCK70">
</signal>
<signal name="SPI1_MISO70">
</signal>
<signal name="SPI1_MOSI70">
</signal>
<signal name="SPI1_SCK71">
</signal>
<signal name="SPI1_MISO71">
</signal>
<signal name="SPI1_MOSI71">
</signal>
<signal name="SPI1_SCK72">
</signal>
<signal name="SPI1_MISO72">
</signal>
<signal name="SPI1_MOSI72">
</signal>
<signal name="SPI1_SCK73">
</signal>
<signal name="SPI1_MISO73">
</signal>
<signal name="SPI1_MOSI73">
</signal>
<signal name="SPI1_SCK74">
</signal>
<signal name="SPI1_MISO74">
</signal>
<signal name="SPI1_MOSI74">
</signal>
<signal name="SPI1_SCK75">
</signal>
<signal name="SPI1_MISO75">
</signal>
<signal name="SPI1_MOSI75">
</signal>
<signal name="SPI1_SCK76">
</signal>
<signal name="SPI1_MISO76">
</signal>
<signal name="SPI1_MOSI76">
</signal>
<signal name="SPI1_SCK77">
</signal>
<signal name="SPI1_MISO77">
</signal>
<signal name="SPI1_MOSI77">
</signal>
<signal name="SPI1_SCK78">
</signal>
<signal name="SPI1_MISO78">
</signal>
<signal name="SPI1_MOSI78">
</signal>
<signal name="SPI1_SCK79">
</signal>
<signal name="SPI1_MISO79">
</signal>
<signal name="SPI1_MOSI79">
</signal>
<signal name="SPI1_SCK80">
</signal>
<signal name="SPI1_MISO80">
</signal>
<signal name="SPI1_MOSI80">
</signal>
<signal name="SPI1_SCK81">
</signal>
<signal name="SPI1_MISO81">
</signal>
<signal name="SPI1_MOSI81">
</signal>
<signal name="SPI1_SCK82">
</signal>
<signal name="SPI1_MISO82">
</signal>
<signal name="SPI1_MOSI82">
</signal>
<signal name="SPI1_SCK83">
</signal>
<signal name="SPI1_MISO83">
</signal>
<signal name="SPI1_MOSI83">
</signal>
<signal name="SPI1_SCK84">
</signal>
<signal name="SPI1_MISO84">
</signal>
<signal name="SPI1_MOSI84">
</signal>
<signal name="SPI1_SCK85">
</signal>
<signal name="SPI1_MISO85">
</signal>
<signal name="SPI1_MOSI85">
</signal>
<signal name="SPI1_SCK86">
</signal>
<signal name="SPI1_MISO86">
</signal>
<signal name="SPI1_MOSI86">
</signal>
<signal name="SPI1_SCK87">
</signal>
<signal name="SPI1_MISO87">
</signal>
<signal name="SPI1_MOSI87">
</signal>
<signal name="SPI1_SCK88">
</signal>
<signal name="SPI1_MISO88">
</signal>
<signal name="SPI1_MOSI88">
</signal>
<signal name="SPI1_SCK89">
</signal>
<signal name="SPI1_MISO89">
</signal>
<signal name="SPI1_MOSI89">
</signal>
<signal name="SPI1_SCK90">
</signal>
<signal name="SPI1_MISO90">
</signal>
<signal name="SPI1_MOSI90">
</signal>
<signal name="SPI1_SCK91">
</signal>
<signal name="SPI1_MISO91">
</signal>
<signal name="SPI1_MOSI91">
</signal>
<signal name="SPI1_SCK92">
</signal>
<signal name="SPI1_MISO92">
</signal>
<signal name="SPI1_MOSI92">
</signal>
<signal name="SPI1_SCK93">
</signal>
<signal name="SPI1_MISO93">
</signal>
<signal name="SPI1_MOSI93">
</signal>
<signal name="SPI1_SCK94">
</signal>
<signal name="SPI1_MISO94">
</signal>
<signal name="SPI1_MOSI94">
</signal>
<signal name="SPI1_SCK95">
</signal>
<signal name="SPI1_MISO95">
</signal>
<signal name="SPI1_MOSI95">
</signal>
<signal name="SPI1_SCK96">
</signal>
<signal name="SPI1_MISO96">
</signal>
<signal name="SPI1_MOSI96">
</signal>
<signal name="SPI1_SCK97">
</signal>
<signal name="SPI1_MISO97">
</signal>
<signal name="SPI1_MOSI97">
</signal>
<signal name="SPI1_SCK98">
</signal>
<signal name="SPI1_MISO98">
</signal>
<signal name="SPI1_MOSI98">
</signal>
<signal name="SPI1_SCK99">
</signal>
<signal name="SPI1_MISO99">
</signal>
<signal name="SPI1_MOSI99">
</signal>
<signal name="SPI1_SCK100">
</signal>
<signal name="SPI1_MISO100">
</signal>
<signal name="SPI1_MOSI100">
</signal>
<signal name="SPI1_SCK101">
</signal>
<signal name="SPI1_MISO101">
</signal>
<signal name="SPI1_MOSI101">
</signal>
<signal name="SPI1_SCK102">
</signal>
<signal name="SPI1_MISO102">
</signal>
<signal name="SPI1_MOSI102">
</signal>
<signal name="SPI1_SCK103">
</signal>
<signal name="SPI1_MISO103">
</signal>
<signal name="SPI1_MOSI103">
</signal>
<signal name="SPI1_SCK104">
</signal>
<signal name="SPI1_MISO104">
</signal>
<signal name="SPI1_MOSI104">
</signal>
<signal name="SPI1_SCK105">
</signal>
<signal name="SPI1_MISO105">
</signal>
<signal name="SPI1_MOSI105">
</signal>
<signal name="SPI1_SCK106">
</signal>
<signal name="SPI1_MISO106">
</signal>
<signal name="SPI1_MOSI106">
</signal>
<signal name="SPI1_SCK107">
</signal>
<signal name="SPI1_MISO107">
</signal>
<signal name="SPI1_MOSI107">
</signal>
<signal name="SPI1_SCK108">
</signal>
<signal name="SPI1_MISO108">
</signal>
<signal name="SPI1_MOSI108">
</signal>
<signal name="SPI1_SCK109">
</signal>
<signal name="SPI1_MISO109">
</signal>
<signal name="SPI1_MOSI109">
</signal>
<signal name="SPI1_SCK110">
</signal>
<signal name="SPI1_MISO110">
</signal>
<signal name="SPI1_MOSI110">
</signal>
<signal name="SPI1_SCK111">
</signal>
<signal name="SPI1_MISO111">
</signal>
<signal name="SPI1_MOSI111">
</signal>
<signal name="SPI1_SCK112">
</signal>
<signal name="SPI1_MISO112">
</signal>
<signal name="SPI1_MOSI112">
</signal>
<signal name="SPI1_SCK113">
</signal>
<signal name="SPI1_MISO113">
</signal>
<signal name="SPI1_MOSI113">
</signal>
<signal name="SPI1_SCK114">
</signal>
<signal name="SPI1_MISO114">
</signal>
<signal name="SPI1_MOSI114">
</signal>
<signal name="SPI1_SCK115">
</signal>
<signal name="SPI1_MISO115">
</signal>
<signal name="SPI1_MOSI115">
</signal>
<signal name="SPI1_SCK116">
</signal>
<signal name="SPI1_MISO116">
</signal>
<signal name="SPI1_MOSI116">
</signal>
<signal name="SPI1_SCK117">
</signal>
<signal name="SPI1_MISO117">
</signal>
<signal name="SPI1_MOSI117">
</signal>
<signal name="SPI1_SCK118">
</signal>
<signal name="SPI1_MISO118">
</signal>
<signal name="SPI1_MOSI118">
</signal>
<signal name="SPI1_SCK119">
</signal>
<signal name="SPI1_MISO119">
</signal>
<signal name="SPI1_MOSI119">
</signal>
<signal name="SPI1_SCK120">
</signal>
<signal name="SPI1_MISO120">
</signal>
<signal name="SPI1_MOSI120">
</signal>
<signal name="SPI1_SCK121">
</signal>
<signal name="SPI1_MISO121">
</signal>
<signal name="SPI1_MOSI121">
</signal>
<signal name="SPI1_SCK122">
</signal>
<signal name="SPI1_MISO122">
</signal>
<signal name="SPI1_MOSI122">
</signal>
<signal name="SPI1_SCK123">
</signal>
<signal name="SPI1_MISO123">
</signal>
<signal name="SPI1_MOSI123">
</signal>
<signal name="SPI1_SCK124">
</signal>
<signal name="SPI1_MISO124">
</signal>
<signal name="SPI1_MOSI124">
</signal>
<signal name="SPI1_SCK125">
</signal>
<signal name="SPI1_MISO125">
</signal>
<signal name="SPI1_MOSI125">
</signal>
<signal name="SPI1_SCK126">
</signal>
<signal name="SPI1_MISO126">
</signal>
<signal name="SPI1_MOSI126">
</signal>
<signal name="SPI1_SCK127">
</signal>
<signal name="SPI1_MISO127">
</signal>
<signal name="SPI1_MOSI127">
</signal>
<signal name="SPI1_SCK128">
</signal>
<signal name="SPI1_MISO128">
</signal>
<signal name="SPI1_MOSI128">
</signal>
<signal name="SPI1_SCK129">
</signal>
<signal name="SPI1_MISO129">
</signal>
<signal name="SPI1_MOSI129">
</signal>
<signal name="SPI1_SCK130">
</signal>
<signal name="SPI1_MISO130">
</signal>
<signal name="SPI1_MOSI130">
</signal>
<signal name="SPI1_SCK131">
</signal>
<signal name="SPI1_MISO131">
</signal>
<signal name="SPI1_MOSI131">
</signal>
<signal name="SPI1_SCK132">
</signal>
<signal name="SPI1_MISO132">
</signal>
<signal name="SPI1_MOSI132">
</signal>
<signal name="SPI1_SCK133">
</signal>
<signal name="SPI1_MISO133">
</signal>
<signal name="SPI1_MOSI133">
</signal>
<signal name="SPI1_SCK134">
</signal>
<signal name="SPI1_MISO134">
</signal>
<signal name="SPI1_MOSI134">
</signal>
<signal name="SPI1_SCK135">
</signal>
<signal name="SPI1_MISO135">
</signal>
<signal name="SPI1_MOSI135">
</signal>
<signal name="SPI1_SCK136">
</signal>
<signal name="SPI1_MISO136">
</signal>
<signal name="SPI1_MOSI136">
</signal>
<signal name="SPI1_SCK137">
</signal>
<signal name="SPI1_MISO137">
</signal>
<signal name="SPI1_MOSI137">
</signal>
<signal name="SPI1_SCK138">
</signal>
<signal name="SPI1_MISO138">
</signal>
<signal name="SPI1_MOSI138">
</signal>
<signal name="SPI1_SCK139">
</signal>
<signal name="SPI1_MISO139">
</signal>
<signal name="SPI1_MOSI139">
</signal>
<signal name="SPI1_SCK140">
</signal>
<signal name="SPI1_MISO140">
</signal>
<signal name="SPI1_MOSI140">
</signal>
<signal name="SPI1_SCK141">
</signal>
<signal name="SPI1_MISO141">
</signal>
<signal name="SPI1_MOSI141">
</signal>
<signal name="SPI1_SCK142">
</signal>
<signal name="SPI1_MISO142">
</signal>
<signal name="SPI1_MOSI142">
</signal>
<signal name="SPI1_SCK143">
</signal>
<signal name="SPI1_MISO143">
</signal>
<signal name="SPI1_MOSI143">
</signal>
<signal name="SPI1_SCK144">
</signal>
<signal name="SPI1_MISO144">
</signal>
<signal name="SPI1_MOSI144">
</signal>
<signal name="SPI1_SCK145">
</signal>
<signal name="SPI1_MISO145">
</signal>
<signal name="SPI1_MOSI145">
</signal>
<signal name="SPI1_SCK146">
</signal>
<signal name="SPI1_MISO146">
</signal>
<signal name="SPI1_MOSI146">
</signal>
<signal name="SPI1_SCK147">
</signal>
<signal name="SPI1_MISO147">
</signal>
<signal name="SPI1_MOSI147">
</signal>
<signal name="SPI1_SCK148">
</signal>
<signal name="SPI1_MISO148">
</signal>
<signal name="SPI1_MOSI148">
</signal>
<signal name="SPI1_SCK149">
</signal>
<signal name="SPI1_MISO149">
</signal>
<signal name="SPI1_MOSI149">
</signal>
<signal name="SPI1_SCK150">
</signal>
<signal name="SPI1_MISO150">
</signal>
<signal name="SPI1_MOSI150">
</signal>
<signal name="SPI1_SCK151">
</signal>
<signal name="SPI1_MISO151">
</signal>
<signal name="SPI1_MOSI151">
</signal>
<signal name="SPI1_SCK152">
</signal>
<signal name="SPI1_MISO152">
</signal>
<signal name="SPI1_MOSI152">
</signal>
<signal name="SPI1_SCK153">
</signal>
<signal name="SPI1_MISO153">
</signal>
<signal name="SPI1_MOSI153">
</signal>
<signal name="SPI1_SCK154">
</signal>
<signal name="SPI1_MISO154">
</signal>
<signal name="SPI1_MOSI154">
</signal>
<signal name="SPI1_SCK155">
</signal>
<signal name="SPI1_MISO155">
</signal>
<signal name="SPI1_MOSI155">
</signal>
<signal name="SPI1_SCK156">
</signal>
<signal name="SPI1_MISO156">
</signal>
<signal name="SPI1_MOSI156">
</signal>
<signal name="SPI1_SCK157">
</signal>
<signal name="SPI1_MISO157">
</signal>
<signal name="SPI1_MOSI157">
</signal>
<signal name="SPI1_SCK158">
</signal>
<signal name="SPI1_MISO158">
</signal>
<signal name="SPI1_MOSI158">
</signal>
<signal name="SPI1_SCK159">
</signal>
<signal name="SPI1_MISO159">
</signal>
<signal name="SPI1_MOSI159">
</signal>
<signal name="SPI1_SCK160">
</signal>
<signal name="SPI1_MISO160">
</signal>
<signal name="SPI1_MOSI160">
</signal>
<signal name="SPI1_SCK161">
</signal>
<signal name="SPI1_MISO161">
</signal>
<signal name="SPI1_MOSI161">
</signal>
<signal name="SPI1_SCK162">
</signal>
<signal name="SPI1_MISO162">
</signal>
<signal name="SPI1_MOSI162">
</signal>
<signal name="SPI1_SCK163">
</signal>
<signal name="SPI1_MISO163">
</signal>
<signal name="SPI1_MOSI163">
</signal>
<signal name="SPI1_SCK164">
</signal>
<signal name="SPI1_MISO164">
</signal>
<signal name="SPI1_MOSI164">
</signal>
<signal name="SPI1_SCK165">
</signal>
<signal name="SPI1_MISO165">
</signal>
<signal name="SPI1_MOSI165">
</signal>
<signal name="SPI1_SCK166">
</signal>
<signal name="SPI1_MISO166">
</signal>
<signal name="SPI1_MOSI166">
</signal>
<signal name="SPI1_SCK167">
</signal>
<signal name="SPI1_MISO167">
</signal>
<signal name="SPI1_MOSI167">
</signal>
<signal name="SPI1_SCK168">
</signal>
<signal name="SPI1_MISO168">
</signal>
<signal name="SPI1_MOSI168">
</signal>
<signal name="SPI1_SCK169">
</signal>
<signal name="SPI1_MISO169">
</signal>
<signal name="SPI1_MOSI169">
</signal>
<signal name="SPI1_SCK170">
</signal>
<signal name="SPI1_MISO170">
</signal>
<signal name="SPI1_MOSI170">
</signal>
<signal name="SPI1_SCK171">
</signal>
<signal name="SPI1_MISO171">
</signal>
<signal name="SPI1_MOSI171">
</signal>
<signal name="SPI1_SCK172">
</signal>
<signal name="SPI1_MISO172">
</signal>
<signal name="SPI1_MOSI172">
</signal>
<signal name="SPI1_SCK173">
</signal>
<signal name="SPI1_MISO173">
</signal>
<signal name="SPI1_MOSI173">
</signal>
<signal name="SPI1_SCK174">
</signal>
<signal name="SPI1_MISO174">
</signal>
<signal name="SPI1_MOSI174">
</signal>
<signal name="SPI1_SCK175">
</signal>
<signal name="SPI1_MISO175">
</signal>
<signal name="SPI1_MOSI175">
</signal>
<signal name="SPI1_SCK176">
</signal>
<signal name="SPI1_MISO176">
</signal>
<signal name="SPI1_MOSI176">
</signal>
<signal name="SPI1_SCK177">
</signal>
<signal name="SPI1_MISO177">
</signal>
<signal name="SPI1_MOSI177">
</signal>
<signal name="SPI1_SCK178">
</signal>
<signal name="SPI1_MISO178">
</signal>
<signal name="SPI1_MOSI178">
</signal>
<signal name="SPI1_SCK179">
</signal>
<signal name="SPI1_MISO179">
</signal>
<signal name="SPI1_MOSI179">
</signal>
<signal name="SPI1_SCK180">
</signal>
<signal name="SPI1_MISO180">
</signal>
<signal name="SPI1_MOSI180">
</signal>
<signal name="SPI1_SCK181">
</signal>
<signal name="SPI1_MISO181">
</signal>
<signal name="SPI1_MOSI181">
</signal>
<signal name="SPI1_SCK182">
</signal>
<signal name="SPI1_MISO182">
</signal>
<signal name="SPI1_MOSI182">
</signal>
<signal name="SPI1_SCK183">
</signal>
<signal name="SPI1_MISO183">
</signal>
<signal name="SPI1_MOSI183">
</signal>
<signal name="SPI1_SCK184">
</signal>
<signal name="SPI1_MISO184">
</signal>
<signal name="SPI1_MOSI184">
</signal>
<signal name="SPI1_SCK185">
</signal>
<signal name="SPI1_MISO185">
</signal>
<signal name="SPI1_MOSI185">
</signal>
<signal name="SPI1_SCK186">
</signal>
<signal name="SPI1_MISO186">
</signal>
<signal name="SPI1_MOSI186">
</signal>
<signal name="SPI1_SCK187">
</signal>
<signal name="SPI1_MISO187">
</signal>
<signal name="SPI1_MOSI187">
</signal>
<signal name="SPI1_SCK188">
</signal>
<signal name="SPI1_MISO188">
</signal>
<signal name="SPI1_MOSI188">
</signal>
<signal name="SPI1_SCK189">
</signal>
<signal name="SPI1_MISO189">
</signal>
<signal name="SPI1_MOSI189">
</signal>
<signal name="SPI1_SCK190">
</signal>
<signal name="SPI1_MISO190">
</signal>
<signal name="SPI1_MOSI190">
</signal>
<signal name="SPI1_SCK191">
</signal>
<signal name="SPI1_MISO191">
</signal>
<signal name="SPI1_MOSI191">
</signal>
<signal name="SPI1_SCK192">
</signal>
<signal name="SPI1_MISO192">
</signal>
<signal name="SPI1_MOSI192">
</signal>
<signal name="SPI1_SCK193">
</signal>
<signal name="SPI1_MISO193">
</signal>
<signal name="SPI1_MOSI193">
</signal>
<signal name="SPI1_SCK194">
</signal>
<signal name="SPI1_MISO194">
</signal>
<signal name="SPI1_MOSI194">
</signal>
<signal name="SPI1_SCK195">
</signal>
<signal name="SPI1_MISO195">
</signal>
<signal name="SPI1_MOSI195">
</signal>
<signal name="SPI1_SCK196">
</signal>
<signal name="SPI1_MISO196">
</signal>
<signal name="SPI1_MOSI196">
</signal>
<signal name="SPI1_SCK197">
</signal>
<signal name="SPI1_MISO197">
</signal>
<signal name="SPI1_MOSI197">
</signal>
<signal name="SPI1_SCK198">
</signal>
<signal name="SPI1_MISO198">
</signal>
<signal name="SPI1_MOSI198">
</signal>
<signal name="SPI1_SCK199">
</signal>
<signal name="SPI1_MISO199">
</signal>
<signal name="SPI1_MOSI199">
</signal>
<signal name="SPI1_SCK200">
</signal>
<signal name="SPI1_MISO200">
</signal>
<signal name="SPI1_MOSI200">
</signal>
<signal name="SPI1_SCK201">
</signal>
<signal name="SPI1_MISO201">
</signal>
<signal name="SPI1_MOSI201">
</signal>
<signal name="SPI1_SCK202">
</signal>
<signal name="SPI1_MISO202">
</signal>
<signal name="SPI1_MOSI202">
</signal>
<signal name="SPI1_SCK203">
</signal>
<signal name="SPI1_MISO203">
</signal>
<signal name="SPI1_MOSI203">
</signal>
<signal name="SPI1_SCK204">
</signal>
<signal name="SPI1_MISO204">
</signal>
<signal name="SPI1_MOSI204">
</signal>
<signal name="SPI1_SCK205">
</signal>
<signal name="SPI1_MISO205">
</signal>
<signal name="SPI1_MOSI205">
</signal>
<signal name="SPI1_SCK206">
</signal>
<signal name="SPI1_MISO206">
</signal>
<signal name="SPI1_MOSI206">
</signal>
<signal name="SPI1_SCK207">
</signal>
<signal name="SPI1_MISO207">
</signal>
<signal name="SPI1_MOSI207">
</signal>
<signal name="SPI1_SCK208">
</signal>
<signal name="SPI1_MISO208">
</signal>
<signal name="SPI1_MOSI208">
</signal>
<signal name="SPI1_SCK209">
</signal>
<signal name="SPI1_MISO209">
</signal>
<signal name="SPI1_MOSI209">
</signal>
<signal name="SPI1_SCK210">
</signal>
<signal name="SPI1_MISO210">
</signal>
<signal name="SPI1_MOSI210">
</signal>
<signal name="SPI1_SCK211">
</signal>
<signal name="SPI1_MISO211">
</signal>
<signal name="SPI1_MOSI211">
</signal>
<signal name="SPI1_SCK212">
</signal>
<signal name="SPI1_MISO212">
</signal>
<signal name="SPI1_MOSI212">
</signal>
<signal name="SPI1_SCK213">
</signal>
<signal name="SPI1_MISO213">
</signal>
<signal name="SPI1_MOSI213">
</signal>
<signal name="SPI1_SCK214">
</signal>
<signal name="SPI1_MISO214">
</signal>
<signal name="SPI1_MOSI214">
</signal>
<signal name="SPI1_SCK215">
</signal>
<signal name="SPI1_MISO215">
</signal>
<signal name="SPI1_MOSI215">
</signal>
<signal name="SPI1_SCK216">
</signal>
<signal name="SPI1_MISO216">
</signal>
<signal name="SPI1_MOSI216">
</signal>
<signal name="SPI1_SCK217">
</signal>
<signal name="SPI1_MISO217">
</signal>
<signal name="SPI1_MOSI217">
</signal>
<signal name="SPI1_SCK218">
</signal>
<signal name="SPI1_MISO218">
</signal>
<signal name="SPI1_MOSI218">
</signal>
<signal name="SPI1_SCK219">
</signal>
<signal name="SPI1_MISO219">
</signal>
<signal name="SPI1_MOSI219">
</signal>
<signal name="SPI1_SCK220">
</signal>
<signal name="SPI1_MISO220">
</signal>
<signal name="SPI1_MOSI220">
</signal>
<signal name="SPI1_SCK221">
</signal>
<signal name="SPI1_MISO221">
</signal>
<signal name="SPI1_MOSI221">
</signal>
<signal name="SPI1_SCK222">
</signal>
<signal name="SPI1_MISO222">
</signal>
<signal name="SPI1_MOSI222">
</signal>
<signal name="SPI1_SCK223">
</signal>
<signal name="SPI1_MISO223">
</signal>
<signal name="SPI1_MOSI223">
</signal>
<signal name="SPI1_SCK224">
</signal>
<signal name="SPI1_MISO224">
</signal>
<signal name="SPI1_MOSI224">
</signal>
<signal name="SPI1_SCK225">
</signal>
<signal name="SPI1_MISO225">
</signal>
<signal name="SPI1_MOSI225">
</signal>
<signal name="SPI1_SCK226">
</signal>
<signal name="SPI1_MISO226">
</signal>
<signal name="SPI1_MOSI226">
</signal>
<signal name="SPI1_SCK227">
</signal>
<signal name="SPI1_MISO227">
</signal>
<signal name="SPI1_MOSI227">
</signal>
<signal name="SPI1_SCK228">
</signal>
<signal name="SPI1_MISO228">
</signal>
<signal name="SPI1_MOSI228">
</signal>
<signal name="SPI1_SCK229">
</signal>
<signal name="SPI1_MISO229">
</signal>
<signal name="SPI1_MOSI229">
</signal>
<signal name="SPI1_SCK230">
</signal>
<signal name="SPI1_MISO230">
</signal>
<signal name="SPI1_MOSI230">
</signal>
<signal name="SPI1_SCK231">
</signal>
<signal name="SPI1_MISO231">
</signal>
<signal name="SPI1_MOSI231">
</signal>
<signal name="SPI1_SCK232">
</signal>
<signal name="SPI1_MISO232">
</signal>
<signal name="SPI1_MOSI232">
</signal>
<signal name="SPI1_SCK233">
</signal>
<signal name="SPI1_MISO233">
</signal>
<signal name="SPI1_MOSI233">
</signal>
<signal name="SPI1_SCK234">
</signal>
<signal name="SPI1_MISO234">
</signal>
<signal name="SPI1_MOSI234">
</signal>
<signal name="SPI1_SCK235">
</signal>
<signal name="SPI1_MISO235">
</signal>
<signal name="SPI1_MOSI235">
</signal>
<signal name="SPI1_SCK236">
</signal>
<signal name="SPI1_MISO236">
</signal>
<signal name="SPI1_MOSI236">
</signal>
<signal name="SPI1_SCK237">
</signal>
<signal name="SPI1_MISO237">
</signal>
<signal name="SPI1_MOSI237">
</signal>
<signal name="SPI1_SCK238">
</signal>
<signal name="SPI1_MISO238">
</signal>
<signal name="SPI1_MOSI238">
</signal>
<signal name="SPI1_SCK239">
</signal>
<signal name="SPI1_MISO239">
</signal>
<signal name="SPI1_MOSI239">
</signal>
<signal name="SPI1_SCK240">
</signal>
<signal name="SPI1_MISO240">
</signal>
<signal name="SPI1_MOSI240">
</signal>
<signal name="SPI1_SCK241">
</signal>
<signal name="SPI1_MISO241">
</signal>
<signal name="SPI1_MOSI241">
</signal>
<signal name="SPI1_SCK242">
</signal>
<signal name="SPI1_MISO242">
</signal>
<signal name="SPI1_MOSI242">
</signal>
<signal name="SPI1_SCK243">
</signal>
<signal name="SPI1_MISO243">
</signal>
<signal name="SPI1_MOSI243">
</signal>
<signal name="SPI1_SCK244">
</signal>
<signal name="SPI1_MISO244">
</signal>
<signal name="SPI1_MOSI244">
</signal>
<signal name="SPI1_SCK245">
</signal>
<signal name="SPI1_MISO245">
</signal>
<signal name="SPI1_MOSI245">
</signal>
<signal name="SPI1_SCK246">
</signal>
<signal name="SPI1_MISO246">
</signal>
<signal name="SPI1_MOSI246">
</signal>
<signal name="SPI1_SCK247">
</signal>
<signal name="SPI1_MISO247">
</signal>
<signal name="SPI1_MOSI247">
</signal>
<signal name="SPI1_SCK248">
</signal>
<signal name="SPI1_MISO248">
</signal>
<signal name="SPI1_MOSI248">
</signal>
<signal name="SPI1_SCK249">
</signal>
<signal name="SPI1_MISO249">
</signal>
<signal name="SPI1_MOSI249">
</signal>
<signal name="SPI1_SCK250">
</signal>
<signal name="SPI1_MISO250">
</signal>
<signal name="SPI1_MOSI250">
</signal>
<signal name="SPI1_SCK251">
</signal>
<signal name="SPI1_MISO251">
</signal>
<signal name="SPI1_MOSI251">
</signal>
<signal name="SPI1_SCK252">
</signal>
<signal name="SPI1_MISO252">
</signal>
<signal name="SPI1_MOSI252">
</signal>
<signal name="SPI1_SCK253">
</signal>
<signal name="SPI1_MISO253">
</signal>
<signal name="SPI1_MOSI253">
</signal>
<signal name="SPI1_SCK254">
</signal>
<signal name="SPI1_MISO254">
</signal>
<signal name="SPI1_MOSI254">
</signal>
<signal name="SPI1_SCK255">
</signal>
<signal name="SPI1_MISO255">
</signal>
<signal name="SPI1_MOSI255">
</signal>
<signal name="SPI1_SCK256">
</signal>
<signal name="SPI1_MISO256">
</signal>
<signal name="SPI1_MOSI256">
</signal>
<signal name="SPI1_SCK257">
</signal>
<signal name="SPI1_MISO257">
</signal>
<signal name="SPI1_MOSI257">
</signal>
<signal name="SPI1_SCK258">
</signal>
<signal name="SPI1_MISO258">
</signal>
<signal name="SPI1_MOSI258">
</signal>
<signal name="SPI1_SCK259">
</signal>
<signal name="SPI1_MISO259">
</signal>
<signal name="SPI1_MOSI259">
</signal>
<signal name="SPI1_SCK260">
</signal>
<signal name="SPI1_MISO260">
</signal>
<signal name="SPI1_MOSI260">
</signal>
<signal name="SPI1_SCK261">
</signal>
<signal name="SPI1_MISO261">
</signal>
<signal name="SPI1_MOSI261">
</signal>
<signal name="SPI1_SCK262">
</signal>
<signal name="SPI1_MISO262">
</signal>
<signal name="SPI1_MOSI262">
</signal>
<signal name="SPI1_SCK263">
</signal>
<signal name="SPI1_MISO263">
</signal>
<signal name="SPI1_MOSI263">
</signal>
<signal name="SPI1_SCK264">
</signal>
<signal name="SPI1_MISO264">
</signal>
<signal name="SPI1_MOSI264">
</signal>
<signal name="SPI1_SCK265">
</signal>
<signal name="SPI1_MISO265">
</signal>
<signal name="SPI1_MOSI265">
</signal>
<signal name="SPI1_SCK266">
</signal>
<signal name="SPI1_MISO266">
</signal>
<signal name="SPI1_MOSI266">
</signal>
<signal name="SPI1_SCK267">
</signal>
<signal name="SPI1_MISO267">
</signal>
<signal name="SPI1_MOSI267">
</signal>
<signal name="SPI1_SCK268">
</signal>
<signal name="SPI1_MISO268">
</signal>
<signal name="SPI1_MOSI268">
</signal>
<signal name="SPI1_SCK269">
</signal>
<signal name="SPI1_MISO269">
</signal>
<signal name="SPI1_MOSI269">
</signal>
<signal name="SPI1_SCK270">
</signal>
<signal name="SPI1_MISO270">
</signal>
<signal name="SPI1_MOSI270">
</signal>
<signal name="SPI1_SCK271">
</signal>
<signal name="SPI1_MISO271">
</signal>
<signal name="SPI1_MOSI271">
</signal>
<signal name="SPI1_SCK272">
</signal>
<signal name="SPI1_MISO272">
</signal>
<signal name="SPI1_MOSI272">
</signal>
<signal name="SPI1_SCK273">
</signal>
<signal name="SPI1_MISO273">
</signal>
<signal name="SPI1_MOSI273">
</signal>
<signal name="SPI1_SCK274">
</signal>
<signal name="SPI1_MISO274">
</signal>
<signal name="SPI1_MOSI274">
</signal>
<signal name="SPI1_SCK275">
</signal>
<signal name="SPI1_MISO275">
</signal>
<signal name="SPI1_MOSI275">
</signal>
<signal name="SPI1_SCK276">
</signal>
<signal name="SPI1_MISO276">
</signal>
<signal name="SPI1_MOSI276">
</signal>
<signal name="SPI1_SCK277">
</signal>
<signal name="SPI1_MISO277">
</signal>
<signal name="SPI1_MOSI277">
</signal>
<signal name="SPI1_SCK278">
</signal>
<signal name="SPI1_MISO278">
</signal>
<signal name="SPI1_MOSI278">
</signal>
<signal name="SPI1_SCK279">
</signal>
<signal name="SPI1_MISO279">
</signal>
<signal name="SPI1_MOSI279">
</signal>
<signal name="SPI1_SCK280">
</signal>
<signal name="SPI1_MISO280">
</signal>
<signal name="SPI1_MOSI280">
</signal>
<signal name="SPI1_SCK281">
</signal>
<signal name="SPI1_MISO281">
</signal>
<signal name="SPI1_MOSI281">
</signal>
<signal name="SPI1_SCK282">
</signal>
<signal name="SPI1_MISO282">
</signal>
<signal name="SPI1_MOSI282">
</signal>
<signal name="SPI1_SCK283">
</signal>
<signal name="SPI1_MISO283">
</signal>
<signal name="SPI1_MOSI283">
</signal>
<signal name="SPI1_SCK284">
</signal>
<signal name="SPI1_MISO284">
</signal>
<signal name="SPI1_MOSI284">
</signal>
<signal name="SPI1_SCK285">
</signal>
<signal name="SPI1_MISO285">
</signal>
<signal name="SPI1_MOSI285">
</signal>
<signal name="SPI1_SCK286">
</signal>
<signal name="SPI1_MISO286">
</signal>
<signal name="SPI1_MOSI286">
</signal>
<signal name="SPI1_SCK287">
</signal>
<signal name="SPI1_MISO287">
</signal>
<signal name="SPI1_MOSI287">
</signal>
<signal name="SPI1_SCK288">
</signal>
<signal name="SPI1_MISO288">
</signal>
<signal name="SPI1_MOSI288">
</signal>
<signal name="SPI1_SCK289">
</signal>
<signal name="SPI1_MISO289">
</signal>
<signal name="SPI1_MOSI289">
</signal>
<signal name="SPI1_SCK290">
</signal>
<signal name="SPI1_MISO290">
</signal>
<signal name="SPI1_MOSI290">
</signal>
<signal name="SPI1_SCK291">
</signal>
<signal name="SPI1_MISO291">
</signal>
<signal name="SPI1_MOSI291">
</signal>
<signal name="SPI1_SCK292">
</signal>
<signal name="SPI1_MISO292">
</signal>
<signal name="SPI1_MOSI292">
</signal>
<signal name="SPI1_SCK293">
</signal>
<signal name="SPI1_MISO293">
</signal>
<signal name="SPI1_MOSI293">
</signal>
<signal name="SPI1_SCK294">
</signal>
<signal name="SPI1_MISO294">
</signal>
<signal name="SPI1_MOSI294">
</signal>
<signal name="SPI1_SCK295">
</signal>
<signal name="SPI1_MISO295">
</signal>
<signal name="SPI1_MOSI295">
</signal>
<signal name="SPI1_SCK296">
</signal>
<signal name="SPI1_MISO296">
</signal>
<signal name="SPI1_MOSI296">
</signal>
<signal name="SPI1_SCK297">
</signal>
<signal name="SPI1_MISO297">
</signal>
<signal name="SPI1_MOSI297">
</signal>
<signal name="SPI1_SCK298">
</signal>
<signal name="SPI1_MISO298">
</signal>
<signal name="SPI1_MOSI298">
</signal>
<signal name="SPI1_SCK299">
</signal>
<signal name="SPI1_MISO299">
</signal>
<signal name="SPI1_MOSI299">
</signal>
<signal name="SPI1_SCK300">
</signal>
<signal name="SPI1_MISO300">
</signal>
<signal name="SPI1_MOSI300">
</signal>
<signal name="SPI1_SCK301">
</signal>
<signal name="SPI1_MISO301">
</signal>
<signal name="SPI1_MOSI301">
</signal>
<signal name="SPI1_SCK302">
</signal>
<signal name="SPI1_MISO302">
</signal>
<signal name="SPI1_MOSI302">
</signal>
<signal name="SPI1_SCK303">
</signal>
<signal name="SPI1_MISO303">
</signal>
<signal name="SPI1_MOSI303">
</signal>
<signal name="SPI1_SCK304">
</signal>
<signal name="SPI1_MISO304">
</signal>
<signal name="SPI1_MOSI304">
</signal>
<signal name="SPI1_SCK305">
</signal>
<signal name="SPI1_MISO305">
</signal>
<signal name="SPI1_MOSI305">
</signal>
<signal name="SPI1_SCK306">
</signal>
<signal name="SPI1_MISO306">
</signal>
<signal name="SPI1_MOSI306">
</signal>
<signal name="SPI1_SCK307">
</signal>
<signal name="SPI1_MISO307">
</signal>
<signal name="SPI1_MOSI307">
</signal>
<signal name="SPI1_SCK308">
</signal>
<signal name="SPI1_MISO308">
</signal>
<signal name="SPI1_MOSI308">
</signal>
<signal name="SPI1_SCK309">
</signal>
<signal name="SPI1_MISO309">
</signal>
<signal name="SPI1_MOSI309">
</signal>
<signal name="SPI1_SCK310">
</signal>
<signal name="SPI1_MISO310">
</signal>
<signal name="SPI1_MOSI310">
</signal>
<signal name="SPI1_SCK311">
</signal>
<signal name="SPI1_MISO311">
</signal>
<signal name="SPI1_MOSI311">
</signal>
<signal name="SPI1_SCK312">
</signal>
<signal name="SPI1_MISO312">
</signal>
<signal name="SPI1_MOSI312">
</signal>
<signal name="SPI1_SCK313">
</signal>
<signal name="SPI1_MISO313">
</signal>
<signal name="SPI1_MOSI313">
</signal>
<signal name="SPI1_SCK314">
</signal>
<signal name="SPI1_MISO314">
</signal>
<signal name="SPI1_MOSI314">
</signal>
<signal name="SPI1_SCK315">
</signal>
<signal name="SPI1_MISO315">
</signal>
<signal name="SPI1_MOSI315">
</signal>
<signal name="SPI1_SCK316">
</signal>
<signal name="SPI1_MISO316">
</signal>
<signal name="SPI1_MOSI316">
</signal>
<signal name="SPI1_SCK317">
</signal>
<signal name="SPI1_MISO317">
</signal>
<signal name="SPI1_MOSI317">
</signal>
<signal name="SPI1_SCK318">
</signal>
<signal name="SPI1_MISO318">
</signal>
<signal name="SPI1_MOSI318">
</signal>
<signal name="SPI1_SCK319">
</signal>
<signal name="SPI1_MISO319">
</signal>
<signal name="SPI1_MOSI319">
</signal>
<signal name="SPI1_SCK320">
</signal>
<signal name="SPI1_MISO320">
</signal>
<signal name="SPI1_MOSI320">
</signal>
<signal name="SPI1_SCK321">
</signal>
<signal name="SPI1_MISO321">
</signal>
<signal name="SPI1_MOSI321">
</signal>
<signal name="SPI1_SCK322">
</signal>
<signal name="SPI1_MISO322">
</signal>
<signal name="SPI1_MOSI322">
</signal>
<signal name="SPI1_SCK323">
</signal>
<signal name="SPI1_MISO323">
</signal>
<signal name="SPI1_MOSI323">
</signal>
<signal name="SPI1_SCK324">
</signal>
<signal name="SPI1_MISO324">
</signal>
<signal name="SPI1_MOSI324">
</signal>
<signal name="SPI1_SCK325">
</signal>
<signal name="SPI1_MISO325">
</signal>
<signal name="SPI1_MOSI325">
</signal>
<signal name="SPI1_SCK326">
</signal>
<signal name="SPI1_MISO326">
</signal>
<signal name="SPI1_MOSI326">
</signal>
<signal name="SPI1_SCK327">
</signal>
<signal name="SPI1_MISO327">
</signal>
<signal name="SPI1_MOSI327">
</signal>
<signal name="SPI1_SCK328">
</signal>
<signal name="SPI1_MISO328">
</signal>
<signal name="SPI1_MOSI328">
</signal>
<signal name="SPI1_SCK329">
</signal>
<signal name="SPI1_MISO329">
</signal>
<signal name="SPI1_MOSI329">
</signal>
<signal name="SPI1_SCK330">
</signal>
<signal name="SPI1_MISO330">
</signal>
<signal name="SPI1_MOSI330">
</signal>
<signal name="SPI1_SCK331">
</signal>
<signal name="SPI1_MISO331">
</signal>
<signal name="SPI1_MOSI331">
</signal>
<signal name="SPI1_SCK332">
</signal>
<signal name="SPI1_MISO332">
</signal>
<signal name="SPI1_MOSI332">
</signal>
<signal name="SPI1_SCK333">
</signal>
<signal name="SPI1_MISO333">
</signal>
<signal name="SPI1_MOSI333">
</signal>
<signal name="SPI1_SCK334">
</signal>
<signal name="SPI1_MISO334">
</signal>
<signal name="SPI1_MOSI334">
</signal>
<signal name="SPI1_SCK335">
</signal>
<signal name="SPI1_MISO335">
</signal>
<signal name="SPI1_MOSI335">
</signal>
<signal name="SPI1_SCK336">
</signal>
<signal name="SPI1_MISO336">
</signal>
<signal name="SPI1_MOSI336">
</signal>
<signal name="SPI1_SCK337">
</signal>
<signal name="SPI1_MISO337">
</signal>
<signal name="SPI1_MOSI337">
</signal>
<signal name="SPI1_SCK338">
</signal>
<signal name="SPI1_MISO338">
</signal>
<signal name="SPI1_MOSI338">
</signal>
<signal name="SPI1_SCK339">
</signal>
<signal name="SPI1_MISO339">
</signal>
<signal name="SPI1_MOSI339">
</signal>
<signal name="SPI1_SCK340">
</signal>
<signal name="SPI1_MISO340">
</signal>
<signal name="SPI1_MOSI340">
</signal>
<signal name="SPI1_SCK341">
</signal>
<signal name="SPI1_MISO341">
</signal>
<signal name="SPI1_MOSI341">
</signal>
<signal name="SPI1_SCK342">
</signal>
<signal name="SPI1_MISO342">
</signal>
<signal name="SPI1_MOSI342">
</signal>
<signal name="SPI1_SCK343">
</signal>
<signal name="SPI1_MISO343">
</signal>
<signal name="SPI1_MOSI343">
</signal>
<signal name="SPI1_SCK344">
</signal>
<signal name="SPI1_MISO344">
</signal>
<signal name="SPI1_MOSI344">
</signal>
<signal name="SPI1_SCK345">
</signal>
<signal name="SPI1_MISO345">
</signal>
<signal name="SPI1_MOSI345">
</signal>
<signal name="SPI1_SCK346">
</signal>
<signal name="SPI1_MISO346">
</signal>
<signal name="SPI1_MOSI346">
</signal>
<signal name="SPI1_SCK347">
</signal>
<signal name="SPI1_MISO347">
</signal>
<signal name="SPI1_MOSI347">
</signal>
<signal name="SPI1_SCK348">
</signal>
<signal name="SPI1_MISO348">
</signal>
<signal name="SPI1_MOSI348">
</signal>
<signal name="SPI1_SCK349">
</signal>
<signal name="SPI1_MISO349">
</signal>
<signal name="SPI1_MOSI349">
</signal>
<signal name="SPI1_SCK350">
</signal>
<signal name="SPI1_MISO350">
</signal>
<signal name="SPI1_MOSI350">
</signal>
<signal name="SPI1_SCK351">
</signal>
<signal name="SPI1_MISO351">
</signal>
<signal name="SPI1_MOSI351">
</signal>
<signal name="SPI1_SCK352">
</signal>
<signal name="SPI1_MISO352">
</signal>
<signal name="SPI1_MOSI352">
</signal>
<signal name="SPI1_SCK353">
</signal>
<signal name="SPI1_MISO353">
</signal>
<signal name="SPI1_MOSI353">
</signal>
<signal name="SPI1_SCK354">
</signal>
<signal name="SPI1_MISO354">
</signal>
<signal name="SPI1_MOSI354">
</signal>
<signal name="SPI1_SCK355">
</signal>
<signal name="SPI1_MISO355">
</signal>
<signal name="SPI1_MOSI355">
</signal>
<signal name="SPI1_SCK356">
</signal>
<signal name="SPI1_MISO356">
</signal>
<signal name="SPI1_MOSI356">
</signal>
<signal name="SPI1_SCK357">
</signal>
<signal name="SPI1_MISO357">
</signal>
<signal name="SPI1_MOSI357">
</signal>
<signal name="SPI1_SCK358">
</signal>
<signal name="SPI1_MISO358">
</signal>
<signal name="SPI1_MOSI358">
</signal>
<signal name="SPI1_SCK359">
</signal>
<signal name="SPI1_MISO359">
</signal>
<signal name="SPI1_MOSI359">
</signal>
<signal name="SPI1_SCK360">
</signal>
<signal name="SPI1_MISO360">
</signal>
<signal name="SPI1_MOSI360">
</signal>
<signal name="SPI1_SCK361">
</signal>
<signal name="SPI1_MISO361">
</signal>
<signal name="SPI1_MOSI361">
</signal>
<signal name="SPI1_SCK362">
</signal>
<signal name="SPI1_MISO362">
</signal>
<signal name="SPI1_MOSI362">
</signal>
<signal name="SPI1_SCK363">
</signal>
<signal name="SPI1_MISO363">
</signal>
<signal name="SPI1_MOSI363">
</signal>
<signal name="SPI1_SCK364">
</signal>
<signal name="SPI1_MISO364">
</signal>
<signal name="SPI1_MOSI364">
</signal>
<signal name="SPI1_SCK365">
</signal>
<signal name="SPI1_MISO365">
</signal>
<signal name="SPI1_MOSI365">
</signal>
<signal name="SPI1_SCK366">
</signal>
<signal name="SPI1_MISO366">
</signal>
<signal name="SPI1_MOSI366">
</signal>
<signal name="SPI1_SCK367">
</signal>
<signal name="SPI1_MISO367">
</signal>
<signal name="SPI1_MOSI367">
</signal>
<signal name="SPI1_SCK368">
</signal>
<signal name="SPI1_MISO368">
</signal>
<signal name="SPI1_MOSI368">
</signal>
<signal name="SPI1_SCK369">
</signal>
<signal name="SPI1_MISO369">
</signal>
<signal name="SPI1_MOSI369">
</signal>
<signal name="SPI1_SCK370">
</signal>
<signal name="SPI1_MISO370">
</signal>
<signal name="SPI1_MOSI370">
</signal>
<signal name="SPI1_SCK371">
</signal>
<signal name="SPI1_MISO371">
</signal>
<signal name="SPI1_MOSI371">
</signal>
<signal name="SPI1_SCK372">
</signal>
<signal name="SPI1_MISO372">
</signal>
<signal name="SPI1_MOSI372">
</signal>
<signal name="SPI1_SCK373">
</signal>
<signal name="SPI1_MISO373">
</signal>
<signal name="SPI1_MOSI373">
</signal>
<signal name="SPI1_SCK374">
</signal>
<signal name="SPI1_MISO374">
</signal>
<signal name="SPI1_MOSI374">
</signal>
<signal name="SPI1_SCK375">
</signal>
<signal name="SPI1_MISO375">
</signal>
<signal name="SPI1_MOSI375">
</signal>
<signal name="SPI1_SCK376">
</signal>
<signal name="SPI1_MISO376">
</signal>
<signal name="SPI1_MOSI376">
</signal>
<signal name="SPI1_SCK377">
</signal>
<signal name="SPI1_MISO377">
</signal>
<signal name="SPI1_MOSI377">
</signal>
<signal name="SPI1_SCK378">
</signal>
<signal name="SPI1_MISO378">
</signal>
<signal name="SPI1_MOSI378">
</signal>
<signal name="SPI1_SCK379">
</signal>
<signal name="SPI1_MISO379">
</signal>
<signal name="SPI1_MOSI379">
</signal>
<signal name="SPI1_SCK380">
</signal>
<signal name="SPI1_MISO380">
</signal>
<signal name="SPI1_MOSI380">
</signal>
<signal name="SPI1_SCK381">
</signal>
<signal name="SPI1_MISO381">
</signal>
<signal name="SPI1_MOSI381">
</signal>
<signal name="SPI1_SCK382">
</signal>
<signal name="SPI1_MISO382">
</signal>
<signal name="SPI1_MOSI382">
</signal>
<signal name="SPI1_SCK383">
</signal>
<signal name="SPI1_MISO383">
</signal>
<signal name="SPI1_MOSI383">
</signal>
<signal name="SPI1_SCK384">
</signal>
<signal name="SPI1_MISO384">
</signal>
<signal name="SPI1_MOSI384">
</signal>
<signal name="SPI1_SCK385">
</signal>
<signal name="SPI1_MISO385">
</signal>
<signal name="SPI1_MOSI385">
</signal>
<signal name="SPI1_SCK386">
</signal>
<signal name="SPI1_MISO386">
</signal>
<signal name="SPI1_MOSI386">
</signal>
<signal name="SPI1_SCK387">
</signal>
<signal name="SPI1_MISO387">
</signal>
<signal name="SPI1_MOSI387">
</signal>
<signal name="SPI1_SCK388">
</signal>
<signal name="SPI1_MISO388">
</signal>
<signal name="SPI1_MOSI388">
</signal>
<signal name="SPI1_SCK389">
</signal>
<signal name="SPI1_MISO389">
</signal>
<signal name="SPI1_MOSI389">
</signal>
<signal name="SPI1_SCK390">
</signal>
<signal name="SPI1_MISO390">
</signal>
<signal name="SPI1_MOSI390">
</signal>
<signal name="SPI1_SCK391">
</signal>
<signal name="SPI1_MISO391">
</signal>
<signal name="SPI1_MOSI391">
</signal>
<signal name="SPI1_SCK392">
</signal>
<signal name="SPI1_MISO392">
</signal>
<signal name="SPI1_MOSI392">
</signal>
<signal name="SPI1_SCK393">
</signal>
<signal name="SPI1_MISO393">
</signal>
<signal name="SPI1_MOSI393">
</signal>
<signal name="SPI1_SCK394">
</signal>
<signal name="SPI1_MISO394">
</signal>
<signal name="SPI1_MOSI394">
</signal>
<signal name="SPI1_SCK395">
</signal>
<signal name="SPI1_MISO395">
</signal>
<signal name="SPI1_MOSI395">
</signal>
<signal name="SPI1_SCK396">
</signal>
<signal name="SPI1_MISO396">
</signal>
<signal name="SPI1_MOSI396">
</signal>
<signal name="SPI1_SCK397">
</signal>
<signal name="SPI1_MISO397">
</signal>
<signal name="SPI1_MOSI397">
</signal>
<signal name="SPI1_SCK398">
</signal>
<signal name="SPI1_MISO398">
</signal>
<signal name="SPI1_MOSI398">
</signal>
<signal name="SPI1_SCK399">
</signal>
<signal name="SPI1_MISO399">
</signal>
<signal name="SPI1_MOSI399">
</signal>
<signal name="SPI1_SCK400">
</signal>
<signal name="SPI1_MISO400">
</signal>
<signal name="SPI1_MOSI400">
</signal>
<signal name="SPI1_SCK401">
</signal>
<signal name="SPI1_MISO401">
</signal>
<signal name="SPI1_MOSI401">
</signal>
<signal name="SPI1_SCK402">
</signal>
<signal name="SPI1_MISO402">
</signal>
<signal name="SPI1_MOSI402">
</signal>
<signal name="SPI1_SCK403">
</signal>
<signal name="SPI1_MISO403">
</signal>
<signal name="SPI1_MOSI403">
</signal>
<signal name="SPI1_SCK404">
</signal>
<signal name="SPI1_MISO404">
</signal>
<signal name="SPI1_MOSI404">
</signal>
<signal name="SPI1_SCK405">
</signal>
<signal name="SPI1_MISO405">
</signal>
<signal name="SPI1_MOSI405">
</signal>
<signal name="SPI1_SCK406">
</signal>
<signal name="SPI1_MISO406">
</signal>
<signal name="SPI1_MOSI406">
</signal>
<signal name="SPI1_SCK407">
</signal>
<signal name="SPI1_MISO407">
</signal>
<signal name="SPI1_MOSI407">
</signal>
<signal name="SPI1_SCK408">
</signal>
<signal name="SPI1_MISO408">
</signal>
<signal name="SPI1_MOSI408">
</signal>
<signal name="SPI1_SCK409">
</signal>
<signal name="SPI1_MISO409">
</signal>
<signal name="SPI1_MOSI409">
</signal>
<signal name="SPI1_SCK410">
</signal>
<signal name="SPI1_MISO410">
</signal>
<signal name="SPI1_MOSI410">
</signal>
<signal name="SPI1_SCK411">
</signal>
<signal name="SPI1_MISO411">
</signal>
<signal name="SPI1_MOSI411">
</signal>
<signal name="SPI1_SCK412">
</signal>
<signal name="SPI1_MISO412">
</signal>
<signal name="SPI1_MOSI412">
</signal>
<signal name="SPI1_SCK413">
</signal>
<signal name="SPI1_MISO413">
</signal>
<signal name="SPI1_MOSI413">
</signal>
<signal name="SPI1_SCK414">
</signal>
<signal name="SPI1_MISO414">
</signal>
<signal name="SPI1_MOSI414">
</signal>
<signal name="SPI1_SCK415">
</signal>
<signal name="SPI1_MISO415">
</signal>
<signal name="SPI1_MOSI415">
</signal>
<signal name="SPI1_SCK416">
</signal>
<signal name="SPI1_MISO416">
</signal>
<signal name="SPI1_MOSI416">
</signal>
<signal name="SPI1_SCK417">
</signal>
<signal name="SPI1_MISO417">
</signal>
<signal name="SPI1_MOSI417">
</signal>
<signal name="SPI1_SCK418">
</signal>
<signal name="SPI1_MISO418">
</signal>
<signal name="SPI1_MOSI418">
</signal>
<signal name="SPI1_SCK419">
</signal>
<signal name="SPI1_MISO419">
</signal>
<signal name="SPI1_MOSI419">
</signal>
<signal name="SPI1_SCK420">
</signal>
<signal name="SPI1_MISO420">
</signal>
<signal name="SPI1_MOSI420">
</signal>
<signal name="SPI1_SCK421">
</signal>
<signal name="SPI1_MISO421">
</signal>
<signal name="SPI1_MOSI421">
</signal>
<signal name="SPI1_SCK422">
</signal>
<signal name="SPI1_MISO422">
</signal>
<signal name="SPI1_MOSI422">
</signal>
<signal name="SPI1_SCK423">
</signal>
<signal name="SPI1_MISO423">
</signal>
<signal name="SPI1_MOSI423">
</signal>
<signal name="SPI1_SCK424">
</signal>
<signal name="SPI1_MISO424">
</signal>
<signal name="SPI1_MOSI424">
</signal>
<signal name="SPI1_SCK425">
</signal>
<signal name="SPI1_MISO425">
</signal>
<signal name="SPI1_MOSI425">
</signal>
<signal name="SPI1_SCK426">
</signal>
<signal name="SPI1_MISO426">
</signal>
<signal name="SPI1_MOSI426">
</signal>
<signal name="SPI1_SCK427">
</signal>
<signal name="SPI1_MISO427">
</signal>
<signal name="SPI1_MOSI427">
</signal>
<signal name="SPI1_SCK428">
</signal>
<signal name="SPI1_MISO428">
</signal>
<signal name="SPI1_MOSI428">
</signal>
<signal name="SPI1_SCK429">
</signal>
<signal name="SPI1_MISO429">
</signal>
<signal name="SPI1_MOSI429">
</signal>
<signal name="SPI1_SCK430">
</signal>
<signal name="SPI1_MISO430">
</signal>
<signal name="SPI1_MOSI430">
</signal>
<signal name="SPI1_SCK431">
</signal>
<signal name="SPI1_MISO431">
</signal>
<signal name="SPI1_MOSI431">
</signal>
<signal name="SPI1_SCK432">
</signal>
<signal name="SPI1_MISO432">
</signal>
<signal name="SPI1_MOSI432">
</signal>
<signal name="SPI1_SCK433">
</signal>
<signal name="SPI1_MISO433">
</signal>
<signal name="SPI1_MOSI433">
</signal>
<signal name="SPI1_SCK434">
</signal>
<signal name="SPI1_MISO434">
</signal>
<signal name="SPI1_MOSI434">
</signal>
<signal name="SPI1_SCK435">
</signal>
<signal name="SPI1_MISO435">
</signal>
<signal name="SPI1_MOSI435">
</signal>
<signal name="SPI1_SCK436">
</signal>
<signal name="SPI1_MISO436">
</signal>
<signal name="SPI1_MOSI436">
</signal>
<signal name="SPI1_SCK437">
</signal>
<signal name="SPI1_MISO437">
</signal>
<signal name="SPI1_MOSI437">
</signal>
<signal name="SPI1_SCK438">
</signal>
<signal name="SPI1_MISO438">
</signal>
<signal name="SPI1_MOSI438">
</signal>
<signal name="SPI1_SCK439">
</signal>
<signal name="SPI1_MISO439">
</signal>
<signal name="SPI1_MOSI439">
</signal>
<signal name="SPI1_SCK440">
</signal>
<signal name="SPI1_MISO440">
</signal>
<signal name="SPI1_MOSI440">
</signal>
<signal name="SPI1_SCK441">
</signal>
<signal name="SPI1_MISO441">
</signal>
<signal name="SPI1_MOSI441">
</signal>
<signal name="SPI1_SCK442">
</signal>
<signal name="SPI1_MISO442">
</signal>
<signal name="SPI1_MOSI442">
</signal>
<signal name="SPI1_SCK443">
</signal>
<signal name="SPI1_MISO443">
</signal>
<signal name="SPI1_MOSI443">
</signal>
<signal name="SPI1_SCK444">
</signal>
<signal name="SPI1_MISO444">
</signal>
<signal name="SPI1_MOSI444">
</signal>
<signal name="SPI1_SCK445">
</signal>
<signal name="SPI1_MISO445">
</signal>
<signal name="SPI1_MOSI445">
</signal>
<signal name="SPI1_SCK446">
</signal>
<signal name="SPI1_MISO446">
</signal>
<signal name="SPI1_MOSI446">
</signal>
<signal name="SPI1_SCK447">
</signal>
<signal name="SPI1_MISO447">
</signal>
<signal name="SPI1_MOSI447">
</signal>
<signal name="SPI1_SCK448">
</signal>
<signal name="SPI1_MISO448">
</signal>
<signal name="SPI1_MOSI448">
</signal>
<signal name="SPI1_SCK449">
</signal>
<signal name="SPI1_MISO449">
</signal>
<signal name="SPI1_MOSI449">
</signal>
<signal name="SPI1_SCK450">
</signal>
<signal name="SPI1_MISO450">
</signal>
<signal name="SPI1_MOSI450">
</signal>
<signal name="SPI1_SCK451">
</signal>
<signal name="SPI1_MISO451">
</signal>
<signal name="SPI1_MOSI451">
</signal>
<signal name="SPI1_SCK452">
</signal>
<signal name="SPI1_MISO452">
</signal>
<signal name="SPI1_MOSI452">
</signal>
<signal name="SPI1_SCK453">
</signal>
<signal name="SPI1_MISO453">
</signal>
<signal name="SPI1_MOSI453">
</signal>
<signal name="SPI1_SCK454">
</signal>
<signal name="SPI1_MISO454">
</signal>
<signal name="SPI1_MOSI454">
</signal>
<signal name="SPI1_SCK455">
</signal>
<signal name="SPI1_MISO455">
</signal>
<signal name="SPI1_MOSI455">
</signal>
<signal name="SPI1_SCK456">
</signal>
<signal name="SPI1_MISO456">
</signal>
<signal name="SPI1_MOSI456">
</signal>
<signal name="SPI1_SCK457">
</signal>
<signal name="SPI1_MISO457">
</signal>
<signal name="SPI1_MOSI457">
</signal>
<signal name="SPI1_SCK458">
</signal>
<signal name="SPI1_MISO458">
</signal>
<signal name="SPI1_MOSI458">
</signal>
<signal name="SPI1_SCK459">
</signal>
<signal name="SPI1_MISO459">
</signal>
<signal name="SPI1_MOSI459">
</signal>
<signal name="SPI1_SCK460">
</signal>
<signal name="SPI1_MISO460">
</signal>
<signal name="SPI1_MOSI460">
</signal>
<signal name="SPI1_SCK461">
</signal>
<signal name="SPI1_MISO461">
</signal>
<signal name="SPI1_MOSI461">
</signal>
<signal name="SPI1_SCK462">
</signal>
<signal name="SPI1_MISO462">
</signal>
<signal name="SPI1_MOSI462">
</signal>
<signal name="SPI1_SCK463">
</signal>
<signal name="SPI1_MISO463">
</signal>
<signal name="SPI1_MOSI463">
</signal>
<signal name="SPI1_SCK464">
</signal>
<signal name="SPI1_MISO464">
</signal>
<signal name="SPI1_MOSI464">
</signal>
<signal name="SPI1_SCK465">
</signal>
<signal name="SPI1_MISO465">
</signal>
<signal name="SPI1_MOSI465">
</signal>
<signal name="SPI1_SCK466">
</signal>
<signal name="SPI1_MISO466">
</signal>
<signal name="SPI1_MOSI466">
</signal>
<signal name="SPI1_SCK467">
</signal>
<signal name="SPI1_MISO467">
</signal>
<signal name="SPI1_MOSI467">
</signal>
<signal name="SPI1_SCK468">
</signal>
<signal name="SPI1_MISO468">
</signal>
<signal name="SPI1_MOSI468">
</signal>
<signal name="SPI1_SCK469">
</signal>
<signal name="SPI1_MISO469">
</signal>
<signal name="SPI1_MOSI469">
</signal>
<signal name="SPI1_SCK470">
</signal>
<signal name="SPI1_MISO470">
</signal>
<signal name="SPI1_MOSI470">
</signal>
<signal name="SPI1_SCK471">
</signal>
<signal name="SPI1_MISO471">
</signal>
<signal name="SPI1_MOSI471">
</signal>
<signal name="SPI1_SCK472">
</signal>
<signal name="SPI1_MISO472">
</signal>
<signal name="SPI1_MOSI472">
</signal>
<signal name="SPI1_SCK473">
</signal>
<signal name="SPI1_MISO473">
</signal>
<signal name="SPI1_MOSI473">
</signal>
<signal name="SPI1_SCK474">
</signal>
<signal name="SPI1_MISO474">
</signal>
<signal name="SPI1_MOSI474">
</signal>
<signal name="SPI1_SCK475">
</signal>
<signal name="SPI1_MISO475">
</signal>
<signal name="SPI1_MOSI475">
</signal>
<signal name="SPI1_SCK476">
</signal>
<signal name="SPI1_MISO476">
</signal>
<signal name="SPI1_MOSI476">
</signal>
<signal name="SPI1_SCK477">
</signal>
<signal name="SPI1_MISO477">
</signal>
<signal name="SPI1_MOSI477">
</signal>
<signal name="SPI1_SCK478">
</signal>
<signal name="SPI1_MISO478">
</signal>
<signal name="SPI1_MOSI478">
</signal>
<signal name="SPI1_SCK479">
</signal>
<signal name="SPI1_MISO479">
</signal>
<signal name="SPI1_MOSI479">
</signal>
<signal name="SPI1_SCK480">
</signal>
<signal name="SPI1_MISO480">
</signal>
<signal name="SPI1_MOSI480">
</signal>
<signal name="SPI1_SCK481">
</signal>
<signal name="SPI1_MISO481">
</signal>
<signal name="SPI1_MOSI481">
</signal>
<signal name="SPI1_SCK482">
</signal>
<signal name="SPI1_MISO482">
</signal>
<signal name="SPI1_MOSI482">
</signal>
<signal name="SPI1_SCK483">
</signal>
<signal name="SPI1_MISO483">
</signal>
<signal name="SPI1_MOSI483">
</signal>
<signal name="SPI1_SCK484">
</signal>
<signal name="SPI1_MISO484">
</signal>
<signal name="SPI1_MOSI484">
</signal>
<signal name="SPI1_SCK485">
</signal>
<signal name="SPI1_MISO485">
</signal>
<signal name="SPI1_MOSI485">
</signal>
<signal name="SPI1_SCK486">
</signal>
<signal name="SPI1_MISO486">
</signal>
<signal name="SPI1_MOSI486">
</signal>
<signal name="SPI1_SCK487">
</signal>
<signal name="SPI1_MISO487">
</signal>
<signal name="SPI1_MOSI487">
</signal>
<signal name="SPI1_SCK488">
</signal>
<signal name="SPI1_MISO488">
</signal>
<signal name="SPI1_MOSI488">
</signal>
<signal name="SPI1_SCK489">
</signal>
<signal name="SPI1_MISO489">
</signal>
<signal name="SPI1_MOSI489">
</signal>
<signal name="SPI1_SCK490">
</signal>
<signal name="SPI1_MISO490">
</signal>
<signal name="SPI1_MOSI490">
</signal>
<signal name="SPI1_SCK491">
</signal>
<signal name="SPI1_MISO491">
</signal>
<signal name="SPI1_MOSI491">
</signal>
<signal name="SPI1_SCK492">
</signal>
<signal name="SPI1_MISO492">
</signal>
<signal name="SPI1_MOSI492">
</signal>
<signal name="SPI1_SCK493">
</signal>
<signal name="SPI1_MISO493">
</signal>
<signal name="SPI1_MOSI493">
</signal>
<signal name="SPI1_SCK494">
</signal>
<signal name="SPI1_MISO494">
</signal>
<signal name="SPI1_MOSI494">
</signal>
<signal name="SPI1_SCK495">
</signal>
<signal name="SPI1_MISO495">
</signal>
<signal name="SPI1_MOSI495">
</signal>
<signal name="SPI1_SCK496">
</signal>
<signal name="SPI1_MISO496">
</signal>
<signal name="SPI1_MOSI496">
</signal>
<signal name="SPI1_SCK497">
</signal>
<signal name="SPI1_MISO497">
</signal>
<signal name="SPI1_MOSI497">
</signal>
<signal name="SPI1_SCK498">
</signal>
<signal name="SPI1_MISO498">
</signal>
<signal name="SPI1_MOSI498">
</signal>
<signal name="SPI1_SCK499">
</signal>
<signal name="SPI1_MISO499">
</signal>
<signal name="SPI1_MOSI499">
</signal>
<signal name="SPI1_SCK500">
</signal>
<signal name="SPI1_MISO500">
</signal>
<signal name="SPI1_MOSI500">
</signal>
<signal name="SPI1_SCK501">
</signal>
<signal name="SPI1_MISO501">
</signal>
<signal name="SPI1_MOSI501">
</signal>
<signal name="SPI1_SCK502">
</signal>
<signal name="SPI1_MISO502">
</signal>
<signal name="SPI1_MOSI502">
</signal>
<signal name="SPI1_SCK503">
</signal>
<signal name="SPI1_MISO503">
</signal>
<signal name="SPI1_MOSI503">
</signal>
<signal name="SPI1_SCK504">
</signal>
<signal name="SPI1_MISO504">
</signal>
<signal name="SPI1_MOSI504">
</signal>
<signal name="SPI1_SCK505">
</signal>
<signal name="SPI1_MISO505">
</signal>
<signal name="SPI1_MOSI505">
</signal>
<signal name="SPI1_SCK506">
</signal>
<signal name="SPI1_MISO506">
</signal>
<signal name="SPI1_MOSI506">
</signal>
<signal name="SPI1_SCK507">
</signal>
<signal name="SPI1_MISO507">
</signal>
<signal name="SPI1_MOSI507">
</signal>
<signal name="SPI1_SCK508">
</signal>
<signal name="SPI1_MISO508">
</signal>
<signal name="SPI1_MOSI508">
</signal>
<signal name="SPI1_SCK509">
</signal>
<signal name="SPI1_MISO509">
</signal>
<signal name="SPI1_MOSI509">
</signal>
<signal name="SPI1_SCK510">
</signal>
<signal name="SPI1_MISO510">
</signal>
<signal name="SPI1_MOSI510">
</signal>
<signal name="SPI1_SCK511">
</signal>
<signal name="SPI1_MISO511">
</signal>
<signal name="SPI1_MOSI511">
</signal>
<signal name="SPI1_SCK512">
</signal>
<signal name="SPI1_MISO512">
</signal>
<signal name="SPI1_MOSI512">
</signal>
<signal name="SPI1_SCK513">
</signal>
<signal name="SPI1_MISO513">
</signal>
<signal name="SPI1_MOSI513">
</signal>
<signal name="SPI1_SCK514">
</signal>
<signal name="SPI1_MISO514">
</signal>
<signal name="SPI1_MOSI514">
</signal>
<signal name="SPI1_SCK515">
</signal>
<signal name="SPI1_MISO515">
</signal>
<signal name="SPI1_MOSI515">
</signal>
<signal name="SPI1_SCK516">
</signal>
<signal name="SPI1_MISO516">
</signal>
<signal name="SPI1_MOSI516">
</signal>
<signal name="SPI1_SCK517">
</signal>
<signal name="SPI1_MISO517">
</signal>
<signal name="SPI1_MOSI517">
</signal>
<signal name="SPI1_SCK518">
</signal>
<signal name="SPI1_MISO518">
</signal>
<signal name="SPI1_MOSI518">
</signal>
<signal name="SPI1_SCK519">
</signal>
<signal name="SPI1_MISO519">
</signal>
<signal name="SPI1_MOSI519">
</signal>
<signal name="SPI1_SCK520">
</signal>
<signal name="SPI1_MISO520">
</signal>
<signal name="SPI1_MOSI520">
</signal>
<signal name="SPI1_SCK521">
</signal>
<signal name="SPI1_MISO521">
</signal>
<signal name="SPI1_MOSI521">
</signal>
<signal name="SPI1_SCK522">
</signal>
<signal name="SPI1_MISO522">
</signal>
<signal name="SPI1_MOSI522">
</signal>
<signal name="SPI1_SCK523">
</signal>
<signal name="SPI1_MISO523">
</signal>
<signal name="SPI1_MOSI523">
</signal>
<signal name="SPI1_SCK524">
</signal>
<signal name="SPI1_MISO524">
</signal>
<signal name="SPI1_MOSI524">
</signal>
<signal name="SPI1_SCK525">
</signal>
<signal name="SPI1_MISO525">
</signal>
<signal name="SPI1_MOSI525">
</signal>
<signal name="SPI1_SCK526">
</signal>
<signal name="SPI1_MISO526">
</signal>
<signal name="SPI1_MOSI526">
</signal>
<signal name="SPI1_SCK527">
</signal>
<signal name="SPI1_MISO527">
</signal>
<signal name="SPI1_MOSI527">
</signal>
<signal name="SPI1_SCK528">
</signal>
<signal name="SPI1_MISO528">
</signal>
<signal name="SPI1_MOSI528">
</signal>
<signal name="SPI1_SCK529">
</signal>
<signal name="SPI1_MISO529">
</signal>
<signal name="SPI1_MOSI529">
</signal>
<signal name="SPI1_SCK530">
</signal>
<signal name="SPI1_MISO530">
</signal>
<signal name="SPI1_MOSI530">
</signal>
<signal name="SPI1_SCK531">
</signal>
<signal name="SPI1_MISO531">
</signal>
<signal name="SPI1_MOSI531">
</signal>
<signal name="SPI1_SCK532">
</signal>
<signal name="SPI1_MISO532">
</signal>
<signal name="SPI1_MOSI532">
</signal>
<signal name="SPI1_SCK533">
</signal>
<signal name="SPI1_MISO533">
</signal>
<signal name="SPI1_MOSI533">
</signal>
<signal name="SPI1_SCK534">
</signal>
<signal name="SPI1_MISO534">
</signal>
<signal name="SPI1_MOSI534">
</signal>
<signal name="SPI1_SCK535">
</signal>
<signal name="SPI1_MISO535">
</signal>
<signal name="SPI1_MOSI535">
</signal>
<signal name="SPI1_SCK536">
</signal>
<signal name="SPI1_MISO536">
</signal>
<signal name="SPI1_MOSI536">
</signal>
<signal name="SPI1_SCK537">
</signal>
<signal name="SPI1_MISO537">
</signal>
<signal name="SPI1_MOSI537">
</signal>
<signal name="SPI1_SCK538">
</signal>
<signal name="SPI1_MISO538">
</signal>
<signal name="SPI1_MOSI538">
</signal>
<signal name="SPI1_SCK539">
</signal>
<signal name="SPI1_MISO539">
</signal>
<signal name="SPI1_MOSI539">
</signal>
<signal name="SPI1_SCK540">
</signal>
<signal name="SPI1_MISO540">
</signal>
<signal name="SPI1_MOSI540">
</signal>
<signal name="SPI1_SCK541">
</signal>
<signal name="SPI1_MISO541">
</signal>
<signal name="SPI1_MOSI541">
</signal>
<signal name="SPI1_SCK542">
</signal>
<signal name="SPI1_MISO542">
</signal>
<signal name="SPI1_MOSI542">
</signal>
<signal name="SPI1_SCK543">
</signal>
<signal name="SPI1_MISO543">
</signal>
<signal name="SPI1_MOSI543">
</signal>
<signal name="SPI1_SCK544">
</signal>
<signal name="SPI1_MISO544">
</signal>
<signal name="SPI1_MOSI544">
</signal>
<signal name="SPI1_SCK545">
</signal>
<signal name="SPI1_MISO545">
</signal>
<signal name="SPI1_MOSI545">
</signal>
<signal name="SPI1_SCK546">
</signal>
<signal name="SPI1_MISO546">
</signal>
<signal name="SPI1_MOSI546">
</signal>
<signal name="SPI1_SCK547">
</signal>
<signal name="SPI1_MISO547">
</signal>
<signal name="SPI1_MOSI547">
</signal>
<signal name="SPI1_SCK548">
</signal>
<signal name="SPI1_MISO548">
</signal>
<signal name="SPI1_MOSI548">
</signal>
<signal name="SPI1_SCK549">
</signal>
<signal name="SPI1_MISO549">
</signal>
<signal name="SPI1_MOSI549">
</signal>
<signal name="SPI1_SCK550">
</signal>
<signal name="SPI1_MISO550">
</signal>
<signal name="SPI1_MOSI550">
</signal>
<signal name="SPI1_SCK551">
</signal>
<signal name="SPI1_MISO551">
</signal>
<signal name="SPI1_MOSI551">
</signal>
<signal name="SPI1_SCK552">
</signal>
<signal name="SPI1_MISO552">
</signal>
<signal name="SPI1_MOSI552">
</signal>
<signal name="SPI1_SCK553">
</signal>
<signal name="SPI1_MISO553">
</signal>
<signal name="SPI1_MOSI553">
</signal>
<signal name="SPI1_SCK554">
</signal>
<signal name="SPI1_MISO554">
</signal>
<signal name="SPI1_MOSI554">
</signal>
<signal name="SPI1_SCK555">
</signal>
<signal name="SPI1_MISO555">
</signal>
<signal name="SPI1_MOSI555">
</signal>
<signal name="SPI1_SCK556">
</signal>
<signal name="SPI1_MISO556">
</signal>
<signal name="SPI1_MOSI556">
</signal>
<signal name="SPI1_SCK557">
</signal>
<signal name="SPI1_MISO557">
</signal>
<signal name="SPI1_MOSI557">
</signal>
<signal name="SPI1_SCK558">
</signal>
<signal name="SPI1_MISO558">
</signal>
<signal name="SPI1_MOSI558">
</signal>
<signal name="SPI1_SCK559">
</signal>
<signal name="SPI1_MISO559">
</signal>
<signal name="SPI1_MOSI559">
</signal>
<signal name="SPI1_SCK560">
</signal>
<signal name="SPI1_MISO560">
</signal>
<signal name="SPI1_MOSI560">
</signal>
<signal name="SPI1_SCK561">
</signal>
<signal name="SPI1_MISO561">
</signal>
<signal name="SPI1_MOSI561">
</signal>
<signal name="SPI1_SCK562">
</signal>
<signal name="SPI1_MISO562">
</signal>
<signal name="SPI1_MOSI562">
</signal>
<signal name="SPI1_SCK563">
</signal>
<signal name="SPI1_MISO563">
</signal>
<signal name="SPI1_MOSI563">
</signal>
<signal name="SPI1_SCK564">
</signal>
<signal name="SPI1_MISO564">
</signal>
<signal name="SPI1_MOSI564">
</signal>
<signal name="SPI1_SCK565">
</signal>
<signal name="SPI1_MISO565">
</signal>
<signal name="SPI1_MOSI565">
</signal>
<signal name="SPI1_SCK566">
</signal>
<signal name="SPI1_MISO566">
</signal>
<signal name="SPI1_MOSI566">
</signal>
<signal name="SPI1_SCK567">
</signal>
<signal name="SPI1_MISO567">
</signal>
<signal name="SPI1_MOSI567">
</signal>
<signal name="SPI1_SCK568">
</signal>
<signal name="SPI1_MISO568">
</signal>
<signal name="SPI1_MOSI568">
</signal>
<signal name="SPI1_SCK569">
</signal>
<signal name="SPI1_MISO569">
</signal>
<signal name="SPI1_MOSI569">
</signal>
<signal name="SPI1_SCK570">
</signal>
<signal name="SPI1_MISO570">
</signal>
<signal name="SPI1_MOSI570">
</signal>
<signal name="SPI1_SCK571">
</signal>
<signal name="SPI1_MISO571">
</signal>
<signal name="SPI1_MOSI571">
</signal>
<signal name="SPI1_SCK572">
</signal>
<signal name="SPI1_MISO572">
</signal>
<signal name="SPI1_MOSI572">
</signal>
<signal name="SPI1_SCK573">
</signal>
<signal name="SPI1_MISO573">
</signal>
<signal name="SPI1_MOSI573">
</signal>
<signal name="SPI1_SCK574">
</signal>
<signal name="SPI1_MISO574">
</signal>
<signal name="SPI1_MOSI574">
</signal>
<signal name="SPI1_SCK575">
</signal>
<signal name="SPI1_MISO575">
</signal>
<signal name="SPI1_MOSI575">
</signal>
<signal name="SPI1_SCK576">
</signal>
<signal name="SPI1_MISO576">
</signal>
<signal name="SPI1_MOSI576">
</signal>
<signal name="SPI1_SCK577">
</signal>
<signal name="SPI1_MISO577">
</signal>
<signal name="SPI1_MOSI577">
</signal>
<signal name="SPI1_SCK578">
</signal>
<signal name="SPI1_MISO578">
</signal>
<signal name="SPI1_MOSI578">
</signal>
<signal name="SPI1_SCK579">
</signal>
<signal name="SPI1_MISO579">
</signal>
<signal name="SPI1_MOSI579">
</signal>
<signal name="SPI1_SCK580">
</signal>
<signal name="SPI1_MISO580">
</signal>
<signal name="SPI1_MOSI580">
</signal>
<signal name="SPI1_SCK581">
</signal>
<signal name="SPI1_MISO581">
</signal>
<signal name="SPI1_MOSI581">
</signal>
<signal name="SPI1_SCK582">
</signal>
<signal name="SPI1_MISO582">
</signal>
<signal name="SPI1_MOSI582">
</signal>
<signal name="SPI1_SCK583">
</signal>
<signal name="SPI1_MISO583">
</signal>
<signal name="SPI1_MOSI583">
</signal>
<signal name="SPI1_SCK584">
</signal>
<signal name="SPI1_MISO584">
</signal>
<signal name="SPI1_MOSI584">
</signal>
<signal name="SPI1_SCK585">
</signal>
<signal name="SPI1_MISO585">
</signal>
<signal name="SPI1_MOSI585">
</signal>
<signal name="SPI1_SCK586">
</signal>
<signal name="SPI1_MISO586">
</signal>
<signal name="SPI1_MOSI586">
</signal>
<signal name="SPI1_SCK587">
</signal>
<signal name="SPI1_MISO587">
</signal>
<signal name="SPI1_MOSI587">
</signal>
<signal name="SPI1_SCK588">
</signal>
<signal name="SPI1_MISO588">
</signal>
<signal name="SPI1_MOSI588">
</signal>
<signal name="SPI1_SCK589">
</signal>
<signal name="SPI1_MISO589">
</signal>
<signal name="SPI1_MOSI589">
</signal>
<signal name="SPI1_SCK590">
</signal>
<signal name="SPI1_MISO590">
</signal>
<signal name="SPI1_MOSI590">
</signal>
<signal name="SPI1_SCK591">
</signal>
<signal name="SPI1_MISO591">
</signal>
<signal name="SPI1_MOSI591">
</signal>
<signal name="SPI1_SCK592">
</signal>
<signal name="SPI1_MISO592">
</signal>
<signal name="SPI1_MOSI592">
</signal>
<signal name="SPI1_SCK593">
</signal>
<signal name="SPI1_MISO593">
</signal>
<signal name="SPI1_MOSI593">
</signal>
<signal name="SPI1_SCK594">
</signal>
<signal name="SPI1_MISO594">
</signal>
<signal name="SPI1_MOSI594">
</signal>
<signal name="SPI1_SCK595">
</signal>
<signal name="SPI1_MISO595">
</signal>
<signal name="SPI1_MOSI595">
</signal>
<signal name="SPI1_SCK596">
</signal>
<signal name="SPI1_MISO596">
</signal>
<signal name="SPI1_MOSI596">
</signal>
<signal name="SPI1_SCK597">
</signal>
<signal name="SPI1_MISO597">
</signal>
<signal name="SPI1_MOSI597">
</signal>
<signal name="SPI1_SCK598">
</signal>
<signal name="SPI1_MISO598">
</signal>
<signal name="SPI1_MOSI598">
</signal>
<signal name="SPI1_SCK599">
</signal>
<signal name="SPI1_MISO599">
</signal>
<signal name="SPI1_MOSI599">
</signal>
<signal name="SPI1_SCK600">
</signal>
<signal name="SPI1_MISO600">
</signal>
<signal name="SPI1_MOSI600">
</signal>
<signal name="SPI1_SCK601">
</signal>
<signal name="SPI1_MISO601">
</signal>
<signal name="SPI1_MOSI601">
</signal>
<signal name="SPI1_SCK602">
</signal>
<signal name="SPI1_MISO602">
</signal>
<signal name="SPI1_MOSI602">
</signal>
<signal name="SPI1_SCK603">
</signal>
<signal name="SPI1_MISO603">
</signal>
<signal name="SPI1_MOSI603">
</signal>
<signal name="SPI1_SCK604">
</signal>
<signal name="SPI1_MISO604">
</signal>
<signal name="SPI1_MOSI604">
</signal>
<signal name="SPI1_SCK605">
</signal>
<signal name="SPI1_MISO605">
</signal>
<signal name="SPI1_MOSI605">
</signal>
<signal name="SPI1_SCK606">
</signal>
<signal name="SPI1_MISO606">
</signal>
<signal name="SPI1_MOSI606">
</signal>
<signal name="SPI1_SCK607">
</signal>
<signal name="SPI1_MISO607">
</signal>
<signal name="SPI1_MOSI607">
</signal>
<signal name="SPI1_SCK608">
</signal>
<signal name="SPI1_MISO608">
</signal>
<signal name="SPI1_MOSI608">
</signal>
<signal name="SPI1_SCK609">
</signal>
<signal name="SPI1_MISO609">
</signal>
<signal name="SPI1_MOSI609">
</signal>
<signal name="SPI1_SCK610">
</signal>
<signal name="SPI1_MISO610">
</signal>
<signal name="SPI1_MOSI610">
</signal>
<signal name="SPI1_SCK611">
</signal>
<signal name="SPI1_MISO611">
</signal>
<signal name="SPI1_MOSI611">
</signal>
<signal name="SPI1_SCK612">
</signal>
<signal name="SPI1_MISO612">
</signal>
<signal name="SPI1_MOSI612">
</signal>
<signal name="SPI1_SCK613">
</signal>
<signal name="SPI1_MISO613">
</signal>
<signal name="SPI1_MOSI613">
</signal>
<signal name="SPI1_SCK614">
</signal>
<signal name="SPI1_MISO614">
</signal>
<signal name="SPI1_MOSI614">
</signal>
<signal name="SPI1_SCK615">
</signal>
<signal name="SPI1_MISO615">
</signal>
<signal name="SPI1_MOSI615">
</signal>
<signal name="SPI1_SCK616">
</signal>
<signal name="SPI1_MISO616">
</signal>
<signal name="SPI1_MOSI616">
</signal>
<signal name="SPI1_SCK617">
</signal>
<signal name="SPI1_MISO617">
</signal>
<signal name="SPI1_MOSI617">
</signal>
<signal name="SPI1_SCK618">
</signal>
<signal name="SPI1_MISO618">
</signal>
<signal name="SPI1_MOSI618">
</signal>
<signal name="SPI1_SCK619">
</signal>
<signal name="SPI1_MISO619">
</signal>
<signal name="SPI1_MOSI619">
</signal>
<signal name="SPI1_SCK620">
</signal>
<signal name="SPI1_MISO620">
</signal>
<signal name="SPI1_MOSI620">
</signal>
<signal name="SPI1_SCK621">
</signal>
<signal name="SPI1_MISO621">
</signal>
<signal name="SPI1_MOSI621">
</signal>
<signal name="SPI1_SCK622">
</signal>
<signal name="SPI1_MISO622">
</signal>
<signal name="SPI1_MOSI622">
</signal>
<signal name="SPI1_SCK623">
</signal>
<signal name="SPI1_MISO623">
</signal>
<signal name="SPI1_MOSI623">
</signal>
<signal name="SPI1_SCK624">
</signal>
<signal name="SPI1_MISO624">
</signal>
<signal name="SPI1_MOSI624">
</signal>
<signal name="SPI1_SCK625">
</signal>
<signal name="SPI1_MISO625">
</signal>
<signal name="SPI1_MOSI625">
</signal>
<signal name="SPI1_SCK626">
</signal>
<signal name="SPI1_MISO626">
</signal>
<signal name="SPI1_MOSI626">
</signal>
<signal name="SPI1_SCK627">
</signal>
<signal name="SPI1_MISO627">
</signal>
<signal name="SPI1_MOSI627">
</signal>
<signal name="SPI1_SCK628">
</signal>
<signal name="SPI1_MISO628">
</signal>
<signal name="SPI1_MOSI628">
</signal>
<signal name="SPI1_SCK629">
</signal>
<signal name="SPI1_MISO629">
</signal>
<signal name="SPI1_MOSI629">
</signal>
<signal name="SPI1_SCK630">
</signal>
<signal name="SPI1_MISO630">
</signal>
<signal name="SPI1_MOSI630">
</signal>
<signal name="SPI1_SCK631">
</signal>
<signal name="SPI1_MISO631">
</signal>
<signal name="SPI1_MOSI631">
</signal>
<signal name="SPI1_SCK632">
</signal>
<signal name="SPI1_MISO632">
</signal>
<signal name="SPI1_MOSI632">
</signal>
<signal name="SPI1_SCK633">
</signal>
<signal name="SPI1_MISO633">
</signal>
<signal name="SPI1_MOSI633">
</signal>
<signal name="SPI1_SCK634">
</signal>
<signal name="SPI1_MISO634">
</signal>
<signal name="SPI1_MOSI634">
</signal>
<signal name="SPI1_SCK635">
</signal>
<signal name="SPI1_MISO635">
</signal>
<signal name="SPI1_MOSI635">
</signal>
<signal name="SPI1_SCK636">
</signal>
<signal name="SPI1_MISO636">
</signal>
<signal name="SPI1_MOSI636">
</signal>
<signal name="SPI1_SCK637">
</signal>
<signal name="SPI1_MISO637">
</signal>
<signal name="SPI1_MOSI637">
</signal>
<signal name="SPI1_SCK638">
</signal>
<signal name="SPI1_MISO638">
</signal>
<signal name="SPI1_MOSI638">
</signal>
<signal name="SPI1_SCK639">
</signal>
<signal name="SPI1_MISO639">
</signal>
<signal name="SPI1_MOSI639">
</signal>
<signal name="SPI1_SCK640">
</signal>
<signal name="SPI1_MISO640">
</signal>
<signal name="SPI1_MOSI640">
</signal>
<signal name="SPI1_SCK641">
</signal>
<signal name="SPI1_MISO641">
</signal>
<signal name="SPI1_MOSI641">
</signal>
<signal name="SPI1_SCK642">
</signal>
<signal name="SPI1_MISO642">
</signal>
<signal name="SPI1_MOSI642">
</signal>
<signal name="SPI1_SCK643">
</signal>
<signal name="SPI1_MISO643">
</signal>
<signal name="SPI1_MOSI643">
</signal>
<signal name="SPI1_SCK644">
</signal>
<signal name="SPI1_MISO644">
</signal>
<signal name="SPI1_MOSI644">
</signal>
<signal name="SPI1_SCK645">
</signal>
<signal name="SPI1_MISO645">
</signal>
<signal name="SPI1_MOSI645">
</signal>
<signal name="SPI1_SCK646">
</signal>
<signal name="SPI1_MISO646">
</signal>
<signal name="SPI1_MOSI646">
</signal>
<signal name="SPI1_SCK647">
</signal>
<signal name="SPI1_MISO647">
</signal>
<signal name="SPI1_MOSI647">
</signal>
<signal name="SPI1_SCK648">
</signal>
<signal name="SPI1_MISO648">
</signal>
<signal name="SPI1_MOSI648">
</signal>
<signal name="SPI1_SCK649">
</signal>
<signal name="SPI1_MISO649">
</signal>
<signal name="SPI1_MOSI649">
</signal>
<signal name="SPI1_SCK650">
</signal>
<signal name="SPI1_MISO650">
</signal>
<signal name="SPI1_MOSI650">
</signal>
<signal name="SPI1_SCK651">
</signal>
<signal name="SPI1_MISO651">
</signal>
<signal name="SPI1_MOSI651">
</signal>
<signal name="SPI1_SCK652">
</signal>
<signal name="SPI1_MISO652">
</signal>
<signal name="SPI1_MOSI652">
</signal>
<signal name="SPI1_SCK653">
</signal>
<signal name="SPI1_MISO653">
</signal>
<signal name="SPI1_MOSI653">
</signal>
<signal name="SPI1_SCK654">
</signal>
<signal name="SPI1_MISO654">
</signal>
<signal name="SPI1_MOSI654">
</signal>
<signal name="SPI1_SCK655">
</signal>
<signal name="SPI1_MISO655">
</signal>
<signal name="SPI1_MOSI655">
</signal>
<signal name="SPI1_SCK656">
</signal>
<signal name="SPI1_MISO656">
</signal>
<signal name="SPI1_MOSI656">
</signal>
<signal name="SPI1_SCK657">
</signal>
<signal name="SPI1_MISO657">
</signal>
<signal name="SPI1_MOSI657">
</signal>
<signal name="SPI1_SCK658">
</signal>
<signal name="SPI1_MISO658">
</signal>
<signal name="SPI1_MOSI658">
</signal>
<signal name="SPI1_SCK659">
</signal>
<signal name="SPI1_MISO659">
</signal>
<signal name="SPI1_MOSI659">
</signal>
<signal name="SPI1_SCK660">
</signal>
<signal name="SPI1_MISO660">
</signal>
<signal name="SPI1_MOSI660">
</signal>
<signal name="SPI1_SCK661">
</signal>
<signal name="SPI1_MISO661">
</signal>
<signal name="SPI1_MOSI661">
</signal>
<signal name="SPI1_SCK662">
</signal>
<signal name="SPI1_MISO662">
</signal>
<signal name="SPI1_MOSI662">
</signal>
<signal name="SPI1_SCK663">
</signal>
<signal name="SPI1_MISO663">
</signal>
<signal name="SPI1_MOSI663">
</signal>
<signal name="ADC1_CH1">
<contactref element="U1" pad="11"/>
<contactref element="R7" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="ADC1_CH2">
<contactref element="U1" pad="12"/>
<contactref element="R22" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="ADC1_CH3">
<contactref element="U1" pad="13"/>
<contactref element="R5" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="ADC1_CH4">
<contactref element="U1" pad="14"/>
<contactref element="R20" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="ADC1_CH5">
<contactref element="U1" pad="15"/>
<contactref element="R3" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="ADC1_CH7">
<contactref element="U1" pad="17"/>
<contactref element="R9" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="ADC1_CH6">
<contactref element="U1" pad="16"/>
<contactref element="R2" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="ADC1_CH0">
<contactref element="U1" pad="10"/>
<contactref element="R8" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="SPI2_MOSI">
<contactref element="U1" pad="28"/>
<contactref element="J3" pad="DAT"/>
</signal>
<signal name="SPI2_CS_OLED">
<contactref element="J3" pad="CS"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="SPI2_SCK">
<contactref element="U1" pad="26"/>
<contactref element="J3" pad="CLK"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="U2" pad="3"/>
<contactref element="M2" pad="2"/>
</signal>
<signal name="LOAD">
<contactref element="M1" pad="4"/>
<contactref element="R30" pad="1"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="OLED_DC">
<contactref element="J3" pad="D/C"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="OLED_RST">
<contactref element="J3" pad="RST"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="3"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="4"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="5"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="6"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="7"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R31" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="M2" pad="1"/>
</signal>
<signal name="VCC1">
</signal>
<signal name="VCC4">
</signal>
<signal name="VCC5">
</signal>
</signals>
</board>
</drawing>
</eagle>
