<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="30.48" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="45.72" y2="0" width="0" layer="20"/>
<wire x1="45.72" y1="0" x2="48.26" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="48.26" y1="2.54" x2="48.26" y2="30.48" width="0" layer="20"/>
<wire x1="48.26" y1="30.48" x2="45.72" y2="33.02" width="0" layer="20" curve="90"/>
<wire x1="45.72" y1="33.02" x2="2.54" y2="33.02" width="0" layer="20"/>
<wire x1="2.54" y1="33.02" x2="0" y2="30.48" width="0" layer="20" curve="90"/>
<text>tiny.akrobotnerd.com</text>
<text>Yellow
LED: 4
Btn: 8</text>
<text>Buzzer: 5</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>Buzzer</text>
<text>Btn</text>
<text>Btn</text>
<text>Btn</text>
<text>Btn</text>
<text>+</text>
<text>Off</text>
<text>On</text>
<text>Green
LED: 7
Btn: 6</text>
<text>Red
LED: 10
Btn: 9</text>
<text>Blue
LED: 3
Btn: 1</text>
<text>Simon Says v3</text>
<text>Created
by
Michael Backus</text>
</plain>
<libraries>
<library name="Backus">
<packages>
<package name="TACTILESWITCH">
</package>
<package name="DIP14">
</package>
<package name="BATTERY-AAA-KIT">
<description>&lt;h3&gt;AAA Battery Clips (KIT Variant)&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AAA battery.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DO41-7">
</package>
<package name="EG1218">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electromechanical Parts&lt;/h3&gt;
This library contains electromechanical devices, like motors, speakers,servos, and relays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM-KIT">
<description>&lt;h3&gt;12mm Buzzer - PTH (KIT VARIANT)&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BT1" library="Backus" package="BATTERY-AAA-KIT" value="">
<attribute name="PROD_ID" value="BATT-08571"/>
<attribute name="SF_SKU" value="PRT-12718"/>
<attribute name="VALUE"/>
</element>
<element name="BT2" library="Backus" package="BATTERY-AAA-KIT" value="">
<attribute name="PROD_ID" value="BATT-08571"/>
<attribute name="SF_SKU" value="PRT-12718"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Backus" package="DIP14" value="ATTINY84ATTINY84-20PU"/>
<element name="BLUE-BTN" library="Backus" package="TACTILESWITCH" value="TACTILESWITCH"/>
<element name="GREEN-BTN" library="Backus" package="TACTILESWITCH" value="TACTILESWITCH"/>
<element name="YELLOW-BTN" library="Backus" package="TACTILESWITCH" value="TACTILESWITCH"/>
<element name="RED-BTN" library="Backus" package="TACTILESWITCH" value="TACTILESWITCH"/>
<element name="BLUE-LED" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="YELLOW-LED" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN-LED" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="RED-LED" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="D5" library="adafruit" package="DO41-7" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="adafruit" package="EG1218" value=""/>
<element name="LS1" library="SparkFun-Electromechanical" package="BUZZER-12MM-KIT" value="BUZZER-PTH_KIT">
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
</element>
<element name="BT3" library="Backus" package="BATTERY-AAA-KIT" value="">
<attribute name="PROD_ID" value="BATT-08571"/>
<attribute name="SF_SKU" value="PRT-12718"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="BT1" pad="GND@1" route="any" routetag="G$1.-"/>
<contactref element="BT2" pad="PWR@1" route="any" routetag="G$1.+"/>
<contactref element="BT1" pad="GND@2" route="any" routetag="G$1.-"/>
<contactref element="BT2" pad="PWR@2" route="any" routetag="G$1.+"/>
</signal>
<signal name="GND">
<contactref element="BLUE-BTN" pad="P$1"/>
<contactref element="GREEN-BTN" pad="P$1"/>
<contactref element="YELLOW-BTN" pad="P$1"/>
<contactref element="RED-BTN" pad="P$1"/>
<contactref element="LS1" pad="-"/>
<contactref element="GREEN-LED" pad="K"/>
<contactref element="RED-LED" pad="K"/>
<contactref element="YELLOW-LED" pad="K"/>
<contactref element="BLUE-LED" pad="K"/>
<contactref element="BT3" pad="GND@1" route="any" routetag="G$1.-"/>
<contactref element="U$1" pad="14"/>
<contactref element="BT3" pad="GND@2" route="any" routetag="G$1.-"/>
</signal>
<signal name="N$5">
<contactref element="YELLOW-BTN" pad="P$2"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="D5" pad="A"/>
<contactref element="S1" pad="S"/>
</signal>
<signal name="N$12">
<contactref element="D5" pad="C"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="BT1" pad="PWR@1" route="any" routetag="G$1.+"/>
<contactref element="S1" pad="P"/>
<contactref element="BT1" pad="PWR@2" route="any" routetag="G$1.+"/>
</signal>
<signal name="N$9">
<contactref element="BLUE-BTN" pad="P$2"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$1">
<contactref element="BT2" pad="GND@1" route="any" routetag="G$1.-"/>
<contactref element="BT3" pad="PWR@1" route="any" routetag="G$1.+"/>
<contactref element="BT3" pad="PWR@2" route="any" routetag="G$1.+"/>
<contactref element="BT2" pad="GND@2" route="any" routetag="G$1.-"/>
</signal>
<signal name="N$13">
<contactref element="GREEN-BTN" pad="P$2"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="GREEN-LED" pad="A"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="RED-BTN" pad="P$2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="2"/>
<contactref element="RED-LED" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="10"/>
<contactref element="BLUE-LED" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="8"/>
<contactref element="LS1" pad="+"/>
</signal>
<signal name="N$10">
<contactref element="YELLOW-LED" pad="A"/>
<contactref element="U$1" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
