(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 46)
    (no_connects 1)
    (area 137.593667 96.06598 168.499334 113.165)
    (thickness 1.6)
    (drawings 4)
    (tracks 104)
    (zones 0)
    (modules 19)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6002 1.6002)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.1)
    (pad_to_paste_clearance -0.05)
    (aux_axis_origin 158.75 100.965)
    (grid_origin 143.002 110.49)
    (visible_elements FFFE7F7F)
    (pcbplotparams
      (layerselection 0x010e8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 bat)
  (net 2 GNDPWR)
  (net 3 vstor)
  (net 4 vin)
  (net 5 vref)
  (net 6 lbst)
  (net 7 bat_ok)
  (net 8 mppt)
  (net 9 ok_prog)
  (net 10 ok_hyst)
  (net 11 rdiv)
  (net 12 SwitchedPower)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net SwitchedPower)
  )
  (net_class OSHpark ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.7)
    (via_drill 0.33)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class logic ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.7)
    (via_drill 0.33)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net bat_ok)
    (add_net mppt)
    (add_net ok_hyst)
    (add_net ok_prog)
    (add_net rdiv)
    (add_net vref)
  )
  (net_class power ""
    (clearance 0.19)
    (trace_width 0.3)
    (via_dia 0.7)
    (via_drill 0.33)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDPWR)
    (add_net bat)
    (add_net lbst)
    (add_net vin)
    (add_net vstor)
  )
  (module myFootprints:TH400nm (layer F.Cu) (tedit 587A4A90)
    (at 162.491 112.19)
    (fp_text reference BatGnd1 (at -10.189 -14.4) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0.9 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -11.489 -12.3) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A4234)
    (at 148.59 101.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Cbyp (at 0.512 1.19) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 vstor))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A407C)
    (at 144.399 103.632)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Chv (at -2.297 0.058) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 vin))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A48A2)
    (at 146.102 108.19 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Cref (at 0.3 -1.4 270) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 vref))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A4034)
    (at 148.59 99.949)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Cstor1 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 4.7uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 vstor))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A42EC)
    (at 143.902 107.89)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference OC1 (at 0.1 1.3) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 mppt))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A4085)
    (at 144.202 105.89)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference OC2 (at -2.3 0.1) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 vin))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 mppt))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A4114)
    (at 153.289 105.283)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference OK1 (at 2.013 0.007) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 ok_prog))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A40CE)
    (at 153.302 107.09)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference ROK2 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 ok_hyst))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 ok_prog))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 placed (layer F.Cu) (tedit 587A4157)
    (at 151.102 108.09 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference OK3 (at -1 1.8 180) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 rdiv))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 ok_hyst))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootprints:TH400nm (layer F.Cu) (tedit 587A417F)
    (at 152.802 99.89)
    (fp_text reference Bat1 (at -0.5 -2.2) (layer F.SilkS) hide)
    (fp_text value Bat (at 0.9 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 bat))
  )
  (module myFootprints:TH400nm (layer F.Cu) (tedit 587A4262)
    (at 142.202 99.99)
    (fp_text reference S+ (at -0.1 1.3) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0.9 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 4 vin))
  )
  (module myFootprints:TH400nm (layer F.Cu) (tedit 587A425A)
    (at 141.802 108.59)
    (fp_text reference S- (at 0 -1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0.9 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
  )
  (module myFootprints:SOT23-6Handsolderable (layer F.Cu) (tedit 587A4122)
    (at 153.202 102.29 180)
    (descr "6 pins, \"Small Outline Transistor\"\nbased on Texas Instruments package named: DBV\nTypical part Texas Instruments TPS22860\nDiscrepancy from TI recommendations: rounded pads")
    (fp_text reference U2 (at 0 -2.2 180) (layer F.SilkS) hide)
    (fp_text value TPS22860 (at 0 2.2 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -1.6 -0.95) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 SwitchedPower))
    (pad 2 smd oval (at -1.6 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 3 smd oval (at -1.6 0.95) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd oval (at 1.6 0.95 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 bat))
    (pad 5 smd oval (at 1.6 0 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 bat))
    (pad 6 smd oval (at 1.6 -0.95 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 bat_ok))
  )
  (module myFootprints:TH400nm (layer F.Cu) (tedit 587A4194)
    (at 154.902 99.89)
    (fp_text reference V+ (at -1 -0.5) (layer F.SilkS))
    (fp_text value M- (at 0.9 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 12 SwitchedPower))
  )
  (module myFootprints:TH400nm (layer F.Cu) (tedit 587A40C2)
    (at 154.702 110.69)
    (fp_text reference V- (at 0.6 -3.3) (layer F.SilkS))
    (fp_text value M+ (at 0.9 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.3 -2.1) (size 1 1) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeE_EIA-7360_HandSoldering (layer B.Cu) (tedit 5879609D)
    (at 148.502 104.59 180)
    (descr "Tantal Cap. , Size E, EIA-7360, Hand Soldering,")
    (tags "Tantal Cap. , Size E, EIA-7360, Hand Soldering,")
    (attr smd)
    (fp_text reference CBat1 (at -0.39878 7.39902 180) (layer B.SilkS) hide)
    (fp_text value CP (at 0 -4.50088 180) (layer B.Fab))
    (fp_text user + (at -6.35 3.39852 180) (layer B.SilkS))
    (pad 2 smd rect (at 4.17576 0 180) (size 4.54914 4.39928) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDPWR))
    (pad 1 smd rect (at -4.17576 0 180) (size 4.54914 4.39928) (layers B.Cu B.Paste B.Mask)
      (net 1 bat))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeE_EIA-7360_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module myFootprints:QFN16thermalpasted (layer F.Cu) (tedit 55D4C881)
    (at 148.59 105.41)
    (fp_text reference U1 (at -2.032 -1.9685) (layer F.SilkS))
    (fp_text value BQ25504 (at 0.1905 -3.3655) (layer F.SilkS) hide)
    (pad 17 thru_hole rect (at -0.4 0.4) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (pad 17 thru_hole rect (at -0.4 -0.4) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (pad 17 thru_hole rect (at 0.4 0.4) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (pad 17 smd rect (at -0.4 -0.4) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 17 smd rect (at -0.4 0.4) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 17 smd rect (at 0.4 0.4) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 17 thru_hole rect (at 0.0445 0.0055) (size 0.85 0.85) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (pad 17 thru_hole rect (at 0.4 -0.4) (size 0.8 0.8) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDPWR))
    (pad 1 smd oval (at -1.5494 -0.7493) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 2 smd oval (at -1.5494 -0.24892) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 4 vin))
    (pad 3 smd oval (at -1.5494 0.24892) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 8 mppt))
    (pad 4 smd oval (at -1.5494 0.7493) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 5 vref))
    (pad 5 smd oval (at -0.7493 1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 6 smd oval (at -0.24892 1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 9 ok_prog))
    (pad 7 smd oval (at 0.24892 1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 11 rdiv))
    (pad 8 smd oval (at 0.7493 1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 11 rdiv))
    (pad 9 smd oval (at 1.5494 0.7493) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 10 ok_hyst))
    (pad 10 smd oval (at 1.5494 0.24892) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 9 ok_prog))
    (pad 11 smd oval (at 1.5494 -0.24892) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 7 bat_ok))
    (pad 12 smd oval (at 1.5494 -0.7493) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 13 smd oval (at 0.7493 -1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
    (pad 14 smd oval (at 0.24892 -1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 bat))
    (pad 15 smd oval (at -0.24892 -1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 3 vstor))
    (pad 16 smd oval (at -0.7493 -1.5494 90) (size 1.00076 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 6 lbst))
    (pad 17 smd rect (at 0.4 -0.4) (size 0.68 0.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDPWR))
  )
  (module myFootprints:Wurth2828 (layer F.Cu) (tedit 587A48AA)
    (at 144.78 100.965)
    (fp_text reference L1 (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value 22uH (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 1.05 0) (size 1.1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 lbst))
    (pad 2 smd rect (at -1.05 0) (size 1.1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 vin))
  )
  (gr_line (start 141.002 98.69) (end 156.402 98.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.802 109.59) (end 141.002 98.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.402 98.69) (end 156.302 109.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.802 109.69) (end 156.302 109.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 157.353 110.617) (xy 157.353 96.52) (xy 139.902 96.72) (xy 139.902 110.817)
      )
    )
  )
  (zone (net 2) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 140.202 98.29) (xy 157.302 98.29) (xy 157.102 110.79) (xy 139.702 110.89) (xy 140.202 98.29)
      )
    )
  )
)
