(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 12)
    (no_connects 0)
    (area 121.336999 78.156999 169.747001 130.123001)
    (thickness 1.6)
    (drawings 13)
    (tracks 36)
    (zones 0)
    (modules 6)
    (nets 41)
  )
  (page A4)
  (title_block
    (title Hidro-Cambodia)
    (rev 0.1)
    (company "DAI Maker Lab")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 VCC)
  (net 4 GND)
  (net 5 "Net-(SHIELD1-PadAD5)")
  (net 6 "Net-(SHIELD1-PadAD4)")
  (net 7 "Net-(SHIELD1-PadAD3)")
  (net 8 "Net-(SHIELD1-PadAD0)")
  (net 9 "Net-(SHIELD1-PadAD1)")
  (net 10 "Net-(SHIELD1-PadAD2)")
  (net 11 "Net-(SHIELD1-PadV_IN)")
  (net 12 "Net-(SHIELD1-PadGND2)")
  (net 13 "Net-(SHIELD1-Pad3V3)")
  (net 14 "Net-(SHIELD1-PadRST)")
  (net 15 "Net-(SHIELD1-Pad0)")
  (net 16 "Net-(SHIELD1-Pad1)")
  (net 17 "Net-(SHIELD1-Pad2)")
  (net 18 "Net-(SHIELD1-Pad3)")
  (net 19 "Net-(SHIELD1-Pad4)")
  (net 20 "Net-(SHIELD1-Pad5)")
  (net 21 "Net-(SHIELD1-Pad6)")
  (net 22 "Net-(SHIELD1-Pad9)")
  (net 23 "Net-(SHIELD1-Pad10)")
  (net 24 "Net-(SHIELD1-Pad11)")
  (net 25 "Net-(SHIELD1-Pad12)")
  (net 26 "Net-(SHIELD1-Pad13)")
  (net 27 "Net-(SHIELD1-PadGND3)")
  (net 28 "Net-(SHIELD1-PadAREF)")
  (net 29 "Net-(SHIELD1-PadSDA)")
  (net 30 "Net-(SHIELD1-PadSCL)")
  (net 31 "Net-(SHIELD1-PadIO_R)")
  (net 32 "Net-(SHIELD1-PadNC)")
  (net 33 "Net-(U1-Pad1)")
  (net 34 "Net-(U1-Pad8)")
  (net 35 "Net-(U1-Pad10)")
  (net 36 "Net-(U1-Pad12)")
  (net 37 "Net-(U1-Pad13)")
  (net 38 "Net-(U1-Pad14)")
  (net 39 "Net-(U1-Pad15)")
  (net 40 "Net-(U1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(SHIELD1-Pad0)")
    (add_net "Net-(SHIELD1-Pad1)")
    (add_net "Net-(SHIELD1-Pad10)")
    (add_net "Net-(SHIELD1-Pad11)")
    (add_net "Net-(SHIELD1-Pad12)")
    (add_net "Net-(SHIELD1-Pad13)")
    (add_net "Net-(SHIELD1-Pad2)")
    (add_net "Net-(SHIELD1-Pad3)")
    (add_net "Net-(SHIELD1-Pad3V3)")
    (add_net "Net-(SHIELD1-Pad4)")
    (add_net "Net-(SHIELD1-Pad5)")
    (add_net "Net-(SHIELD1-Pad6)")
    (add_net "Net-(SHIELD1-Pad9)")
    (add_net "Net-(SHIELD1-PadAD0)")
    (add_net "Net-(SHIELD1-PadAD1)")
    (add_net "Net-(SHIELD1-PadAD2)")
    (add_net "Net-(SHIELD1-PadAD3)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadGND2)")
    (add_net "Net-(SHIELD1-PadGND3)")
    (add_net "Net-(SHIELD1-PadIO_R)")
    (add_net "Net-(SHIELD1-PadNC)")
    (add_net "Net-(SHIELD1-PadRST)")
    (add_net "Net-(SHIELD1-PadSCL)")
    (add_net "Net-(SHIELD1-PadSDA)")
    (add_net "Net-(SHIELD1-PadV_IN)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad8)")
  )
  (net_class Power ""
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module graphics:tepmachcha (layer B.Cu) (tedit 0)
    (at 166.624 113.665 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module graphics:tepmachcha (layer F.Cu) (tedit 0)
    (at 167.386 100.33 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module DAI_Maker_Lab_footprints:Grove_straight (layer F.Cu) (tedit 57680D84)
    (at 168.656 87.376 270)
    (fp_text reference P1 (at 0 4 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 -3 270) (layer F.Fab) hide)
    (fp_text user GND (at 3 -1.5 270) (layer F.SilkS))
    (fp_text user Vcc (at 1 -1.5 270) (layer F.SilkS))
    (fp_text user 2 (at -1 -1.5 270) (layer F.SilkS))
    (fp_text user 1 (at -3 -1.5 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -1 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 1 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 4 thru_hole circle (at 3 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module DAI_Maker_Lab_footprints:ARDUINO locked (layer F.Cu) (tedit 573C8890)
    (at 148.5011 105.0036)
    (descr test)
    (fp_text reference SHIELD1 (at -3.5 20 180) (layer F.SilkS) hide)
    (fp_text value ARDUINO_SHIELD (at -1.5 -29) (layer F.SilkS) hide)
    (pad AD5 thru_hole circle (at 19 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole circle (at 16.46 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole circle (at 13.92 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SHIELD1-PadAD3)"))
    (pad AD0 thru_hole circle (at 6.3 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(SHIELD1-PadAD0)"))
    (pad AD1 thru_hole circle (at 8.84 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SHIELD1-PadAD1)"))
    (pad AD2 thru_hole circle (at 11.38 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SHIELD1-PadAD2)"))
    (pad V_IN thru_hole circle (at 1.22 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SHIELD1-PadV_IN)"))
    (pad GND2 thru_hole circle (at -1.32 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SHIELD1-PadGND2)"))
    (pad GND1 thru_hole circle (at -3.86 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 3V3 thru_hole circle (at -8.94 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SHIELD1-Pad3V3)"))
    (pad RST thru_hole circle (at -11.48 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-PadRST)"))
    (pad 0 thru_hole circle (at 19 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SHIELD1-Pad0)"))
    (pad 1 thru_hole circle (at 16.46 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SHIELD1-Pad1)"))
    (pad 2 thru_hole circle (at 13.92 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(SHIELD1-Pad2)"))
    (pad 3 thru_hole circle (at 11.38 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(SHIELD1-Pad3)"))
    (pad 4 thru_hole circle (at 8.84 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SHIELD1-Pad4)"))
    (pad 5 thru_hole circle (at 6.3 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(SHIELD1-Pad5)"))
    (pad 6 thru_hole circle (at 3.76 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SHIELD1-Pad6)"))
    (pad 7 thru_hole circle (at 1.22 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 8 thru_hole circle (at -2.844 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 9 thru_hole circle (at -5.384 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(SHIELD1-Pad9)"))
    (pad 10 thru_hole circle (at -7.924 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(SHIELD1-Pad10)"))
    (pad 11 thru_hole circle (at -10.464 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad11)"))
    (pad 12 thru_hole circle (at -13.004 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-Pad12)"))
    (pad 13 thru_hole circle (at -15.544 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(SHIELD1-Pad13)"))
    (pad GND3 thru_hole circle (at -18.084 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(SHIELD1-PadGND3)"))
    (pad AREF thru_hole circle (at -20.624 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole circle (at -6.4 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad SDA thru_hole circle (at -23.164 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(SHIELD1-PadSDA)"))
    (pad SCL thru_hole circle (at -25.704 -24.8 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(SHIELD1-PadSCL)"))
    (pad IO_R thru_hole circle (at -14.02 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(SHIELD1-PadIO_R)"))
    (pad NC thru_hole circle (at -16.56 23.46 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(SHIELD1-PadNC)"))
  )
  (module hidro-cambodia:DAI-PIN_logos (layer B.Cu) (tedit 0)
    (at 155.829 103.505 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module DAI_Maker_Lab_footprints:FONA_808 (layer F.Cu) (tedit 5768101C)
    (at 141.732 105.156 180)
    (fp_text reference U1 (at -5.715 -13.335 180) (layer F.SilkS) hide)
    (fp_text value FONA_808 (at -0.635 -17.78 180) (layer F.Fab) hide)
    (fp_text user SIM (at 8.89 0 270) (layer F.SilkS))
    (fp_text user Spk- (at 19 19 270) (layer F.SilkS))
    (fp_text user Spk+ (at 16.5 19 270) (layer F.SilkS))
    (fp_text user Mic- (at 14 19 270) (layer F.SilkS))
    (fp_text user Mic+ (at 11.5 19 270) (layer F.SilkS))
    (fp_text user NS (at 9 20 270) (layer F.SilkS))
    (fp_text user PStat (at 6.5 19 270) (layer F.SilkS))
    (fp_text user RI (at 4 20.25 270) (layer F.SilkS))
    (fp_text user Key (at 1.5 19.75 270) (layer F.SilkS))
    (fp_text user RTS (at -1.25 19.75 270) (layer F.SilkS))
    (fp_text user TX (at -3.75 20 270) (layer F.SilkS))
    (fp_text user RX (at -6.25 20 270) (layer F.SilkS))
    (fp_text user Rst (at -8.75 19.75 270) (layer F.SilkS))
    (fp_text user Vio (at -11.25 19.75 270) (layer F.SilkS))
    (fp_text user GND (at -14 19.5 270) (layer F.SilkS))
    (fp_text user Bat (at -16.5 19.75 270) (layer F.SilkS))
    (fp_text user 5V (at -19 20 270) (layer F.SilkS))
    (pad 18 thru_hole circle (at 17.75 -18.25 180) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -19.05 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -16.51 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 3 thru_hole circle (at -13.97 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 4 thru_hole circle (at -11.43 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 5 thru_hole circle (at -8.89 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SHIELD1-Pad4)"))
    (pad 6 thru_hole circle (at -6.35 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SHIELD1-Pad6)"))
    (pad 7 thru_hole circle (at -3.81 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(SHIELD1-Pad9)"))
    (pad 8 thru_hole circle (at -1.27 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 1.27 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad11)"))
    (pad 10 thru_hole circle (at 3.81 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at 6.35 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-Pad12)"))
    (pad 12 thru_hole circle (at 8.89 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at 11.43 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 13.97 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at 16.51 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at 19.05 22.225 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U1-Pad16)"))
    (pad 17 thru_hole circle (at -17.75 -18.25 180) (size 3.81 3.81) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text https://github.com/DAI-Maker-Lab/tepmachcha (at 145.288 104.648 270) (layer B.SilkS))
  (gr_text "v0.3\nFlood Early Warning" (at 167.386 104.775 270) (layer B.SilkS))
  (gr_text "v0.3\nFlood Early Warning\n" (at 168.021 109.855 270) (layer F.SilkS))
  (gr_line (start 121.412 78.232) (end 121.412 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.7 78.232) (end 121.412 78.232) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.704 130.048) (end 171.704 78.232) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.556 130.048) (end 171.7 130.048) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 127.508) (end 130.556 130.048) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.412 127.508) (end 130.048 127.508) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.412 120.904) (end 121.412 127.508) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.748 120.904) (end 121.412 120.904) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.748 88.9) (end 142.748 120.904) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.412 88.9) (end 142.748 88.9) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.577 130.048) (xy 130.556 130.048) (xy 130.048 127.635) (xy 121.285 127.635) (xy 121.412 120.904)
        (xy 142.748 121.031) (xy 142.748 88.9) (xy 121.412 88.9) (xy 121.412 78.359) (xy 171.704 78.359)
        (xy 171.577 130.048)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.704 129.921) (xy 130.556 130.048) (xy 130.048 127.508) (xy 121.412 127.508) (xy 121.412 120.904)
        (xy 142.748 120.904) (xy 142.748 88.9) (xy 121.412 88.9) (xy 121.412 78.232) (xy 171.577 78.232)
        (xy 171.704 129.921)
      )
    )
  )
)
