(kicad_pcb (version 4) (host pcbnew 4.0.7-e1-6374~58~ubuntu16.04.1)
  (general
    (links 40)
    (no_connects 0)
    (area 111.149999 91.949999 211.250001 136.050001)
    (thickness 1.6)
    (drawings 4)
    (tracks 149)
    (zones 0)
    (modules 23)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.7)
    (user_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 0.6)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00020_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(10K1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(10K2-Pad2)")
  (net 4 "Net-(10K3-Pad2)")
  (net 5 "Net-(10K4-Pad1)")
  (net 6 "Net-(10K5-Pad1)")
  (net 7 "Net-(10K6-Pad1)")
  (net 8 "Net-(10nF1-Pad2)")
  (net 9 "Net-(U1-Pad2)")
  (net 10 VCC)
  (net 11 "Net-(J4-Pad1)")
  (net 12 "Net-(J5-Pad1)")
  (net 13 "Net-(J6-Pad1)")
  (net 14 "Net-(J7-Pad1)")
  (net 15 "Net-(J8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.7)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(10K1-Pad1)")
    (add_net "Net-(10K2-Pad2)")
    (add_net "Net-(10K3-Pad2)")
    (add_net "Net-(10K4-Pad1)")
    (add_net "Net-(10K5-Pad1)")
    (add_net "Net-(10K6-Pad1)")
    (add_net "Net-(10nF1-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net VCC)
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 139.192 98.552 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 10K1 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(10K1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 146.304 98.552 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 10K2 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(10K1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(10K2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 151.384 104.648 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 10K3 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(10K2-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(10K3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 168.656 124.46 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 10K4 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(10K4-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 180.848 124.46 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 10K5 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(10K5-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 193.548 124.46 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 10K6 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(10K6-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5991E619)
    (at 160.528 116.332 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference 10nF1 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value C (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(10nF1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5991E61E)
    (at 137.16 106.68 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference 47uF1 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value C (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(10K3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5991E5FA)
    (at 167.64 114.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(10K4-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5991E5FF)
    (at 179.832 114.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(10K5-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5991E607)
    (at 192.532 114.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC817-40 (at 0 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(10K6-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 58CC8E33)
    (at 145.796 118.364 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 -2.39 90) (layer F.SilkS))
    (fp_text value LM555N (at 3.81 10.01 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(10nF1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J7-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(10K2-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(10K1-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(10K1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W11.48mm_SMD (layer F.Cu) (tedit 58CC8E2D)
    (at 131.572 123.952)
    (descr "16-lead dip package, row spacing 11.48 mm (451 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 11.48mm 451mil SMD")
    (attr smd)
    (fp_text reference U2 (at 0 -11.28) (layer F.SilkS))
    (fp_text value 74LS06 (at 0 11.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.74 -8.89) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(10K1-Pad1)"))
    (pad 9 smd rect (at 5.74 8.89) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -5.74 -6.35) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(10K4-Pad1)"))
    (pad 10 smd rect (at 5.74 6.35) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.74 -3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 5.74 3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -5.74 -1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 5.74 1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -5.74 1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 5.74 -1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -5.74 3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 5.74 -3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 7 smd rect (at -5.74 6.35) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 5.74 -6.35) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -5.74 8.89) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 5.74 -8.89) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W11.48mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_WAGO-804_RM7.5mm_1pol (layer F.Cu) (tedit 599342E7)
    (at 115.824 109.22)
    (fp_text reference J1 (at 0 -9.5) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 "Net-(10K1-Pad1)"))
    (pad 1 thru_hole circle (at 2.49936 -5.00126) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 "Net-(10K1-Pad1)"))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_WAGO-804_RM7.5mm_1pol (layer F.Cu) (tedit 599342E3)
    (at 127.508 104.14)
    (fp_text reference J2 (at 0 -9.5) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 10 VCC))
    (pad 1 thru_hole circle (at 2.49936 -5.00126) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 10 VCC))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_WAGO-804_RM7.5mm_1pol (layer F.Cu) (tedit 599204A6)
    (at 115.824 127)
    (fp_text reference J3 (at 0 -9.5) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.49936 -5.00126) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_WAGO-804_RM7.5mm_1pol (layer F.Cu) (tedit 599342DE)
    (at 200.152 107.696)
    (fp_text reference J4 (at 0 -9.5) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at 2.49936 -5.00126) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad1)"))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_WAGO-804_RM7.5mm_1pol (layer F.Cu) (tedit 599342D0)
    (at 165.608 103.124)
    (fp_text reference J5 (at 0 -9.5) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad1)"))
    (pad 1 thru_hole circle (at 2.49936 -5.00126) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad1)"))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_WAGO-804_RM7.5mm_1pol (layer F.Cu) (tedit 599342D4)
    (at 177.8 103.124)
    (fp_text reference J6 (at 0 -9.5) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad1)"))
    (pad 1 thru_hole circle (at 2.49936 -5.00126) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad1)"))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-4pol (layer F.Cu) (tedit 599342D7)
    (at 146.812 125.984)
    (descr "4-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J7 (at 7.5 5.9) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x04 (at 7.5 -6.6) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 43.18 -3.556) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(10K6-Pad1)"))
    (pad 3 thru_hole circle (at 30.48 -3.556) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(10K5-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(J7-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(10K1-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-4pol.wrl
      (at (xyz 0.2953 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_WAGO-804_RM7.5mm_1pol (layer F.Cu) (tedit 599342DB)
    (at 190.5 103.124)
    (fp_text reference J8 (at 0 -9.5) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x01 (at 0 8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 15 "Net-(J8-Pad1)"))
    (pad 1 thru_hole circle (at 2.49936 -5.00126) (size 3.175 3.175) (drill 1.19888) (layers *.Cu *.Mask)
      (net 15 "Net-(J8-Pad1)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 59944D6E)
    (at 121.158 114.046)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 201.422 114.046)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (gr_line (start 111.2 136) (end 211.2 136) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2 92) (end 111.2 136) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.2 92) (end 111.2 92) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.2 136) (end 211.2 92) (angle 90) (layer Edge.Cuts) (width 0.1))
)
