(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 62)
    (zones 0)
    (modules 12)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 L+)
  (net 2 "Net-(6k8-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C1-Pad1)")
  (net 5 LV-)
  (net 6 LV+)
  (net 7 LCB)
  (net 8 L-)
  (net 9 LComp)
  (net 10 LBal)
  (net 11 "Net-(J4-Pad1)")
  (net 12 "Net-(U1-Pad8)")
  (net 13 "Net-(U1-Pad5)")
  (net 14 "Net-(U1-Pad1)")
  (net 15 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net L+)
    (add_net L-)
    (add_net LBal)
    (add_net LCB)
    (add_net LComp)
    (add_net LV+)
    (add_net LV-)
    (add_net "Net-(6k8-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5FFA5FB1)
    (at 182.753 59.69)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference J2 (at -3.429 -0.127) (layer F.SilkS) hide)
    (fp_text value GND (at -5.715 -2.54) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 LCB))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 LV-))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 LV+))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 L+))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 L-))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 L-))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 LComp))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 LBal))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:DIP794W53P254L959H508Q8N (layer F.Cu) (tedit 5FFA5F45)
    (at 191.229 63.5)
    (descr "P (R-PDIP-T8)")
    (tags "Integrated Circuit")
    (fp_text reference U1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "NE5   534" (at 1.811 0 90) (layer F.SilkS))
    (fp_text user %R (at 1.938 3.937) (layer F.Fab))
    (pad 8 thru_hole circle (at 3.97 -3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at 3.97 -1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 6 LV+))
    (pad 6 thru_hole circle (at 3.97 1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 1 L+))
    (pad 5 thru_hole circle (at 3.97 3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at -3.97 3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 5 LV-))
    (pad 3 thru_hole circle (at -3.97 1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at -3.97 -1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 2 "Net-(6k8-Pad1)"))
    (pad 1 thru_hole circle (at -3.97 -3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad1)"))
    (model "C:\\Users\\julvi\\Google Drive\\KiCad Libraries\\SamacSys_Parts.3dshapes\\NE5534AP.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:DIP794W53P254L959H508Q8N (layer F.Cu) (tedit 5FFA5F17)
    (at 180.754 63.5)
    (descr "P (R-PDIP-T8)")
    (tags "Integrated Circuit")
    (fp_text reference U2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value TL071 (at -0.16 0.254 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 thru_hole circle (at 3.97 -3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 7 LCB))
    (pad 7 thru_hole circle (at 3.97 -1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 6 LV+))
    (pad 6 thru_hole circle (at 3.97 1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 8 L-))
    (pad 5 thru_hole circle (at 3.97 3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 9 LComp))
    (pad 4 thru_hole circle (at -3.97 3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 5 LV-))
    (pad 3 thru_hole circle (at -3.97 1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 1 L+))
    (pad 2 thru_hole circle (at -3.97 -1.27) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 8 L-))
    (pad 1 thru_hole circle (at -3.97 -3.81) (size 1.13 1.13) (drill 0.73) (layers *.Cu *.Mask)
      (net 10 LBal))
    (model "C:\\Users\\julvi\\Google Drive\\KiCad Libraries\\SamacSys_Parts.3dshapes\\NE5534AP.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 5FFA5C65)
    (at 187.96 50.165)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference NC (at 2.032 0) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 4.385 -2.27) (layer B.Fab))
    (fp_text user %R (at 2.77 0 -90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 5FFA46FA)
    (at 192.532 63.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference In (at 0 1.778) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 4.385 -2.27) (layer B.Fab))
    (fp_text user %R (at 2.77 0 -90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 180.34 57.15)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 1.905 0.508) (layer B.SilkS) hide)
    (fp_text value Conn_01x01 (at 4.385 -2.27) (layer B.Fab))
    (fp_text user %R (at 2.77 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module orig:orig_320dpi (layer F.Cu) (tedit 0)
    (at 192.45 61.55 270)
    (fp_text reference G*** (at 1.569 6.014 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 2.077 6.141 90) (layer F.SilkS) hide)
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 184.912 52.832)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 2.921 0) (layer B.SilkS) hide)
    (fp_text value 68R (at 4.826 0.127) (layer B.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(6k8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 195.072 55.88 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 6k8 (at 4.953 0) (layer B.SilkS))
    (fp_text value R (at 0 0) (layer B.SilkS) hide)
    (fp_text user %R (at -3.175 3.175) (layer B.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 L+))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(6k8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:185104J63RAAF (layer F.Cu) (tedit 0)
    (at 185.42 55.753)
    (descr 185104J63RAA-F)
    (tags Capacitor)
    (fp_text reference C3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.651) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 LV-))
    (pad 1 thru_hole circle (at -2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 LV+))
    (model "C:\\Users\\julvi\\Google Drive\\KiCad Libraries\\SamacSys_Parts.3dshapes\\185104J63RAA-F.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:R82MC1220AA50J (layer F.Cu) (tedit 0)
    (at 192.278 55.88 90)
    (descr R82MC1220AA50J-4)
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 0 90) (layer F.SilkS) hide)
    (fp_text value 2n2 (at 2.413 0.127 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(6k8-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 L+))
    (model "C:\\Users\\julvi\\Google Drive\\KiCad Libraries\\SamacSys_Parts.3dshapes\\R82MC1220AA50J.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:CAPPRD250W55D630H1320 (layer F.Cu) (tedit 5FFA3B22)
    (at 180.34 52.07 180)
    (descr EEU-FC1H330)
    (tags "Capacitor Polarised")
    (fp_text reference C1 (at 1.143 1.778) (layer F.SilkS) hide)
    (fp_text value 33u (at 1.143 -1.778) (layer F.SilkS))
    (pad 2 thru_hole rect (at 2.5 0 180) (size 1.15 1.15) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.15 1.15) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (model "C:\\Users\\julvi\\Google Drive\\KiCad Libraries\\SamacSys_Parts.3dshapes\\EEU-FC1H330.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "PCB\nrev 1" (at 187.071 52.832) (layer F.SilkS))
  (gr_text "Nordcore/\nRinner" (at 184.277 49.784) (layer F.SilkS))
  (gr_line (start 175.387 68.834) (end 196.215 68.834) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 175.387 46.99) (end 175.387 68.834) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.215 46.99) (end 175.387 46.99) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 196.215 68.834) (end 196.215 46.99) (layer Edge.Cuts) (width 0.05))
  (gr_text "TTSH v4 reverb amp\n" (at 185.801 47.879) (layer F.SilkS))
)
