(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 23)
    (no_connects 0)
    (area 54.534999 64.694999 90.245001 126.440001)
    (thickness 1.6)
    (drawings 12)
    (tracks 123)
    (zones 0)
    (modules 6)
    (nets 11)
  )
  (page User 148.006 210.007)
  (title_block
    (title "Nokia Color TFT LCD")
    (date 2017-01-29)
    (rev 1)
    (company "Discovery Center")
    (comment 1 karibe.co)
    (comment 2 @muriukidavid)
    (comment 3 "Karibe David")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory 1616LCD_gerbers/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 RESET)
  (net 4 CE)
  (net 5 MOSI)
  (net 6 CLK)
  (net 7 LED)
  (net 8 LED-)
  (net 9 "Net-(Q1-Pad1)")
  (net 10 5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net CE)
    (add_net CLK)
    (add_net GND)
    (add_net LED)
    (add_net LED-)
    (add_net MOSI)
    (add_net "Net-(Q1-Pad1)")
    (add_net RESET)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5BEDE2BC)
    (at 86.995 123.952)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 0.1 (at 2.8194 1.2446) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:Nokia1616_LCD (layer F.Cu) (tedit 5BEDE2AF)
    (at 76.57812 115.23218 180)
    (fp_text reference CONN1 (at -2.36508 1.13538 180) (layer F.SilkS) hide)
    (fp_text value Nokia1616_LCD (at 0 -4.826 180) (layer F.Fab))
    (pad 1 smd rect (at -7.08148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -6.48148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 3 RESET))
    (pad 3 smd rect (at -5.88148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 4 CE))
    (pad 4 smd rect (at -5.28148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -4.68148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 5 MOSI))
    (pad 6 smd rect (at -4.08148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 6 CLK))
    (pad 7 smd rect (at -3.48148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 8 smd rect (at -2.88148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 9 smd rect (at -2.28148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1.68148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 8 LED-))
    (pad 11 smd rect (at -1.08148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask)
      (net 10 5V))
    (pad 12 smd rect (at -0.48148 -1.20142 180) (size 0.319989 2.399995) (layers F.Cu F.Paste F.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BEDE281)
    (at 57.404 123.19 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.3716 -1.8796 180) (layer F.SilkS))
    (fp_text value BC547_BEC_123 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 LED-))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5BEDE299)
    (at 60.833 123.19 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 1.9304 1.651 360) (layer F.SilkS))
    (fp_text value 1K (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 LED))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 5BEDE096)
    (at 81.01838 123.04268 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P1 (at 0 2.54762 90) (layer B.SilkS))
    (fp_text value CONN_01X08 (at -2.62382 -12.18438 180) (layer B.Fab) hide)
    (fp_text user %R (at -2.62382 1.72212 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 CE))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 LED))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 MOSI))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 CLK))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 63.2333 67.2846 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P2 (at -0.0381 -20.3327 270) (layer B.SilkS))
    (fp_text value CONN_01X08 (at 0 -20.11 270) (layer B.Fab))
    (fp_text user %R (at 0 -8.89 540) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 5V))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 CLK))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 MOSI))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 LED))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 CE))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5V (at 63.238 125.222) (layer F.SilkS))
  (gr_text CLK (at 65.778 125.222) (layer F.SilkS))
  (gr_text MOSI (at 68.318 125.222) (layer F.SilkS))
  (gr_text "LED\n" (at 70.866 125.222) (layer F.SilkS))
  (gr_text RST (at 73.39838 125.222) (layer F.SilkS))
  (gr_text CE (at 75.93838 125.222) (layer F.SilkS))
  (gr_text "GND\n" (at 78.478 125.222) (layer F.SilkS))
  (gr_text 3v3 (at 81.018 125.222) (layer F.SilkS))
  (gr_line (start 90.17 64.77) (end 90.17 126.365) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 64.77) (end 90.17 64.77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 126.365) (end 54.61 64.77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.17 126.365) (end 54.61 126.365) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.17 126.365) (xy 54.61 126.365) (xy 54.61 64.77) (xy 90.17 64.77)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.17 127) (xy 54.61 127) (xy 54.61 64.77) (xy 90.17 64.77)
      )
    )
  )
)
